Callisto4Bootloader: ENET Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
ENET Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| ENET Register Masks

## Data Structures

struct | ENET_Type

## Macros

#define | ENET_BASE (0x402D8000u)
#define | ENET ((ENET_Type *)ENET_BASE)
#define | ENET2_BASE (0x402D4000u)
#define | ENET2 ((ENET_Type *)ENET2_BASE)
#define | ENET_BASE_ADDRS { ENET_BASE, 0u, ENET2_BASE }
#define | ENET_BASE_PTRS { ENET, (ENET_Type *)0u, ENET2 }
#define | ENET_Transmit_IRQS { ENET_IRQn, NotAvail_IRQn, ENET2_IRQn }
#define | ENET_Receive_IRQS { ENET_IRQn, NotAvail_IRQn, ENET2_IRQn }
#define | ENET_Error_IRQS { ENET_IRQn, NotAvail_IRQn, ENET2_IRQn }
#define | ENET_1588_Timer_IRQS { ENET_1588_Timer_IRQn, NotAvail_IRQn, ENET2_1588_Timer_IRQn }
#define | ENET_BUFF_ALIGNMENT (64U)

## Detailed Description

## Macro Definition Documentation

## ◆ ENET

#define ENET ((ENET_Type *)ENET_BASE)

Peripheral ENET base pointer

Definition at line 18401 of file MIMXRT1062.h.

## ◆ ENET2

#define ENET2 ((ENET_Type *)ENET2_BASE)

Peripheral ENET2 base pointer

Definition at line 18405 of file MIMXRT1062.h.

## ◆ ENET2_BASE

#define ENET2_BASE (0x402D4000u)

Peripheral ENET2 base address

Definition at line 18403 of file MIMXRT1062.h.

## ◆ ENET_1588_Timer_IRQS

#define ENET_1588_Timer_IRQS { ENET_1588_Timer_IRQn, NotAvail_IRQn, ENET2_1588_Timer_IRQn }

Definition at line 18414 of file MIMXRT1062.h.

## ◆ ENET_BASE

#define ENET_BASE (0x402D8000u)

Peripheral ENET base address

Definition at line 18399 of file MIMXRT1062.h.

## ◆ ENET_BASE_ADDRS

#define ENET_BASE_ADDRS { ENET_BASE, 0u, ENET2_BASE }

Array initializer of ENET peripheral base addresses

Definition at line 18407 of file MIMXRT1062.h.

## ◆ ENET_BASE_PTRS

#define ENET_BASE_PTRS { ENET, (ENET_Type *)0u, ENET2 }

Array initializer of ENET peripheral base pointers

Definition at line 18409 of file MIMXRT1062.h.

## ◆ ENET_BUFF_ALIGNMENT

#define ENET_BUFF_ALIGNMENT (64U)

Definition at line 18416 of file MIMXRT1062.h.

## ◆ ENET_Error_IRQS

#define ENET_Error_IRQS { ENET_IRQn, NotAvail_IRQn, ENET2_IRQn }

Definition at line 18413 of file MIMXRT1062.h.

## ◆ ENET_Receive_IRQS

#define ENET_Receive_IRQS { ENET_IRQn, NotAvail_IRQn, ENET2_IRQn }

Definition at line 18412 of file MIMXRT1062.h.

## ◆ ENET_Transmit_IRQS

#define ENET_Transmit_IRQS { ENET_IRQn, NotAvail_IRQn, ENET2_IRQn }

Interrupt vectors for the ENET peripheral type

Definition at line 18411 of file MIMXRT1062.h.