Callisto4Bootloader: RTWDOG Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
RTWDOG Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| RTWDOG Register Masks

## Data Structures

struct | RTWDOG_Type

## Macros

#define | RTWDOG_BASE (0x400BC000u)
#define | RTWDOG ((RTWDOG_Type *)RTWDOG_BASE)
#define | RTWDOG_BASE_ADDRS { RTWDOG_BASE }
#define | RTWDOG_BASE_PTRS { RTWDOG }
#define | RTWDOG_IRQS { RTWDOG_IRQn }
#define | RTWDOG_UPDATE_KEY (0xD928C520U)
#define | RTWDOG_REFRESH_KEY (0xB480A602U)

## Detailed Description

## Macro Definition Documentation

## ◆ RTWDOG

#define RTWDOG ((RTWDOG_Type *)RTWDOG_BASE)

Peripheral RTWDOG base pointer

Definition at line 36319 of file MIMXRT1062.h.

## ◆ RTWDOG_BASE

#define RTWDOG_BASE (0x400BC000u)

Peripheral RTWDOG base address

Definition at line 36317 of file MIMXRT1062.h.

## ◆ RTWDOG_BASE_ADDRS

#define RTWDOG_BASE_ADDRS { RTWDOG_BASE }

Array initializer of RTWDOG peripheral base addresses

Definition at line 36321 of file MIMXRT1062.h.

## ◆ RTWDOG_BASE_PTRS

#define RTWDOG_BASE_PTRS { RTWDOG }

Array initializer of RTWDOG peripheral base pointers

Definition at line 36323 of file MIMXRT1062.h.

## ◆ RTWDOG_IRQS

#define RTWDOG_IRQS { RTWDOG_IRQn }

Interrupt vectors for the RTWDOG peripheral type

Definition at line 36325 of file MIMXRT1062.h.

## ◆ RTWDOG_REFRESH_KEY

#define RTWDOG_REFRESH_KEY (0xB480A602U)

Definition at line 36328 of file MIMXRT1062.h.

## ◆ RTWDOG_UPDATE_KEY

#define RTWDOG_UPDATE_KEY (0xD928C520U)

Definition at line 36327 of file MIMXRT1062.h.