Callisto4Bootloader: TSC Register Masks

Callisto4Bootloader

TSC Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » TSC Peripheral Access Layer

## BASIC_SETTING - Basic Setting

#define | TSC_BASIC_SETTING_AUTO_MEASURE_MASK (0x1U)
#define | TSC_BASIC_SETTING_AUTO_MEASURE_SHIFT (0U)
#define | TSC_BASIC_SETTING_AUTO_MEASURE(x) (((uint32_t)(((uint32_t)(x)) << TSC_BASIC_SETTING_AUTO_MEASURE_SHIFT)) & TSC_BASIC_SETTING_AUTO_MEASURE_MASK)
#define | TSC_BASIC_SETTING_WIRE_4_5_MASK (0x10U)
#define | TSC_BASIC_SETTING_WIRE_4_5_SHIFT (4U)
#define | TSC_BASIC_SETTING_WIRE_4_5(x) (((uint32_t)(((uint32_t)(x)) << TSC_BASIC_SETTING_WIRE_4_5_SHIFT)) & TSC_BASIC_SETTING_WIRE_4_5_MASK)
#define | TSC_BASIC_SETTING_MEASURE_DELAY_TIME_MASK (0xFFFFFF00U)
#define | TSC_BASIC_SETTING_MEASURE_DELAY_TIME_SHIFT (8U)
#define | TSC_BASIC_SETTING_MEASURE_DELAY_TIME(x) (((uint32_t)(((uint32_t)(x)) << TSC_BASIC_SETTING_MEASURE_DELAY_TIME_SHIFT)) & TSC_BASIC_SETTING_MEASURE_DELAY_TIME_MASK)

## PRE_CHARGE_TIME - Pre-charge Time

#define | TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_MASK (0xFFFFFFFFU)
#define | TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_SHIFT (0U)
#define | TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME(x) (((uint32_t)(((uint32_t)(x)) << TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_SHIFT)) & TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_MASK)

## FLOW_CONTROL - Flow Control

#define | TSC_FLOW_CONTROL_SW_RST_MASK (0x1U)
#define | TSC_FLOW_CONTROL_SW_RST_SHIFT (0U)
#define | TSC_FLOW_CONTROL_SW_RST(x) (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_SW_RST_SHIFT)) & TSC_FLOW_CONTROL_SW_RST_MASK)
#define | TSC_FLOW_CONTROL_START_MEASURE_MASK (0x10U)
#define | TSC_FLOW_CONTROL_START_MEASURE_SHIFT (4U)
#define | TSC_FLOW_CONTROL_START_MEASURE(x) (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_START_MEASURE_SHIFT)) & TSC_FLOW_CONTROL_START_MEASURE_MASK)
#define | TSC_FLOW_CONTROL_DROP_MEASURE_MASK (0x100U)
#define | TSC_FLOW_CONTROL_DROP_MEASURE_SHIFT (8U)
#define | TSC_FLOW_CONTROL_DROP_MEASURE(x) (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_DROP_MEASURE_SHIFT)) & TSC_FLOW_CONTROL_DROP_MEASURE_MASK)
#define | TSC_FLOW_CONTROL_START_SENSE_MASK (0x1000U)
#define | TSC_FLOW_CONTROL_START_SENSE_SHIFT (12U)
#define | TSC_FLOW_CONTROL_START_SENSE(x) (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_START_SENSE_SHIFT)) & TSC_FLOW_CONTROL_START_SENSE_MASK)
#define | TSC_FLOW_CONTROL_DISABLE_MASK (0x10000U)
#define | TSC_FLOW_CONTROL_DISABLE_SHIFT (16U)
#define | TSC_FLOW_CONTROL_DISABLE(x) (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_DISABLE_SHIFT)) & TSC_FLOW_CONTROL_DISABLE_MASK)

## MEASEURE_VALUE - Measure Value

#define | TSC_MEASEURE_VALUE_Y_VALUE_MASK (0xFFFU)
#define | TSC_MEASEURE_VALUE_Y_VALUE_SHIFT (0U)
#define | TSC_MEASEURE_VALUE_Y_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TSC_MEASEURE_VALUE_Y_VALUE_SHIFT)) & TSC_MEASEURE_VALUE_Y_VALUE_MASK)
#define | TSC_MEASEURE_VALUE_X_VALUE_MASK (0xFFF0000U)
#define | TSC_MEASEURE_VALUE_X_VALUE_SHIFT (16U)
#define | TSC_MEASEURE_VALUE_X_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TSC_MEASEURE_VALUE_X_VALUE_SHIFT)) & TSC_MEASEURE_VALUE_X_VALUE_MASK)

## INT_EN - Interrupt Enable

#define | TSC_INT_EN_MEASURE_INT_EN_MASK (0x1U)
#define | TSC_INT_EN_MEASURE_INT_EN_SHIFT (0U)
#define | TSC_INT_EN_MEASURE_INT_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_EN_MEASURE_INT_EN_SHIFT)) & TSC_INT_EN_MEASURE_INT_EN_MASK)
#define | TSC_INT_EN_DETECT_INT_EN_MASK (0x10U)
#define | TSC_INT_EN_DETECT_INT_EN_SHIFT (4U)
#define | TSC_INT_EN_DETECT_INT_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_EN_DETECT_INT_EN_SHIFT)) & TSC_INT_EN_DETECT_INT_EN_MASK)
#define | TSC_INT_EN_IDLE_SW_INT_EN_MASK (0x1000U)
#define | TSC_INT_EN_IDLE_SW_INT_EN_SHIFT (12U)
#define | TSC_INT_EN_IDLE_SW_INT_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_EN_IDLE_SW_INT_EN_SHIFT)) & TSC_INT_EN_IDLE_SW_INT_EN_MASK)

## INT_SIG_EN - Interrupt Signal Enable

#define | TSC_INT_SIG_EN_MEASURE_SIG_EN_MASK (0x1U)
#define | TSC_INT_SIG_EN_MEASURE_SIG_EN_SHIFT (0U)
#define | TSC_INT_SIG_EN_MEASURE_SIG_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_MEASURE_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_MEASURE_SIG_EN_MASK)
#define | TSC_INT_SIG_EN_DETECT_SIG_EN_MASK (0x10U)
#define | TSC_INT_SIG_EN_DETECT_SIG_EN_SHIFT (4U)
#define | TSC_INT_SIG_EN_DETECT_SIG_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_DETECT_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_DETECT_SIG_EN_MASK)
#define | TSC_INT_SIG_EN_VALID_SIG_EN_MASK (0x100U)
#define | TSC_INT_SIG_EN_VALID_SIG_EN_SHIFT (8U)
#define | TSC_INT_SIG_EN_VALID_SIG_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_VALID_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_VALID_SIG_EN_MASK)
#define | TSC_INT_SIG_EN_IDLE_SW_SIG_EN_MASK (0x1000U)
#define | TSC_INT_SIG_EN_IDLE_SW_SIG_EN_SHIFT (12U)
#define | TSC_INT_SIG_EN_IDLE_SW_SIG_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_IDLE_SW_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_IDLE_SW_SIG_EN_MASK)

## INT_STATUS - Intterrupt Status

#define | TSC_INT_STATUS_MEASURE_MASK (0x1U)
#define | TSC_INT_STATUS_MEASURE_SHIFT (0U)
#define | TSC_INT_STATUS_MEASURE(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_MEASURE_SHIFT)) & TSC_INT_STATUS_MEASURE_MASK)
#define | TSC_INT_STATUS_DETECT_MASK (0x10U)
#define | TSC_INT_STATUS_DETECT_SHIFT (4U)
#define | TSC_INT_STATUS_DETECT(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_DETECT_SHIFT)) & TSC_INT_STATUS_DETECT_MASK)
#define | TSC_INT_STATUS_VALID_MASK (0x100U)
#define | TSC_INT_STATUS_VALID_SHIFT (8U)
#define | TSC_INT_STATUS_VALID(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_VALID_SHIFT)) & TSC_INT_STATUS_VALID_MASK)
#define | TSC_INT_STATUS_IDLE_SW_MASK (0x1000U)
#define | TSC_INT_STATUS_IDLE_SW_SHIFT (12U)
#define | TSC_INT_STATUS_IDLE_SW(x) (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_IDLE_SW_SHIFT)) & TSC_INT_STATUS_IDLE_SW_MASK)

## DEBUG_MODE - Debug Mode Register

#define | TSC_DEBUG_MODE_ADC_CONV_VALUE_MASK (0xFFFU)
#define | TSC_DEBUG_MODE_ADC_CONV_VALUE_SHIFT (0U)
#define | TSC_DEBUG_MODE_ADC_CONV_VALUE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_CONV_VALUE_SHIFT)) & TSC_DEBUG_MODE_ADC_CONV_VALUE_MASK)
#define | TSC_DEBUG_MODE_ADC_COCO_MASK (0x1000U)
#define | TSC_DEBUG_MODE_ADC_COCO_SHIFT (12U)
#define | TSC_DEBUG_MODE_ADC_COCO(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_COCO_SHIFT)) & TSC_DEBUG_MODE_ADC_COCO_MASK)
#define | TSC_DEBUG_MODE_EXT_HWTS_MASK (0x1F0000U)
#define | TSC_DEBUG_MODE_EXT_HWTS_SHIFT (16U)
#define | TSC_DEBUG_MODE_EXT_HWTS(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_EXT_HWTS_SHIFT)) & TSC_DEBUG_MODE_EXT_HWTS_MASK)
#define | TSC_DEBUG_MODE_TRIGGER_MASK (0x1000000U)
#define | TSC_DEBUG_MODE_TRIGGER_SHIFT (24U)
#define | TSC_DEBUG_MODE_TRIGGER(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_TRIGGER_SHIFT)) & TSC_DEBUG_MODE_TRIGGER_MASK)
#define | TSC_DEBUG_MODE_ADC_COCO_CLEAR_MASK (0x2000000U)
#define | TSC_DEBUG_MODE_ADC_COCO_CLEAR_SHIFT (25U)
#define | TSC_DEBUG_MODE_ADC_COCO_CLEAR(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_COCO_CLEAR_SHIFT)) & TSC_DEBUG_MODE_ADC_COCO_CLEAR_MASK)
#define | TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_MASK (0x4000000U)
#define | TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_SHIFT (26U)
#define | TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_SHIFT)) & TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_MASK)
#define | TSC_DEBUG_MODE_DEBUG_EN_MASK (0x10000000U)
#define | TSC_DEBUG_MODE_DEBUG_EN_SHIFT (28U)
#define | TSC_DEBUG_MODE_DEBUG_EN(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_DEBUG_EN_SHIFT)) & TSC_DEBUG_MODE_DEBUG_EN_MASK)

## DEBUG_MODE2 - Debug Mode Register 2

#define | TSC_DEBUG_MODE2_XPUL_PULL_DOWN_MASK (0x1U)
#define | TSC_DEBUG_MODE2_XPUL_PULL_DOWN_SHIFT (0U)
#define | TSC_DEBUG_MODE2_XPUL_PULL_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XPUL_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_XPUL_PULL_DOWN_MASK)
#define | TSC_DEBUG_MODE2_XPUL_PULL_UP_MASK (0x2U)
#define | TSC_DEBUG_MODE2_XPUL_PULL_UP_SHIFT (1U)
#define | TSC_DEBUG_MODE2_XPUL_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XPUL_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XPUL_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_MASK (0x4U)
#define | TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_SHIFT (2U)
#define | TSC_DEBUG_MODE2_XPUL_200K_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_XNUR_PULL_DOWN_MASK (0x8U)
#define | TSC_DEBUG_MODE2_XNUR_PULL_DOWN_SHIFT (3U)
#define | TSC_DEBUG_MODE2_XNUR_PULL_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XNUR_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_XNUR_PULL_DOWN_MASK)
#define | TSC_DEBUG_MODE2_XNUR_PULL_UP_MASK (0x10U)
#define | TSC_DEBUG_MODE2_XNUR_PULL_UP_SHIFT (4U)
#define | TSC_DEBUG_MODE2_XNUR_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XNUR_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XNUR_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_MASK (0x20U)
#define | TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_SHIFT (5U)
#define | TSC_DEBUG_MODE2_XNUR_200K_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_YPLL_PULL_DOWN_MASK (0x40U)
#define | TSC_DEBUG_MODE2_YPLL_PULL_DOWN_SHIFT (6U)
#define | TSC_DEBUG_MODE2_YPLL_PULL_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YPLL_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_YPLL_PULL_DOWN_MASK)
#define | TSC_DEBUG_MODE2_YPLL_PULL_UP_MASK (0x80U)
#define | TSC_DEBUG_MODE2_YPLL_PULL_UP_SHIFT (7U)
#define | TSC_DEBUG_MODE2_YPLL_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YPLL_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YPLL_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_MASK (0x100U)
#define | TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_SHIFT (8U)
#define | TSC_DEBUG_MODE2_YPLL_200K_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_YNLR_PULL_DOWN_MASK (0x200U)
#define | TSC_DEBUG_MODE2_YNLR_PULL_DOWN_SHIFT (9U)
#define | TSC_DEBUG_MODE2_YNLR_PULL_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YNLR_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_YNLR_PULL_DOWN_MASK)
#define | TSC_DEBUG_MODE2_YNLR_PULL_UP_MASK (0x400U)
#define | TSC_DEBUG_MODE2_YNLR_PULL_UP_SHIFT (10U)
#define | TSC_DEBUG_MODE2_YNLR_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YNLR_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YNLR_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_MASK (0x800U)
#define | TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_SHIFT (11U)
#define | TSC_DEBUG_MODE2_YNLR_200K_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_WIPER_PULL_DOWN_MASK (0x1000U)
#define | TSC_DEBUG_MODE2_WIPER_PULL_DOWN_SHIFT (12U)
#define | TSC_DEBUG_MODE2_WIPER_PULL_DOWN(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_WIPER_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_WIPER_PULL_DOWN_MASK)
#define | TSC_DEBUG_MODE2_WIPER_PULL_UP_MASK (0x2000U)
#define | TSC_DEBUG_MODE2_WIPER_PULL_UP_SHIFT (13U)
#define | TSC_DEBUG_MODE2_WIPER_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_WIPER_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_WIPER_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_MASK (0x4000U)
#define | TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_SHIFT (14U)
#define | TSC_DEBUG_MODE2_WIPER_200K_PULL_UP(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_MASK)
#define | TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_MASK (0x10000U)
#define | TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_SHIFT (16U)
#define | TSC_DEBUG_MODE2_DETECT_FOUR_WIRE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_MASK)
#define | TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_MASK (0x20000U)
#define | TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_SHIFT (17U)
#define | TSC_DEBUG_MODE2_DETECT_FIVE_WIRE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_MASK)
#define | TSC_DEBUG_MODE2_STATE_MACHINE_MASK (0x700000U)
#define | TSC_DEBUG_MODE2_STATE_MACHINE_SHIFT (20U)
#define | TSC_DEBUG_MODE2_STATE_MACHINE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_STATE_MACHINE_SHIFT)) & TSC_DEBUG_MODE2_STATE_MACHINE_MASK)
#define | TSC_DEBUG_MODE2_INTERMEDIATE_MASK (0x800000U)
#define | TSC_DEBUG_MODE2_INTERMEDIATE_SHIFT (23U)
#define | TSC_DEBUG_MODE2_INTERMEDIATE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_INTERMEDIATE_SHIFT)) & TSC_DEBUG_MODE2_INTERMEDIATE_MASK)
#define | TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_MASK (0x1000000U)
#define | TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_SHIFT (24U)
#define | TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_MASK)
#define | TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_MASK (0x10000000U)
#define | TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_SHIFT (28U)
#define | TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_MASK)
#define | TSC_DEBUG_MODE2_DE_GLITCH_MASK (0x60000000U)
#define | TSC_DEBUG_MODE2_DE_GLITCH_SHIFT (29U)
#define | TSC_DEBUG_MODE2_DE_GLITCH(x) (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DE_GLITCH_SHIFT)) & TSC_DEBUG_MODE2_DE_GLITCH_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ TSC_BASIC_SETTING_AUTO_MEASURE

#define TSC_BASIC_SETTING_AUTO_MEASURE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_BASIC_SETTING_AUTO_MEASURE_SHIFT)) & TSC_BASIC_SETTING_AUTO_MEASURE_MASK)

AUTO_MEASURE - Auto Measure 0b0..Disable Auto Measure 0b1..Auto Measure

Definition at line 40968 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_AUTO_MEASURE_MASK

#define TSC_BASIC_SETTING_AUTO_MEASURE_MASK (0x1U)

Definition at line 40962 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_AUTO_MEASURE_SHIFT

#define TSC_BASIC_SETTING_AUTO_MEASURE_SHIFT (0U)

Definition at line 40963 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_MEASURE_DELAY_TIME

#define TSC_BASIC_SETTING_MEASURE_DELAY_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_BASIC_SETTING_MEASURE_DELAY_TIME_SHIFT)) & TSC_BASIC_SETTING_MEASURE_DELAY_TIME_MASK)

MEASURE_DELAY_TIME - Measure Delay Time

Definition at line 40980 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_MEASURE_DELAY_TIME_MASK

#define TSC_BASIC_SETTING_MEASURE_DELAY_TIME_MASK (0xFFFFFF00U)

Definition at line 40976 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_MEASURE_DELAY_TIME_SHIFT

#define TSC_BASIC_SETTING_MEASURE_DELAY_TIME_SHIFT (8U)

Definition at line 40977 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_WIRE_4_5

#define TSC_BASIC_SETTING_WIRE_4_5 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_BASIC_SETTING_WIRE_4_5_SHIFT)) & TSC_BASIC_SETTING_WIRE_4_5_MASK)

WIRE_4_5 - 4/5 Wire detection 0b0..4-Wire Detection Mode 0b1..5-Wire Detection Mode

Definition at line 40975 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_WIRE_4_5_MASK

#define TSC_BASIC_SETTING_WIRE_4_5_MASK (0x10U)

Definition at line 40969 of file MIMXRT1062.h.

## ◆ TSC_BASIC_SETTING_WIRE_4_5_SHIFT

#define TSC_BASIC_SETTING_WIRE_4_5_SHIFT (4U)

Definition at line 40970 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DE_GLITCH

#define TSC_DEBUG_MODE2_DE_GLITCH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DE_GLITCH_SHIFT)) & TSC_DEBUG_MODE2_DE_GLITCH_MASK)

DE_GLITCH 0b00..Normal function: 0x1fff ipg clock cycles; Low power mode: 0x9 low power clock cycles 0b01..Normal function: 0xfff ipg clock cycles; Low power mode: :0x7 low power clock cycles 0b10..Normal function: 0x7ff ipg clock cycles; Low power mode:0x5 low power clock cycles 0b11..Normal function: 0x3 ipg clock cycles; Low power mode:0x3 low power clock cycles

Definition at line 41337 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DE_GLITCH_MASK

#define TSC_DEBUG_MODE2_DE_GLITCH_MASK (0x60000000U)

Definition at line 41329 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DE_GLITCH_SHIFT

#define TSC_DEBUG_MODE2_DE_GLITCH_SHIFT (29U)

Definition at line 41330 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE

#define TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_MASK)

DETECT_ENABLE_FIVE_WIRE - Detect Enable Five Wire 0b0..Do not read five wire detect value, read default value from analogue 0b1..Read five wire detect status from analogue

Definition at line 41328 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_MASK

#define TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_MASK (0x10000000U)

Definition at line 41322 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_SHIFT

#define TSC_DEBUG_MODE2_DETECT_ENABLE_FIVE_WIRE_SHIFT (28U)

Definition at line 41323 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE

#define TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_MASK)

DETECT_ENABLE_FOUR_WIRE - Detect Enable Four Wire 0b0..Do not read four wire detect value, read default value from analogue 0b1..Read four wire detect status from analogue

Definition at line 41321 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_MASK

#define TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_MASK (0x1000000U)

Definition at line 41315 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_SHIFT

#define TSC_DEBUG_MODE2_DETECT_ENABLE_FOUR_WIRE_SHIFT (24U)

Definition at line 41316 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_FIVE_WIRE

#define TSC_DEBUG_MODE2_DETECT_FIVE_WIRE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_MASK)

DETECT_FIVE_WIRE - Detect Five Wire 0b0..No detect signal 0b1..Yes, there is a detect on the touch screen.

Definition at line 41295 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_MASK

#define TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_MASK (0x20000U)

Definition at line 41289 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_SHIFT

#define TSC_DEBUG_MODE2_DETECT_FIVE_WIRE_SHIFT (17U)

Definition at line 41290 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_FOUR_WIRE

#define TSC_DEBUG_MODE2_DETECT_FOUR_WIRE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_SHIFT)) & TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_MASK)

DETECT_FOUR_WIRE - Detect Four Wire 0b0..No detect signal 0b1..Yes, there is a detect on the touch screen.

Definition at line 41288 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_MASK

#define TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_MASK (0x10000U)

Definition at line 41282 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_SHIFT

#define TSC_DEBUG_MODE2_DETECT_FOUR_WIRE_SHIFT (16U)

Definition at line 41283 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_INTERMEDIATE

#define TSC_DEBUG_MODE2_INTERMEDIATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_INTERMEDIATE_SHIFT)) & TSC_DEBUG_MODE2_INTERMEDIATE_MASK)

INTERMEDIATE - Intermediate State 0b0..Not in intermedia 0b1..Intermedia

Definition at line 41314 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_INTERMEDIATE_MASK

#define TSC_DEBUG_MODE2_INTERMEDIATE_MASK (0x800000U)

Definition at line 41308 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_INTERMEDIATE_SHIFT

#define TSC_DEBUG_MODE2_INTERMEDIATE_SHIFT (23U)

Definition at line 41309 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_STATE_MACHINE

#define TSC_DEBUG_MODE2_STATE_MACHINE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_STATE_MACHINE_SHIFT)) & TSC_DEBUG_MODE2_STATE_MACHINE_MASK)

STATE_MACHINE - State Machine 0b000..Idle 0b001..Pre-charge 0b010..Detect 0b011..X-measure 0b100..Y-measure 0b101..Pre-charge 0b110..Detect

Definition at line 41307 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_STATE_MACHINE_MASK

#define TSC_DEBUG_MODE2_STATE_MACHINE_MASK (0x700000U)

Definition at line 41296 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_STATE_MACHINE_SHIFT

#define TSC_DEBUG_MODE2_STATE_MACHINE_SHIFT (20U)

Definition at line 41297 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_200K_PULL_UP

#define TSC_DEBUG_MODE2_WIPER_200K_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_MASK)

WIPER_200K_PULL_UP - Wiper Wire 200K Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41281 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_MASK

#define TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_MASK (0x4000U)

Definition at line 41275 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_WIPER_200K_PULL_UP_SHIFT (14U)

Definition at line 41276 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_PULL_DOWN

#define TSC_DEBUG_MODE2_WIPER_PULL_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_WIPER_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_WIPER_PULL_DOWN_MASK)

WIPER_PULL_DOWN - Wiper Wire Pull Down Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41267 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_PULL_DOWN_MASK

#define TSC_DEBUG_MODE2_WIPER_PULL_DOWN_MASK (0x1000U)

Definition at line 41261 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_PULL_DOWN_SHIFT

#define TSC_DEBUG_MODE2_WIPER_PULL_DOWN_SHIFT (12U)

Definition at line 41262 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_PULL_UP

#define TSC_DEBUG_MODE2_WIPER_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_WIPER_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_WIPER_PULL_UP_MASK)

WIPER_PULL_UP - Wiper Wire Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41274 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_PULL_UP_MASK

#define TSC_DEBUG_MODE2_WIPER_PULL_UP_MASK (0x2000U)

Definition at line 41268 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_WIPER_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_WIPER_PULL_UP_SHIFT (13U)

Definition at line 41269 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_200K_PULL_UP

#define TSC_DEBUG_MODE2_XNUR_200K_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_MASK)

XNUR_200K_PULL_UP - XNUR Wire 200K Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41218 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_MASK

#define TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_MASK (0x20U)

Definition at line 41212 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_XNUR_200K_PULL_UP_SHIFT (5U)

Definition at line 41213 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_PULL_DOWN

#define TSC_DEBUG_MODE2_XNUR_PULL_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XNUR_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_XNUR_PULL_DOWN_MASK)

XNUR_PULL_DOWN - XNUR Wire Pull Down Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41204 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_PULL_DOWN_MASK

#define TSC_DEBUG_MODE2_XNUR_PULL_DOWN_MASK (0x8U)

Definition at line 41198 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_PULL_DOWN_SHIFT

#define TSC_DEBUG_MODE2_XNUR_PULL_DOWN_SHIFT (3U)

Definition at line 41199 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_PULL_UP

#define TSC_DEBUG_MODE2_XNUR_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XNUR_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XNUR_PULL_UP_MASK)

XNUR_PULL_UP - XNUR Wire Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41211 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_PULL_UP_MASK

#define TSC_DEBUG_MODE2_XNUR_PULL_UP_MASK (0x10U)

Definition at line 41205 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XNUR_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_XNUR_PULL_UP_SHIFT (4U)

Definition at line 41206 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_200K_PULL_UP

#define TSC_DEBUG_MODE2_XPUL_200K_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_MASK)

XPUL_200K_PULL_UP - XPUL Wire 200K Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41197 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_MASK

#define TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_MASK (0x4U)

Definition at line 41191 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_XPUL_200K_PULL_UP_SHIFT (2U)

Definition at line 41192 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_PULL_DOWN

#define TSC_DEBUG_MODE2_XPUL_PULL_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XPUL_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_XPUL_PULL_DOWN_MASK)

XPUL_PULL_DOWN - XPUL Wire Pull Down Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41183 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_PULL_DOWN_MASK

#define TSC_DEBUG_MODE2_XPUL_PULL_DOWN_MASK (0x1U)

Definition at line 41177 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_PULL_DOWN_SHIFT

#define TSC_DEBUG_MODE2_XPUL_PULL_DOWN_SHIFT (0U)

Definition at line 41178 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_PULL_UP

#define TSC_DEBUG_MODE2_XPUL_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_XPUL_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_XPUL_PULL_UP_MASK)

XPUL_PULL_UP - XPUL Wire Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41190 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_PULL_UP_MASK

#define TSC_DEBUG_MODE2_XPUL_PULL_UP_MASK (0x2U)

Definition at line 41184 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_XPUL_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_XPUL_PULL_UP_SHIFT (1U)

Definition at line 41185 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_200K_PULL_UP

#define TSC_DEBUG_MODE2_YNLR_200K_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_MASK)

YNLR_200K_PULL_UP - YNLR Wire 200K Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41260 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_MASK

#define TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_MASK (0x800U)

Definition at line 41254 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_YNLR_200K_PULL_UP_SHIFT (11U)

Definition at line 41255 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_PULL_DOWN

#define TSC_DEBUG_MODE2_YNLR_PULL_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YNLR_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_YNLR_PULL_DOWN_MASK)

YNLR_PULL_DOWN - YNLR Wire Pull Down Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41246 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_PULL_DOWN_MASK

#define TSC_DEBUG_MODE2_YNLR_PULL_DOWN_MASK (0x200U)

Definition at line 41240 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_PULL_DOWN_SHIFT

#define TSC_DEBUG_MODE2_YNLR_PULL_DOWN_SHIFT (9U)

Definition at line 41241 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_PULL_UP

#define TSC_DEBUG_MODE2_YNLR_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YNLR_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YNLR_PULL_UP_MASK)

YNLR_PULL_UP - YNLR Wire Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41253 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_PULL_UP_MASK

#define TSC_DEBUG_MODE2_YNLR_PULL_UP_MASK (0x400U)

Definition at line 41247 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YNLR_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_YNLR_PULL_UP_SHIFT (10U)

Definition at line 41248 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_200K_PULL_UP

#define TSC_DEBUG_MODE2_YPLL_200K_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_MASK)

YPLL_200K_PULL_UP - YPLL Wire 200K Pull Up Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41239 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_MASK

#define TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_MASK (0x100U)

Definition at line 41233 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_YPLL_200K_PULL_UP_SHIFT (8U)

Definition at line 41234 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_PULL_DOWN

#define TSC_DEBUG_MODE2_YPLL_PULL_DOWN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YPLL_PULL_DOWN_SHIFT)) & TSC_DEBUG_MODE2_YPLL_PULL_DOWN_MASK)

YPLL_PULL_DOWN - YPLL Wire Pull Down Switch 0b0..Close the switch 0b1..Open up the switch

Definition at line 41225 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_PULL_DOWN_MASK

#define TSC_DEBUG_MODE2_YPLL_PULL_DOWN_MASK (0x40U)

Definition at line 41219 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_PULL_DOWN_SHIFT

#define TSC_DEBUG_MODE2_YPLL_PULL_DOWN_SHIFT (6U)

Definition at line 41220 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_PULL_UP

#define TSC_DEBUG_MODE2_YPLL_PULL_UP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE2_YPLL_PULL_UP_SHIFT)) & TSC_DEBUG_MODE2_YPLL_PULL_UP_MASK)

YPLL_PULL_UP - YPLL Wire Pull Up Switch 0b0..Close the switch 0b1..Open the switch

Definition at line 41232 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_PULL_UP_MASK

#define TSC_DEBUG_MODE2_YPLL_PULL_UP_MASK (0x80U)

Definition at line 41226 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE2_YPLL_PULL_UP_SHIFT

#define TSC_DEBUG_MODE2_YPLL_PULL_UP_SHIFT (7U)

Definition at line 41227 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO

#define TSC_DEBUG_MODE_ADC_COCO | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_COCO_SHIFT)) & TSC_DEBUG_MODE_ADC_COCO_MASK)

ADC_COCO - ADC COCO Signal

Definition at line 41139 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_CLEAR

#define TSC_DEBUG_MODE_ADC_COCO_CLEAR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_COCO_CLEAR_SHIFT)) & TSC_DEBUG_MODE_ADC_COCO_CLEAR_MASK)

ADC_COCO_CLEAR - ADC Coco Clear 0b0..No ADC COCO clear 0b1..Set ADC COCO clear

Definition at line 41158 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE

#define TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_SHIFT)) & TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_MASK)

ADC_COCO_CLEAR_DISABLE - ADC COCO Clear Disable 0b0..Allow TSC hardware generates ADC COCO clear 0b1..Prevent TSC from generate ADC COCO clear signal

Definition at line 41165 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_MASK

#define TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_MASK (0x4000000U)

Definition at line 41159 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_SHIFT

#define TSC_DEBUG_MODE_ADC_COCO_CLEAR_DISABLE_SHIFT (26U)

Definition at line 41160 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_CLEAR_MASK

#define TSC_DEBUG_MODE_ADC_COCO_CLEAR_MASK (0x2000000U)

Definition at line 41152 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_CLEAR_SHIFT

#define TSC_DEBUG_MODE_ADC_COCO_CLEAR_SHIFT (25U)

Definition at line 41153 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_MASK

#define TSC_DEBUG_MODE_ADC_COCO_MASK (0x1000U)

Definition at line 41135 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_COCO_SHIFT

#define TSC_DEBUG_MODE_ADC_COCO_SHIFT (12U)

Definition at line 41136 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_CONV_VALUE

#define TSC_DEBUG_MODE_ADC_CONV_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_ADC_CONV_VALUE_SHIFT)) & TSC_DEBUG_MODE_ADC_CONV_VALUE_MASK)

ADC_CONV_VALUE - ADC Conversion Value

Definition at line 41134 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_CONV_VALUE_MASK

#define TSC_DEBUG_MODE_ADC_CONV_VALUE_MASK (0xFFFU)

Definition at line 41130 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_ADC_CONV_VALUE_SHIFT

#define TSC_DEBUG_MODE_ADC_CONV_VALUE_SHIFT (0U)

Definition at line 41131 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_DEBUG_EN

#define TSC_DEBUG_MODE_DEBUG_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_DEBUG_EN_SHIFT)) & TSC_DEBUG_MODE_DEBUG_EN_MASK)

DEBUG_EN - Debug Enable 0b0..Enable debug mode 0b1..Disable debug mode

Definition at line 41172 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_DEBUG_EN_MASK

#define TSC_DEBUG_MODE_DEBUG_EN_MASK (0x10000000U)

Definition at line 41166 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_DEBUG_EN_SHIFT

#define TSC_DEBUG_MODE_DEBUG_EN_SHIFT (28U)

Definition at line 41167 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_EXT_HWTS

#define TSC_DEBUG_MODE_EXT_HWTS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_EXT_HWTS_SHIFT)) & TSC_DEBUG_MODE_EXT_HWTS_MASK)

EXT_HWTS - Hardware Trigger Select Signal

Definition at line 41144 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_EXT_HWTS_MASK

#define TSC_DEBUG_MODE_EXT_HWTS_MASK (0x1F0000U)

Definition at line 41140 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_EXT_HWTS_SHIFT

#define TSC_DEBUG_MODE_EXT_HWTS_SHIFT (16U)

Definition at line 41141 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_TRIGGER

#define TSC_DEBUG_MODE_TRIGGER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_DEBUG_MODE_TRIGGER_SHIFT)) & TSC_DEBUG_MODE_TRIGGER_MASK)

TRIGGER - Trigger 0b0..No hardware trigger signal 0b1..Hardware trigger signal, the signal must last at least 1 ips clock period

Definition at line 41151 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_TRIGGER_MASK

#define TSC_DEBUG_MODE_TRIGGER_MASK (0x1000000U)

Definition at line 41145 of file MIMXRT1062.h.

## ◆ TSC_DEBUG_MODE_TRIGGER_SHIFT

#define TSC_DEBUG_MODE_TRIGGER_SHIFT (24U)

Definition at line 41146 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_DISABLE

#define TSC_FLOW_CONTROL_DISABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_DISABLE_SHIFT)) & TSC_FLOW_CONTROL_DISABLE_MASK)

DISABLE 0b0..Leave HW state machine control 0b1..SW set to idle status

Definition at line 41024 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_DISABLE_MASK

#define TSC_FLOW_CONTROL_DISABLE_MASK (0x10000U)

Definition at line 41018 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_DISABLE_SHIFT

#define TSC_FLOW_CONTROL_DISABLE_SHIFT (16U)

Definition at line 41019 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_DROP_MEASURE

#define TSC_FLOW_CONTROL_DROP_MEASURE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_DROP_MEASURE_SHIFT)) & TSC_FLOW_CONTROL_DROP_MEASURE_MASK)

DROP_MEASURE - Drop Measure 0b0..Do not drop measure for now 0b1..Drop the measure and controller return to idle status

Definition at line 41010 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_DROP_MEASURE_MASK

#define TSC_FLOW_CONTROL_DROP_MEASURE_MASK (0x100U)

Definition at line 41004 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_DROP_MEASURE_SHIFT

#define TSC_FLOW_CONTROL_DROP_MEASURE_SHIFT (8U)

Definition at line 41005 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_START_MEASURE

#define TSC_FLOW_CONTROL_START_MEASURE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_START_MEASURE_SHIFT)) & TSC_FLOW_CONTROL_START_MEASURE_MASK)

START_MEASURE - Start Measure 0b0..Do not start measure for now 0b1..Start measure the X/Y coordinate value

Definition at line 41003 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_START_MEASURE_MASK

#define TSC_FLOW_CONTROL_START_MEASURE_MASK (0x10U)

Definition at line 40997 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_START_MEASURE_SHIFT

#define TSC_FLOW_CONTROL_START_MEASURE_SHIFT (4U)

Definition at line 40998 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_START_SENSE

#define TSC_FLOW_CONTROL_START_SENSE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_START_SENSE_SHIFT)) & TSC_FLOW_CONTROL_START_SENSE_MASK)

START_SENSE - Start Sense 0b0..Stay at idle status 0b1..Start sense detection and (if auto_measure set to 1) measure after detect a touch

Definition at line 41017 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_START_SENSE_MASK

#define TSC_FLOW_CONTROL_START_SENSE_MASK (0x1000U)

Definition at line 41011 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_START_SENSE_SHIFT

#define TSC_FLOW_CONTROL_START_SENSE_SHIFT (12U)

Definition at line 41012 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_SW_RST

#define TSC_FLOW_CONTROL_SW_RST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_FLOW_CONTROL_SW_RST_SHIFT)) & TSC_FLOW_CONTROL_SW_RST_MASK)

SW_RST - Soft Reset

Definition at line 40996 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_SW_RST_MASK

#define TSC_FLOW_CONTROL_SW_RST_MASK (0x1U)

Definition at line 40992 of file MIMXRT1062.h.

## ◆ TSC_FLOW_CONTROL_SW_RST_SHIFT

#define TSC_FLOW_CONTROL_SW_RST_SHIFT (0U)

Definition at line 40993 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_DETECT_INT_EN

#define TSC_INT_EN_DETECT_INT_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_EN_DETECT_INT_EN_SHIFT)) & TSC_INT_EN_DETECT_INT_EN_MASK)

DETECT_INT_EN - Detect Interrupt Enable 0b0..Disable detect interrupt 0b1..Enable detect interrupt

Definition at line 41056 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_DETECT_INT_EN_MASK

#define TSC_INT_EN_DETECT_INT_EN_MASK (0x10U)

Definition at line 41050 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_DETECT_INT_EN_SHIFT

#define TSC_INT_EN_DETECT_INT_EN_SHIFT (4U)

Definition at line 41051 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_IDLE_SW_INT_EN

#define TSC_INT_EN_IDLE_SW_INT_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_EN_IDLE_SW_INT_EN_SHIFT)) & TSC_INT_EN_IDLE_SW_INT_EN_MASK)

IDLE_SW_INT_EN - Idle Software Interrupt Enable 0b0..Disable idle software interrupt 0b1..Enable idle software interrupt

Definition at line 41063 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_IDLE_SW_INT_EN_MASK

#define TSC_INT_EN_IDLE_SW_INT_EN_MASK (0x1000U)

Definition at line 41057 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_IDLE_SW_INT_EN_SHIFT

#define TSC_INT_EN_IDLE_SW_INT_EN_SHIFT (12U)

Definition at line 41058 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_MEASURE_INT_EN

#define TSC_INT_EN_MEASURE_INT_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_EN_MEASURE_INT_EN_SHIFT)) & TSC_INT_EN_MEASURE_INT_EN_MASK)

MEASURE_INT_EN - Measure Interrupt Enable 0b0..Disable measure interrupt 0b1..Enable measure interrupt

Definition at line 41049 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_MEASURE_INT_EN_MASK

#define TSC_INT_EN_MEASURE_INT_EN_MASK (0x1U)

Definition at line 41043 of file MIMXRT1062.h.

## ◆ TSC_INT_EN_MEASURE_INT_EN_SHIFT

#define TSC_INT_EN_MEASURE_INT_EN_SHIFT (0U)

Definition at line 41044 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_DETECT_SIG_EN

#define TSC_INT_SIG_EN_DETECT_SIG_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_DETECT_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_DETECT_SIG_EN_MASK)

DETECT_SIG_EN - Detect Signal Enable 0b0..Disable detect signal 0b1..Enable detect signal

Definition at line 41079 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_DETECT_SIG_EN_MASK

#define TSC_INT_SIG_EN_DETECT_SIG_EN_MASK (0x10U)

Definition at line 41073 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_DETECT_SIG_EN_SHIFT

#define TSC_INT_SIG_EN_DETECT_SIG_EN_SHIFT (4U)

Definition at line 41074 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_IDLE_SW_SIG_EN

#define TSC_INT_SIG_EN_IDLE_SW_SIG_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_IDLE_SW_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_IDLE_SW_SIG_EN_MASK)

IDLE_SW_SIG_EN - Idle Software Signal Enable 0b0..Disable idle software signal 0b1..Enable idle software signal

Definition at line 41093 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_IDLE_SW_SIG_EN_MASK

#define TSC_INT_SIG_EN_IDLE_SW_SIG_EN_MASK (0x1000U)

Definition at line 41087 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_IDLE_SW_SIG_EN_SHIFT

#define TSC_INT_SIG_EN_IDLE_SW_SIG_EN_SHIFT (12U)

Definition at line 41088 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_MEASURE_SIG_EN

#define TSC_INT_SIG_EN_MEASURE_SIG_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_MEASURE_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_MEASURE_SIG_EN_MASK)

MEASURE_SIG_EN - Measure Signal Enable

Definition at line 41072 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_MEASURE_SIG_EN_MASK

#define TSC_INT_SIG_EN_MEASURE_SIG_EN_MASK (0x1U)

Definition at line 41068 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_MEASURE_SIG_EN_SHIFT

#define TSC_INT_SIG_EN_MEASURE_SIG_EN_SHIFT (0U)

Definition at line 41069 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_VALID_SIG_EN

#define TSC_INT_SIG_EN_VALID_SIG_EN | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_SIG_EN_VALID_SIG_EN_SHIFT)) & TSC_INT_SIG_EN_VALID_SIG_EN_MASK)

VALID_SIG_EN - Valid Signal Enable 0b0..Disable valid signal 0b1..Enable valid signal

Definition at line 41086 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_VALID_SIG_EN_MASK

#define TSC_INT_SIG_EN_VALID_SIG_EN_MASK (0x100U)

Definition at line 41080 of file MIMXRT1062.h.

## ◆ TSC_INT_SIG_EN_VALID_SIG_EN_SHIFT

#define TSC_INT_SIG_EN_VALID_SIG_EN_SHIFT (8U)

Definition at line 41081 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_DETECT

#define TSC_INT_STATUS_DETECT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_DETECT_SHIFT)) & TSC_INT_STATUS_DETECT_MASK)

DETECT - Detect Signal 0b0..Does not exist a detect signal 0b1..Exist detect signal

Definition at line 41111 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_DETECT_MASK

#define TSC_INT_STATUS_DETECT_MASK (0x10U)

Definition at line 41105 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_DETECT_SHIFT

#define TSC_INT_STATUS_DETECT_SHIFT (4U)

Definition at line 41106 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_IDLE_SW

#define TSC_INT_STATUS_IDLE_SW | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_IDLE_SW_SHIFT)) & TSC_INT_STATUS_IDLE_SW_MASK)

IDLE_SW - Idle Software 0b0..Haven't return to idle status 0b1..Already return to idle status

Definition at line 41125 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_IDLE_SW_MASK

#define TSC_INT_STATUS_IDLE_SW_MASK (0x1000U)

Definition at line 41119 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_IDLE_SW_SHIFT

#define TSC_INT_STATUS_IDLE_SW_SHIFT (12U)

Definition at line 41120 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_MEASURE

#define TSC_INT_STATUS_MEASURE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_MEASURE_SHIFT)) & TSC_INT_STATUS_MEASURE_MASK)

MEASURE - Measure Signal 0b0..Does not exist a measure signal 0b1..Exist a measure signal

Definition at line 41104 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_MEASURE_MASK

#define TSC_INT_STATUS_MEASURE_MASK (0x1U)

Definition at line 41098 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_MEASURE_SHIFT

#define TSC_INT_STATUS_MEASURE_SHIFT (0U)

Definition at line 41099 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_VALID

#define TSC_INT_STATUS_VALID | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_INT_STATUS_VALID_SHIFT)) & TSC_INT_STATUS_VALID_MASK)

VALID - Valid Signal 0b0..There is no touch detected after measurement, indicates that the measured value is not valid 0b1..There is touch detection after measurement, indicates that the measure is valid

Definition at line 41118 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_VALID_MASK

#define TSC_INT_STATUS_VALID_MASK (0x100U)

Definition at line 41112 of file MIMXRT1062.h.

## ◆ TSC_INT_STATUS_VALID_SHIFT

#define TSC_INT_STATUS_VALID_SHIFT (8U)

Definition at line 41113 of file MIMXRT1062.h.

## ◆ TSC_MEASEURE_VALUE_X_VALUE

#define TSC_MEASEURE_VALUE_X_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_MEASEURE_VALUE_X_VALUE_SHIFT)) & TSC_MEASEURE_VALUE_X_VALUE_MASK)

X_VALUE - X Value

Definition at line 41038 of file MIMXRT1062.h.

## ◆ TSC_MEASEURE_VALUE_X_VALUE_MASK

#define TSC_MEASEURE_VALUE_X_VALUE_MASK (0xFFF0000U)

Definition at line 41034 of file MIMXRT1062.h.

## ◆ TSC_MEASEURE_VALUE_X_VALUE_SHIFT

#define TSC_MEASEURE_VALUE_X_VALUE_SHIFT (16U)

Definition at line 41035 of file MIMXRT1062.h.

## ◆ TSC_MEASEURE_VALUE_Y_VALUE

#define TSC_MEASEURE_VALUE_Y_VALUE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_MEASEURE_VALUE_Y_VALUE_SHIFT)) & TSC_MEASEURE_VALUE_Y_VALUE_MASK)

Y_VALUE - Y Value

Definition at line 41033 of file MIMXRT1062.h.

## ◆ TSC_MEASEURE_VALUE_Y_VALUE_MASK

#define TSC_MEASEURE_VALUE_Y_VALUE_MASK (0xFFFU)

Definition at line 41029 of file MIMXRT1062.h.

## ◆ TSC_MEASEURE_VALUE_Y_VALUE_SHIFT

#define TSC_MEASEURE_VALUE_Y_VALUE_SHIFT (0U)

Definition at line 41030 of file MIMXRT1062.h.

## ◆ TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME

#define TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_SHIFT)) & TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_MASK)

Definition at line 40987 of file MIMXRT1062.h.

## ◆ TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_MASK

#define TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_MASK (0xFFFFFFFFU)

Definition at line 40985 of file MIMXRT1062.h.

## ◆ TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_SHIFT

#define TSC_PRE_CHARGE_TIME_PRE_CHARGE_TIME_SHIFT (0U)

Definition at line 40986 of file MIMXRT1062.h.