Callisto4Bootloader: FLEXSPI_Type Struct Reference

Callisto4Bootloader

Data Fields
FLEXSPI_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » FLEXSPI Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | MCR0
__IO uint32_t | MCR1
__IO uint32_t | MCR2
__IO uint32_t | AHBCR
__IO uint32_t | INTEN
__IO uint32_t | INTR
__IO uint32_t | LUTKEY
__IO uint32_t | LUTCR
__IO uint32_t | AHBRXBUFCR0 [4]
uint8_t | RESERVED_0 [48]
__IO uint32_t | FLSHCR0 [4]
__IO uint32_t | FLSHCR1 [4]
__IO uint32_t | FLSHCR2 [4]
uint8_t | RESERVED_1 [4]
__IO uint32_t | FLSHCR4
uint8_t | RESERVED_2 [8]
__IO uint32_t | IPCR0
__IO uint32_t | IPCR1
uint8_t | RESERVED_3 [8]
__IO uint32_t | IPCMD
uint8_t | RESERVED_4 [4]
__IO uint32_t | IPRXFCR
__IO uint32_t | IPTXFCR
__IO uint32_t | DLLCR [2]
uint8_t | RESERVED_5 [24]
__I uint32_t | STS0
__I uint32_t | STS1
__I uint32_t | STS2
__I uint32_t | AHBSPNDSTS
__I uint32_t | IPRXFSTS
__I uint32_t | IPTXFSTS
uint8_t | RESERVED_6 [8]
__I uint32_t | RFDR [32]
__O uint32_t | TFDR [32]
__IO uint32_t | LUT [64]

## Detailed Description

FLEXSPI - Register Layout Typedef

Definition at line 19281 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h