Callisto4Bootloader: PXP Register Masks

Callisto4Bootloader

PXP Register Masks
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » PXP Peripheral Access Layer

## CTRL - Control Register 0

#define | PXP_CTRL_ENABLE_MASK (0x1U)
#define | PXP_CTRL_ENABLE_SHIFT (0U)
#define | PXP_CTRL_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ENABLE_SHIFT)) & PXP_CTRL_ENABLE_MASK)
#define | PXP_CTRL_IRQ_ENABLE_MASK (0x2U)
#define | PXP_CTRL_IRQ_ENABLE_SHIFT (1U)
#define | PXP_CTRL_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_IRQ_ENABLE_SHIFT)) & PXP_CTRL_IRQ_ENABLE_MASK)
#define | PXP_CTRL_NEXT_IRQ_ENABLE_MASK (0x4U)
#define | PXP_CTRL_NEXT_IRQ_ENABLE_SHIFT (2U)
#define | PXP_CTRL_NEXT_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_NEXT_IRQ_ENABLE_MASK)
#define | PXP_CTRL_ENABLE_LCD_HANDSHAKE_MASK (0x10U)
#define | PXP_CTRL_ENABLE_LCD_HANDSHAKE_SHIFT (4U)
#define | PXP_CTRL_ENABLE_LCD_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_ENABLE_LCD_HANDSHAKE_MASK)
#define | PXP_CTRL_RSVD0_MASK (0xE0U)
#define | PXP_CTRL_RSVD0_SHIFT (5U)
#define | PXP_CTRL_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD0_SHIFT)) & PXP_CTRL_RSVD0_MASK)
#define | PXP_CTRL_ROTATE_MASK (0x300U)
#define | PXP_CTRL_ROTATE_SHIFT (8U)
#define | PXP_CTRL_ROTATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ROTATE_SHIFT)) & PXP_CTRL_ROTATE_MASK)
#define | PXP_CTRL_HFLIP_MASK (0x400U)
#define | PXP_CTRL_HFLIP_SHIFT (10U)
#define | PXP_CTRL_HFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_HFLIP_SHIFT)) & PXP_CTRL_HFLIP_MASK)
#define | PXP_CTRL_VFLIP_MASK (0x800U)
#define | PXP_CTRL_VFLIP_SHIFT (11U)
#define | PXP_CTRL_VFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_VFLIP_SHIFT)) & PXP_CTRL_VFLIP_MASK)
#define | PXP_CTRL_RSVD1_MASK (0x3FF000U)
#define | PXP_CTRL_RSVD1_SHIFT (12U)
#define | PXP_CTRL_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD1_SHIFT)) & PXP_CTRL_RSVD1_MASK)
#define | PXP_CTRL_ROT_POS_MASK (0x400000U)
#define | PXP_CTRL_ROT_POS_SHIFT (22U)
#define | PXP_CTRL_ROT_POS(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ROT_POS_SHIFT)) & PXP_CTRL_ROT_POS_MASK)
#define | PXP_CTRL_BLOCK_SIZE_MASK (0x800000U)
#define | PXP_CTRL_BLOCK_SIZE_SHIFT (23U)
#define | PXP_CTRL_BLOCK_SIZE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_BLOCK_SIZE_SHIFT)) & PXP_CTRL_BLOCK_SIZE_MASK)
#define | PXP_CTRL_RSVD3_MASK (0xF000000U)
#define | PXP_CTRL_RSVD3_SHIFT (24U)
#define | PXP_CTRL_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD3_SHIFT)) & PXP_CTRL_RSVD3_MASK)
#define | PXP_CTRL_EN_REPEAT_MASK (0x10000000U)
#define | PXP_CTRL_EN_REPEAT_SHIFT (28U)
#define | PXP_CTRL_EN_REPEAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_EN_REPEAT_SHIFT)) & PXP_CTRL_EN_REPEAT_MASK)
#define | PXP_CTRL_RSVD4_MASK (0x20000000U)
#define | PXP_CTRL_RSVD4_SHIFT (29U)
#define | PXP_CTRL_RSVD4(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD4_SHIFT)) & PXP_CTRL_RSVD4_MASK)
#define | PXP_CTRL_CLKGATE_MASK (0x40000000U)
#define | PXP_CTRL_CLKGATE_SHIFT (30U)
#define | PXP_CTRL_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLKGATE_SHIFT)) & PXP_CTRL_CLKGATE_MASK)
#define | PXP_CTRL_SFTRST_MASK (0x80000000U)
#define | PXP_CTRL_SFTRST_SHIFT (31U)
#define | PXP_CTRL_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SFTRST_SHIFT)) & PXP_CTRL_SFTRST_MASK)

## CTRL_SET - Control Register 0

#define | PXP_CTRL_SET_ENABLE_MASK (0x1U)
#define | PXP_CTRL_SET_ENABLE_SHIFT (0U)
#define | PXP_CTRL_SET_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ENABLE_SHIFT)) & PXP_CTRL_SET_ENABLE_MASK)
#define | PXP_CTRL_SET_IRQ_ENABLE_MASK (0x2U)
#define | PXP_CTRL_SET_IRQ_ENABLE_SHIFT (1U)
#define | PXP_CTRL_SET_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_IRQ_ENABLE_SHIFT)) & PXP_CTRL_SET_IRQ_ENABLE_MASK)
#define | PXP_CTRL_SET_NEXT_IRQ_ENABLE_MASK (0x4U)
#define | PXP_CTRL_SET_NEXT_IRQ_ENABLE_SHIFT (2U)
#define | PXP_CTRL_SET_NEXT_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_SET_NEXT_IRQ_ENABLE_MASK)
#define | PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_MASK (0x10U)
#define | PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_SHIFT (4U)
#define | PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_MASK)
#define | PXP_CTRL_SET_RSVD0_MASK (0xE0U)
#define | PXP_CTRL_SET_RSVD0_SHIFT (5U)
#define | PXP_CTRL_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD0_SHIFT)) & PXP_CTRL_SET_RSVD0_MASK)
#define | PXP_CTRL_SET_ROTATE_MASK (0x300U)
#define | PXP_CTRL_SET_ROTATE_SHIFT (8U)
#define | PXP_CTRL_SET_ROTATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ROTATE_SHIFT)) & PXP_CTRL_SET_ROTATE_MASK)
#define | PXP_CTRL_SET_HFLIP_MASK (0x400U)
#define | PXP_CTRL_SET_HFLIP_SHIFT (10U)
#define | PXP_CTRL_SET_HFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_HFLIP_SHIFT)) & PXP_CTRL_SET_HFLIP_MASK)
#define | PXP_CTRL_SET_VFLIP_MASK (0x800U)
#define | PXP_CTRL_SET_VFLIP_SHIFT (11U)
#define | PXP_CTRL_SET_VFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_VFLIP_SHIFT)) & PXP_CTRL_SET_VFLIP_MASK)
#define | PXP_CTRL_SET_RSVD1_MASK (0x3FF000U)
#define | PXP_CTRL_SET_RSVD1_SHIFT (12U)
#define | PXP_CTRL_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD1_SHIFT)) & PXP_CTRL_SET_RSVD1_MASK)
#define | PXP_CTRL_SET_ROT_POS_MASK (0x400000U)
#define | PXP_CTRL_SET_ROT_POS_SHIFT (22U)
#define | PXP_CTRL_SET_ROT_POS(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ROT_POS_SHIFT)) & PXP_CTRL_SET_ROT_POS_MASK)
#define | PXP_CTRL_SET_BLOCK_SIZE_MASK (0x800000U)
#define | PXP_CTRL_SET_BLOCK_SIZE_SHIFT (23U)
#define | PXP_CTRL_SET_BLOCK_SIZE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_BLOCK_SIZE_SHIFT)) & PXP_CTRL_SET_BLOCK_SIZE_MASK)
#define | PXP_CTRL_SET_RSVD3_MASK (0xF000000U)
#define | PXP_CTRL_SET_RSVD3_SHIFT (24U)
#define | PXP_CTRL_SET_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD3_SHIFT)) & PXP_CTRL_SET_RSVD3_MASK)
#define | PXP_CTRL_SET_EN_REPEAT_MASK (0x10000000U)
#define | PXP_CTRL_SET_EN_REPEAT_SHIFT (28U)
#define | PXP_CTRL_SET_EN_REPEAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_EN_REPEAT_SHIFT)) & PXP_CTRL_SET_EN_REPEAT_MASK)
#define | PXP_CTRL_SET_RSVD4_MASK (0x20000000U)
#define | PXP_CTRL_SET_RSVD4_SHIFT (29U)
#define | PXP_CTRL_SET_RSVD4(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD4_SHIFT)) & PXP_CTRL_SET_RSVD4_MASK)
#define | PXP_CTRL_SET_CLKGATE_MASK (0x40000000U)
#define | PXP_CTRL_SET_CLKGATE_SHIFT (30U)
#define | PXP_CTRL_SET_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_CLKGATE_SHIFT)) & PXP_CTRL_SET_CLKGATE_MASK)
#define | PXP_CTRL_SET_SFTRST_MASK (0x80000000U)
#define | PXP_CTRL_SET_SFTRST_SHIFT (31U)
#define | PXP_CTRL_SET_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_SFTRST_SHIFT)) & PXP_CTRL_SET_SFTRST_MASK)

## CTRL_CLR - Control Register 0

#define | PXP_CTRL_CLR_ENABLE_MASK (0x1U)
#define | PXP_CTRL_CLR_ENABLE_SHIFT (0U)
#define | PXP_CTRL_CLR_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ENABLE_SHIFT)) & PXP_CTRL_CLR_ENABLE_MASK)
#define | PXP_CTRL_CLR_IRQ_ENABLE_MASK (0x2U)
#define | PXP_CTRL_CLR_IRQ_ENABLE_SHIFT (1U)
#define | PXP_CTRL_CLR_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_IRQ_ENABLE_SHIFT)) & PXP_CTRL_CLR_IRQ_ENABLE_MASK)
#define | PXP_CTRL_CLR_NEXT_IRQ_ENABLE_MASK (0x4U)
#define | PXP_CTRL_CLR_NEXT_IRQ_ENABLE_SHIFT (2U)
#define | PXP_CTRL_CLR_NEXT_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_CLR_NEXT_IRQ_ENABLE_MASK)
#define | PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_MASK (0x10U)
#define | PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_SHIFT (4U)
#define | PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_MASK)
#define | PXP_CTRL_CLR_RSVD0_MASK (0xE0U)
#define | PXP_CTRL_CLR_RSVD0_SHIFT (5U)
#define | PXP_CTRL_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD0_SHIFT)) & PXP_CTRL_CLR_RSVD0_MASK)
#define | PXP_CTRL_CLR_ROTATE_MASK (0x300U)
#define | PXP_CTRL_CLR_ROTATE_SHIFT (8U)
#define | PXP_CTRL_CLR_ROTATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ROTATE_SHIFT)) & PXP_CTRL_CLR_ROTATE_MASK)
#define | PXP_CTRL_CLR_HFLIP_MASK (0x400U)
#define | PXP_CTRL_CLR_HFLIP_SHIFT (10U)
#define | PXP_CTRL_CLR_HFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_HFLIP_SHIFT)) & PXP_CTRL_CLR_HFLIP_MASK)
#define | PXP_CTRL_CLR_VFLIP_MASK (0x800U)
#define | PXP_CTRL_CLR_VFLIP_SHIFT (11U)
#define | PXP_CTRL_CLR_VFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_VFLIP_SHIFT)) & PXP_CTRL_CLR_VFLIP_MASK)
#define | PXP_CTRL_CLR_RSVD1_MASK (0x3FF000U)
#define | PXP_CTRL_CLR_RSVD1_SHIFT (12U)
#define | PXP_CTRL_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD1_SHIFT)) & PXP_CTRL_CLR_RSVD1_MASK)
#define | PXP_CTRL_CLR_ROT_POS_MASK (0x400000U)
#define | PXP_CTRL_CLR_ROT_POS_SHIFT (22U)
#define | PXP_CTRL_CLR_ROT_POS(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ROT_POS_SHIFT)) & PXP_CTRL_CLR_ROT_POS_MASK)
#define | PXP_CTRL_CLR_BLOCK_SIZE_MASK (0x800000U)
#define | PXP_CTRL_CLR_BLOCK_SIZE_SHIFT (23U)
#define | PXP_CTRL_CLR_BLOCK_SIZE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_BLOCK_SIZE_SHIFT)) & PXP_CTRL_CLR_BLOCK_SIZE_MASK)
#define | PXP_CTRL_CLR_RSVD3_MASK (0xF000000U)
#define | PXP_CTRL_CLR_RSVD3_SHIFT (24U)
#define | PXP_CTRL_CLR_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD3_SHIFT)) & PXP_CTRL_CLR_RSVD3_MASK)
#define | PXP_CTRL_CLR_EN_REPEAT_MASK (0x10000000U)
#define | PXP_CTRL_CLR_EN_REPEAT_SHIFT (28U)
#define | PXP_CTRL_CLR_EN_REPEAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_EN_REPEAT_SHIFT)) & PXP_CTRL_CLR_EN_REPEAT_MASK)
#define | PXP_CTRL_CLR_RSVD4_MASK (0x20000000U)
#define | PXP_CTRL_CLR_RSVD4_SHIFT (29U)
#define | PXP_CTRL_CLR_RSVD4(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD4_SHIFT)) & PXP_CTRL_CLR_RSVD4_MASK)
#define | PXP_CTRL_CLR_CLKGATE_MASK (0x40000000U)
#define | PXP_CTRL_CLR_CLKGATE_SHIFT (30U)
#define | PXP_CTRL_CLR_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_CLKGATE_SHIFT)) & PXP_CTRL_CLR_CLKGATE_MASK)
#define | PXP_CTRL_CLR_SFTRST_MASK (0x80000000U)
#define | PXP_CTRL_CLR_SFTRST_SHIFT (31U)
#define | PXP_CTRL_CLR_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_SFTRST_SHIFT)) & PXP_CTRL_CLR_SFTRST_MASK)

## CTRL_TOG - Control Register 0

#define | PXP_CTRL_TOG_ENABLE_MASK (0x1U)
#define | PXP_CTRL_TOG_ENABLE_SHIFT (0U)
#define | PXP_CTRL_TOG_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ENABLE_SHIFT)) & PXP_CTRL_TOG_ENABLE_MASK)
#define | PXP_CTRL_TOG_IRQ_ENABLE_MASK (0x2U)
#define | PXP_CTRL_TOG_IRQ_ENABLE_SHIFT (1U)
#define | PXP_CTRL_TOG_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_IRQ_ENABLE_SHIFT)) & PXP_CTRL_TOG_IRQ_ENABLE_MASK)
#define | PXP_CTRL_TOG_NEXT_IRQ_ENABLE_MASK (0x4U)
#define | PXP_CTRL_TOG_NEXT_IRQ_ENABLE_SHIFT (2U)
#define | PXP_CTRL_TOG_NEXT_IRQ_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_TOG_NEXT_IRQ_ENABLE_MASK)
#define | PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_MASK (0x10U)
#define | PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_SHIFT (4U)
#define | PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_MASK)
#define | PXP_CTRL_TOG_RSVD0_MASK (0xE0U)
#define | PXP_CTRL_TOG_RSVD0_SHIFT (5U)
#define | PXP_CTRL_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD0_SHIFT)) & PXP_CTRL_TOG_RSVD0_MASK)
#define | PXP_CTRL_TOG_ROTATE_MASK (0x300U)
#define | PXP_CTRL_TOG_ROTATE_SHIFT (8U)
#define | PXP_CTRL_TOG_ROTATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ROTATE_SHIFT)) & PXP_CTRL_TOG_ROTATE_MASK)
#define | PXP_CTRL_TOG_HFLIP_MASK (0x400U)
#define | PXP_CTRL_TOG_HFLIP_SHIFT (10U)
#define | PXP_CTRL_TOG_HFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_HFLIP_SHIFT)) & PXP_CTRL_TOG_HFLIP_MASK)
#define | PXP_CTRL_TOG_VFLIP_MASK (0x800U)
#define | PXP_CTRL_TOG_VFLIP_SHIFT (11U)
#define | PXP_CTRL_TOG_VFLIP(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_VFLIP_SHIFT)) & PXP_CTRL_TOG_VFLIP_MASK)
#define | PXP_CTRL_TOG_RSVD1_MASK (0x3FF000U)
#define | PXP_CTRL_TOG_RSVD1_SHIFT (12U)
#define | PXP_CTRL_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD1_SHIFT)) & PXP_CTRL_TOG_RSVD1_MASK)
#define | PXP_CTRL_TOG_ROT_POS_MASK (0x400000U)
#define | PXP_CTRL_TOG_ROT_POS_SHIFT (22U)
#define | PXP_CTRL_TOG_ROT_POS(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ROT_POS_SHIFT)) & PXP_CTRL_TOG_ROT_POS_MASK)
#define | PXP_CTRL_TOG_BLOCK_SIZE_MASK (0x800000U)
#define | PXP_CTRL_TOG_BLOCK_SIZE_SHIFT (23U)
#define | PXP_CTRL_TOG_BLOCK_SIZE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_BLOCK_SIZE_SHIFT)) & PXP_CTRL_TOG_BLOCK_SIZE_MASK)
#define | PXP_CTRL_TOG_RSVD3_MASK (0xF000000U)
#define | PXP_CTRL_TOG_RSVD3_SHIFT (24U)
#define | PXP_CTRL_TOG_RSVD3(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD3_SHIFT)) & PXP_CTRL_TOG_RSVD3_MASK)
#define | PXP_CTRL_TOG_EN_REPEAT_MASK (0x10000000U)
#define | PXP_CTRL_TOG_EN_REPEAT_SHIFT (28U)
#define | PXP_CTRL_TOG_EN_REPEAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_EN_REPEAT_SHIFT)) & PXP_CTRL_TOG_EN_REPEAT_MASK)
#define | PXP_CTRL_TOG_RSVD4_MASK (0x20000000U)
#define | PXP_CTRL_TOG_RSVD4_SHIFT (29U)
#define | PXP_CTRL_TOG_RSVD4(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD4_SHIFT)) & PXP_CTRL_TOG_RSVD4_MASK)
#define | PXP_CTRL_TOG_CLKGATE_MASK (0x40000000U)
#define | PXP_CTRL_TOG_CLKGATE_SHIFT (30U)
#define | PXP_CTRL_TOG_CLKGATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_CLKGATE_SHIFT)) & PXP_CTRL_TOG_CLKGATE_MASK)
#define | PXP_CTRL_TOG_SFTRST_MASK (0x80000000U)
#define | PXP_CTRL_TOG_SFTRST_SHIFT (31U)
#define | PXP_CTRL_TOG_SFTRST(x) (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_SFTRST_SHIFT)) & PXP_CTRL_TOG_SFTRST_MASK)

## STAT - Status Register

#define | PXP_STAT_IRQ_MASK (0x1U)
#define | PXP_STAT_IRQ_SHIFT (0U)
#define | PXP_STAT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_IRQ_SHIFT)) & PXP_STAT_IRQ_MASK)
#define | PXP_STAT_AXI_WRITE_ERROR_MASK (0x2U)
#define | PXP_STAT_AXI_WRITE_ERROR_SHIFT (1U)
#define | PXP_STAT_AXI_WRITE_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_AXI_WRITE_ERROR_MASK)
#define | PXP_STAT_AXI_READ_ERROR_MASK (0x4U)
#define | PXP_STAT_AXI_READ_ERROR_SHIFT (2U)
#define | PXP_STAT_AXI_READ_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_AXI_READ_ERROR_SHIFT)) & PXP_STAT_AXI_READ_ERROR_MASK)
#define | PXP_STAT_NEXT_IRQ_MASK (0x8U)
#define | PXP_STAT_NEXT_IRQ_SHIFT (3U)
#define | PXP_STAT_NEXT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_NEXT_IRQ_SHIFT)) & PXP_STAT_NEXT_IRQ_MASK)
#define | PXP_STAT_AXI_ERROR_ID_MASK (0xF0U)
#define | PXP_STAT_AXI_ERROR_ID_SHIFT (4U)
#define | PXP_STAT_AXI_ERROR_ID(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_AXI_ERROR_ID_SHIFT)) & PXP_STAT_AXI_ERROR_ID_MASK)
#define | PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)
#define | PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)
#define | PXP_STAT_LUT_DMA_LOAD_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_MASK)
#define | PXP_STAT_RSVD2_MASK (0xFE00U)
#define | PXP_STAT_RSVD2_SHIFT (9U)
#define | PXP_STAT_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_RSVD2_SHIFT)) & PXP_STAT_RSVD2_MASK)
#define | PXP_STAT_BLOCKY_MASK (0xFF0000U)
#define | PXP_STAT_BLOCKY_SHIFT (16U)
#define | PXP_STAT_BLOCKY(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_BLOCKY_SHIFT)) & PXP_STAT_BLOCKY_MASK)
#define | PXP_STAT_BLOCKX_MASK (0xFF000000U)
#define | PXP_STAT_BLOCKX_SHIFT (24U)
#define | PXP_STAT_BLOCKX(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_BLOCKX_SHIFT)) & PXP_STAT_BLOCKX_MASK)

## STAT_SET - Status Register

#define | PXP_STAT_SET_IRQ_MASK (0x1U)
#define | PXP_STAT_SET_IRQ_SHIFT (0U)
#define | PXP_STAT_SET_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_IRQ_SHIFT)) & PXP_STAT_SET_IRQ_MASK)
#define | PXP_STAT_SET_AXI_WRITE_ERROR_MASK (0x2U)
#define | PXP_STAT_SET_AXI_WRITE_ERROR_SHIFT (1U)
#define | PXP_STAT_SET_AXI_WRITE_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_SET_AXI_WRITE_ERROR_MASK)
#define | PXP_STAT_SET_AXI_READ_ERROR_MASK (0x4U)
#define | PXP_STAT_SET_AXI_READ_ERROR_SHIFT (2U)
#define | PXP_STAT_SET_AXI_READ_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_AXI_READ_ERROR_SHIFT)) & PXP_STAT_SET_AXI_READ_ERROR_MASK)
#define | PXP_STAT_SET_NEXT_IRQ_MASK (0x8U)
#define | PXP_STAT_SET_NEXT_IRQ_SHIFT (3U)
#define | PXP_STAT_SET_NEXT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_NEXT_IRQ_SHIFT)) & PXP_STAT_SET_NEXT_IRQ_MASK)
#define | PXP_STAT_SET_AXI_ERROR_ID_MASK (0xF0U)
#define | PXP_STAT_SET_AXI_ERROR_ID_SHIFT (4U)
#define | PXP_STAT_SET_AXI_ERROR_ID(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_AXI_ERROR_ID_SHIFT)) & PXP_STAT_SET_AXI_ERROR_ID_MASK)
#define | PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)
#define | PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)
#define | PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_MASK)
#define | PXP_STAT_SET_RSVD2_MASK (0xFE00U)
#define | PXP_STAT_SET_RSVD2_SHIFT (9U)
#define | PXP_STAT_SET_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_RSVD2_SHIFT)) & PXP_STAT_SET_RSVD2_MASK)
#define | PXP_STAT_SET_BLOCKY_MASK (0xFF0000U)
#define | PXP_STAT_SET_BLOCKY_SHIFT (16U)
#define | PXP_STAT_SET_BLOCKY(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_BLOCKY_SHIFT)) & PXP_STAT_SET_BLOCKY_MASK)
#define | PXP_STAT_SET_BLOCKX_MASK (0xFF000000U)
#define | PXP_STAT_SET_BLOCKX_SHIFT (24U)
#define | PXP_STAT_SET_BLOCKX(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_BLOCKX_SHIFT)) & PXP_STAT_SET_BLOCKX_MASK)

## STAT_CLR - Status Register

#define | PXP_STAT_CLR_IRQ_MASK (0x1U)
#define | PXP_STAT_CLR_IRQ_SHIFT (0U)
#define | PXP_STAT_CLR_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_IRQ_SHIFT)) & PXP_STAT_CLR_IRQ_MASK)
#define | PXP_STAT_CLR_AXI_WRITE_ERROR_MASK (0x2U)
#define | PXP_STAT_CLR_AXI_WRITE_ERROR_SHIFT (1U)
#define | PXP_STAT_CLR_AXI_WRITE_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_CLR_AXI_WRITE_ERROR_MASK)
#define | PXP_STAT_CLR_AXI_READ_ERROR_MASK (0x4U)
#define | PXP_STAT_CLR_AXI_READ_ERROR_SHIFT (2U)
#define | PXP_STAT_CLR_AXI_READ_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_AXI_READ_ERROR_SHIFT)) & PXP_STAT_CLR_AXI_READ_ERROR_MASK)
#define | PXP_STAT_CLR_NEXT_IRQ_MASK (0x8U)
#define | PXP_STAT_CLR_NEXT_IRQ_SHIFT (3U)
#define | PXP_STAT_CLR_NEXT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_NEXT_IRQ_SHIFT)) & PXP_STAT_CLR_NEXT_IRQ_MASK)
#define | PXP_STAT_CLR_AXI_ERROR_ID_MASK (0xF0U)
#define | PXP_STAT_CLR_AXI_ERROR_ID_SHIFT (4U)
#define | PXP_STAT_CLR_AXI_ERROR_ID(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_AXI_ERROR_ID_SHIFT)) & PXP_STAT_CLR_AXI_ERROR_ID_MASK)
#define | PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)
#define | PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)
#define | PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_MASK)
#define | PXP_STAT_CLR_RSVD2_MASK (0xFE00U)
#define | PXP_STAT_CLR_RSVD2_SHIFT (9U)
#define | PXP_STAT_CLR_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_RSVD2_SHIFT)) & PXP_STAT_CLR_RSVD2_MASK)
#define | PXP_STAT_CLR_BLOCKY_MASK (0xFF0000U)
#define | PXP_STAT_CLR_BLOCKY_SHIFT (16U)
#define | PXP_STAT_CLR_BLOCKY(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_BLOCKY_SHIFT)) & PXP_STAT_CLR_BLOCKY_MASK)
#define | PXP_STAT_CLR_BLOCKX_MASK (0xFF000000U)
#define | PXP_STAT_CLR_BLOCKX_SHIFT (24U)
#define | PXP_STAT_CLR_BLOCKX(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_BLOCKX_SHIFT)) & PXP_STAT_CLR_BLOCKX_MASK)

## STAT_TOG - Status Register

#define | PXP_STAT_TOG_IRQ_MASK (0x1U)
#define | PXP_STAT_TOG_IRQ_SHIFT (0U)
#define | PXP_STAT_TOG_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_IRQ_SHIFT)) & PXP_STAT_TOG_IRQ_MASK)
#define | PXP_STAT_TOG_AXI_WRITE_ERROR_MASK (0x2U)
#define | PXP_STAT_TOG_AXI_WRITE_ERROR_SHIFT (1U)
#define | PXP_STAT_TOG_AXI_WRITE_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_TOG_AXI_WRITE_ERROR_MASK)
#define | PXP_STAT_TOG_AXI_READ_ERROR_MASK (0x4U)
#define | PXP_STAT_TOG_AXI_READ_ERROR_SHIFT (2U)
#define | PXP_STAT_TOG_AXI_READ_ERROR(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_AXI_READ_ERROR_SHIFT)) & PXP_STAT_TOG_AXI_READ_ERROR_MASK)
#define | PXP_STAT_TOG_NEXT_IRQ_MASK (0x8U)
#define | PXP_STAT_TOG_NEXT_IRQ_SHIFT (3U)
#define | PXP_STAT_TOG_NEXT_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_NEXT_IRQ_SHIFT)) & PXP_STAT_TOG_NEXT_IRQ_MASK)
#define | PXP_STAT_TOG_AXI_ERROR_ID_MASK (0xF0U)
#define | PXP_STAT_TOG_AXI_ERROR_ID_SHIFT (4U)
#define | PXP_STAT_TOG_AXI_ERROR_ID(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_AXI_ERROR_ID_SHIFT)) & PXP_STAT_TOG_AXI_ERROR_ID_MASK)
#define | PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)
#define | PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)
#define | PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_MASK)
#define | PXP_STAT_TOG_RSVD2_MASK (0xFE00U)
#define | PXP_STAT_TOG_RSVD2_SHIFT (9U)
#define | PXP_STAT_TOG_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_RSVD2_SHIFT)) & PXP_STAT_TOG_RSVD2_MASK)
#define | PXP_STAT_TOG_BLOCKY_MASK (0xFF0000U)
#define | PXP_STAT_TOG_BLOCKY_SHIFT (16U)
#define | PXP_STAT_TOG_BLOCKY(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_BLOCKY_SHIFT)) & PXP_STAT_TOG_BLOCKY_MASK)
#define | PXP_STAT_TOG_BLOCKX_MASK (0xFF000000U)
#define | PXP_STAT_TOG_BLOCKX_SHIFT (24U)
#define | PXP_STAT_TOG_BLOCKX(x) (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_BLOCKX_SHIFT)) & PXP_STAT_TOG_BLOCKX_MASK)

## OUT_CTRL - Output Buffer Control Register

#define | PXP_OUT_CTRL_FORMAT_MASK (0x1FU)
#define | PXP_OUT_CTRL_FORMAT_SHIFT (0U)
#define | PXP_OUT_CTRL_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_FORMAT_SHIFT)) & PXP_OUT_CTRL_FORMAT_MASK)
#define | PXP_OUT_CTRL_RSVD0_MASK (0xE0U)
#define | PXP_OUT_CTRL_RSVD0_SHIFT (5U)
#define | PXP_OUT_CTRL_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_RSVD0_SHIFT)) & PXP_OUT_CTRL_RSVD0_MASK)
#define | PXP_OUT_CTRL_INTERLACED_OUTPUT_MASK (0x300U)
#define | PXP_OUT_CTRL_INTERLACED_OUTPUT_SHIFT (8U)
#define | PXP_OUT_CTRL_INTERLACED_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_INTERLACED_OUTPUT_MASK)
#define | PXP_OUT_CTRL_RSVD1_MASK (0x7FFC00U)
#define | PXP_OUT_CTRL_RSVD1_SHIFT (10U)
#define | PXP_OUT_CTRL_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_RSVD1_SHIFT)) & PXP_OUT_CTRL_RSVD1_MASK)
#define | PXP_OUT_CTRL_ALPHA_OUTPUT_MASK (0x800000U)
#define | PXP_OUT_CTRL_ALPHA_OUTPUT_SHIFT (23U)
#define | PXP_OUT_CTRL_ALPHA_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_ALPHA_OUTPUT_MASK)
#define | PXP_OUT_CTRL_ALPHA_MASK (0xFF000000U)
#define | PXP_OUT_CTRL_ALPHA_SHIFT (24U)
#define | PXP_OUT_CTRL_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_ALPHA_SHIFT)) & PXP_OUT_CTRL_ALPHA_MASK)

## OUT_CTRL_SET - Output Buffer Control Register

#define | PXP_OUT_CTRL_SET_FORMAT_MASK (0x1FU)
#define | PXP_OUT_CTRL_SET_FORMAT_SHIFT (0U)
#define | PXP_OUT_CTRL_SET_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_FORMAT_SHIFT)) & PXP_OUT_CTRL_SET_FORMAT_MASK)
#define | PXP_OUT_CTRL_SET_RSVD0_MASK (0xE0U)
#define | PXP_OUT_CTRL_SET_RSVD0_SHIFT (5U)
#define | PXP_OUT_CTRL_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_RSVD0_SHIFT)) & PXP_OUT_CTRL_SET_RSVD0_MASK)
#define | PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_MASK (0x300U)
#define | PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_SHIFT (8U)
#define | PXP_OUT_CTRL_SET_INTERLACED_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_MASK)
#define | PXP_OUT_CTRL_SET_RSVD1_MASK (0x7FFC00U)
#define | PXP_OUT_CTRL_SET_RSVD1_SHIFT (10U)
#define | PXP_OUT_CTRL_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_RSVD1_SHIFT)) & PXP_OUT_CTRL_SET_RSVD1_MASK)
#define | PXP_OUT_CTRL_SET_ALPHA_OUTPUT_MASK (0x800000U)
#define | PXP_OUT_CTRL_SET_ALPHA_OUTPUT_SHIFT (23U)
#define | PXP_OUT_CTRL_SET_ALPHA_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_SET_ALPHA_OUTPUT_MASK)
#define | PXP_OUT_CTRL_SET_ALPHA_MASK (0xFF000000U)
#define | PXP_OUT_CTRL_SET_ALPHA_SHIFT (24U)
#define | PXP_OUT_CTRL_SET_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_ALPHA_SHIFT)) & PXP_OUT_CTRL_SET_ALPHA_MASK)

## OUT_CTRL_CLR - Output Buffer Control Register

#define | PXP_OUT_CTRL_CLR_FORMAT_MASK (0x1FU)
#define | PXP_OUT_CTRL_CLR_FORMAT_SHIFT (0U)
#define | PXP_OUT_CTRL_CLR_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_FORMAT_SHIFT)) & PXP_OUT_CTRL_CLR_FORMAT_MASK)
#define | PXP_OUT_CTRL_CLR_RSVD0_MASK (0xE0U)
#define | PXP_OUT_CTRL_CLR_RSVD0_SHIFT (5U)
#define | PXP_OUT_CTRL_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_RSVD0_SHIFT)) & PXP_OUT_CTRL_CLR_RSVD0_MASK)
#define | PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_MASK (0x300U)
#define | PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_SHIFT (8U)
#define | PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_MASK)
#define | PXP_OUT_CTRL_CLR_RSVD1_MASK (0x7FFC00U)
#define | PXP_OUT_CTRL_CLR_RSVD1_SHIFT (10U)
#define | PXP_OUT_CTRL_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_RSVD1_SHIFT)) & PXP_OUT_CTRL_CLR_RSVD1_MASK)
#define | PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_MASK (0x800000U)
#define | PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_SHIFT (23U)
#define | PXP_OUT_CTRL_CLR_ALPHA_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_MASK)
#define | PXP_OUT_CTRL_CLR_ALPHA_MASK (0xFF000000U)
#define | PXP_OUT_CTRL_CLR_ALPHA_SHIFT (24U)
#define | PXP_OUT_CTRL_CLR_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_ALPHA_SHIFT)) & PXP_OUT_CTRL_CLR_ALPHA_MASK)

## OUT_CTRL_TOG - Output Buffer Control Register

#define | PXP_OUT_CTRL_TOG_FORMAT_MASK (0x1FU)
#define | PXP_OUT_CTRL_TOG_FORMAT_SHIFT (0U)
#define | PXP_OUT_CTRL_TOG_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_FORMAT_SHIFT)) & PXP_OUT_CTRL_TOG_FORMAT_MASK)
#define | PXP_OUT_CTRL_TOG_RSVD0_MASK (0xE0U)
#define | PXP_OUT_CTRL_TOG_RSVD0_SHIFT (5U)
#define | PXP_OUT_CTRL_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_RSVD0_SHIFT)) & PXP_OUT_CTRL_TOG_RSVD0_MASK)
#define | PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_MASK (0x300U)
#define | PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_SHIFT (8U)
#define | PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_MASK)
#define | PXP_OUT_CTRL_TOG_RSVD1_MASK (0x7FFC00U)
#define | PXP_OUT_CTRL_TOG_RSVD1_SHIFT (10U)
#define | PXP_OUT_CTRL_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_RSVD1_SHIFT)) & PXP_OUT_CTRL_TOG_RSVD1_MASK)
#define | PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_MASK (0x800000U)
#define | PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_SHIFT (23U)
#define | PXP_OUT_CTRL_TOG_ALPHA_OUTPUT(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_MASK)
#define | PXP_OUT_CTRL_TOG_ALPHA_MASK (0xFF000000U)
#define | PXP_OUT_CTRL_TOG_ALPHA_SHIFT (24U)
#define | PXP_OUT_CTRL_TOG_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_ALPHA_SHIFT)) & PXP_OUT_CTRL_TOG_ALPHA_MASK)

## OUT_BUF - Output Frame Buffer Pointer

#define | PXP_OUT_BUF_ADDR_MASK (0xFFFFFFFFU)
#define | PXP_OUT_BUF_ADDR_SHIFT (0U)
#define | PXP_OUT_BUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_BUF_ADDR_SHIFT)) & PXP_OUT_BUF_ADDR_MASK)

## OUT_BUF2 - Output Frame Buffer Pointer #2

#define | PXP_OUT_BUF2_ADDR_MASK (0xFFFFFFFFU)
#define | PXP_OUT_BUF2_ADDR_SHIFT (0U)
#define | PXP_OUT_BUF2_ADDR(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_BUF2_ADDR_SHIFT)) & PXP_OUT_BUF2_ADDR_MASK)

## OUT_PITCH - Output Buffer Pitch

#define | PXP_OUT_PITCH_PITCH_MASK (0xFFFFU)
#define | PXP_OUT_PITCH_PITCH_SHIFT (0U)
#define | PXP_OUT_PITCH_PITCH(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PITCH_PITCH_SHIFT)) & PXP_OUT_PITCH_PITCH_MASK)
#define | PXP_OUT_PITCH_RSVD_MASK (0xFFFF0000U)
#define | PXP_OUT_PITCH_RSVD_SHIFT (16U)
#define | PXP_OUT_PITCH_RSVD(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PITCH_RSVD_SHIFT)) & PXP_OUT_PITCH_RSVD_MASK)

## OUT_LRC - Output Surface Lower Right Coordinate

#define | PXP_OUT_LRC_Y_MASK (0x3FFFU)
#define | PXP_OUT_LRC_Y_SHIFT (0U)
#define | PXP_OUT_LRC_Y(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_Y_SHIFT)) & PXP_OUT_LRC_Y_MASK)
#define | PXP_OUT_LRC_RSVD0_MASK (0xC000U)
#define | PXP_OUT_LRC_RSVD0_SHIFT (14U)
#define | PXP_OUT_LRC_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_RSVD0_SHIFT)) & PXP_OUT_LRC_RSVD0_MASK)
#define | PXP_OUT_LRC_X_MASK (0x3FFF0000U)
#define | PXP_OUT_LRC_X_SHIFT (16U)
#define | PXP_OUT_LRC_X(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_X_SHIFT)) & PXP_OUT_LRC_X_MASK)
#define | PXP_OUT_LRC_RSVD1_MASK (0xC0000000U)
#define | PXP_OUT_LRC_RSVD1_SHIFT (30U)
#define | PXP_OUT_LRC_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_RSVD1_SHIFT)) & PXP_OUT_LRC_RSVD1_MASK)

## OUT_PS_ULC - Processed Surface Upper Left Coordinate

#define | PXP_OUT_PS_ULC_Y_MASK (0x3FFFU)
#define | PXP_OUT_PS_ULC_Y_SHIFT (0U)
#define | PXP_OUT_PS_ULC_Y(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_Y_SHIFT)) & PXP_OUT_PS_ULC_Y_MASK)
#define | PXP_OUT_PS_ULC_RSVD0_MASK (0xC000U)
#define | PXP_OUT_PS_ULC_RSVD0_SHIFT (14U)
#define | PXP_OUT_PS_ULC_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_RSVD0_SHIFT)) & PXP_OUT_PS_ULC_RSVD0_MASK)
#define | PXP_OUT_PS_ULC_X_MASK (0x3FFF0000U)
#define | PXP_OUT_PS_ULC_X_SHIFT (16U)
#define | PXP_OUT_PS_ULC_X(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_X_SHIFT)) & PXP_OUT_PS_ULC_X_MASK)
#define | PXP_OUT_PS_ULC_RSVD1_MASK (0xC0000000U)
#define | PXP_OUT_PS_ULC_RSVD1_SHIFT (30U)
#define | PXP_OUT_PS_ULC_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_RSVD1_SHIFT)) & PXP_OUT_PS_ULC_RSVD1_MASK)

## OUT_PS_LRC - Processed Surface Lower Right Coordinate

#define | PXP_OUT_PS_LRC_Y_MASK (0x3FFFU)
#define | PXP_OUT_PS_LRC_Y_SHIFT (0U)
#define | PXP_OUT_PS_LRC_Y(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_Y_SHIFT)) & PXP_OUT_PS_LRC_Y_MASK)
#define | PXP_OUT_PS_LRC_RSVD0_MASK (0xC000U)
#define | PXP_OUT_PS_LRC_RSVD0_SHIFT (14U)
#define | PXP_OUT_PS_LRC_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_RSVD0_SHIFT)) & PXP_OUT_PS_LRC_RSVD0_MASK)
#define | PXP_OUT_PS_LRC_X_MASK (0x3FFF0000U)
#define | PXP_OUT_PS_LRC_X_SHIFT (16U)
#define | PXP_OUT_PS_LRC_X(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_X_SHIFT)) & PXP_OUT_PS_LRC_X_MASK)
#define | PXP_OUT_PS_LRC_RSVD1_MASK (0xC0000000U)
#define | PXP_OUT_PS_LRC_RSVD1_SHIFT (30U)
#define | PXP_OUT_PS_LRC_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_RSVD1_SHIFT)) & PXP_OUT_PS_LRC_RSVD1_MASK)

## OUT_AS_ULC - Alpha Surface Upper Left Coordinate

#define | PXP_OUT_AS_ULC_Y_MASK (0x3FFFU)
#define | PXP_OUT_AS_ULC_Y_SHIFT (0U)
#define | PXP_OUT_AS_ULC_Y(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_Y_SHIFT)) & PXP_OUT_AS_ULC_Y_MASK)
#define | PXP_OUT_AS_ULC_RSVD0_MASK (0xC000U)
#define | PXP_OUT_AS_ULC_RSVD0_SHIFT (14U)
#define | PXP_OUT_AS_ULC_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_RSVD0_SHIFT)) & PXP_OUT_AS_ULC_RSVD0_MASK)
#define | PXP_OUT_AS_ULC_X_MASK (0x3FFF0000U)
#define | PXP_OUT_AS_ULC_X_SHIFT (16U)
#define | PXP_OUT_AS_ULC_X(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_X_SHIFT)) & PXP_OUT_AS_ULC_X_MASK)
#define | PXP_OUT_AS_ULC_RSVD1_MASK (0xC0000000U)
#define | PXP_OUT_AS_ULC_RSVD1_SHIFT (30U)
#define | PXP_OUT_AS_ULC_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_RSVD1_SHIFT)) & PXP_OUT_AS_ULC_RSVD1_MASK)

## OUT_AS_LRC - Alpha Surface Lower Right Coordinate

#define | PXP_OUT_AS_LRC_Y_MASK (0x3FFFU)
#define | PXP_OUT_AS_LRC_Y_SHIFT (0U)
#define | PXP_OUT_AS_LRC_Y(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_Y_SHIFT)) & PXP_OUT_AS_LRC_Y_MASK)
#define | PXP_OUT_AS_LRC_RSVD0_MASK (0xC000U)
#define | PXP_OUT_AS_LRC_RSVD0_SHIFT (14U)
#define | PXP_OUT_AS_LRC_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_RSVD0_SHIFT)) & PXP_OUT_AS_LRC_RSVD0_MASK)
#define | PXP_OUT_AS_LRC_X_MASK (0x3FFF0000U)
#define | PXP_OUT_AS_LRC_X_SHIFT (16U)
#define | PXP_OUT_AS_LRC_X(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_X_SHIFT)) & PXP_OUT_AS_LRC_X_MASK)
#define | PXP_OUT_AS_LRC_RSVD1_MASK (0xC0000000U)
#define | PXP_OUT_AS_LRC_RSVD1_SHIFT (30U)
#define | PXP_OUT_AS_LRC_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_RSVD1_SHIFT)) & PXP_OUT_AS_LRC_RSVD1_MASK)

## PS_CTRL - Processed Surface (PS) Control Register

#define | PXP_PS_CTRL_FORMAT_MASK (0x1FU)
#define | PXP_PS_CTRL_FORMAT_SHIFT (0U)
#define | PXP_PS_CTRL_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_FORMAT_SHIFT)) & PXP_PS_CTRL_FORMAT_MASK)
#define | PXP_PS_CTRL_WB_SWAP_MASK (0x20U)
#define | PXP_PS_CTRL_WB_SWAP_SHIFT (5U)
#define | PXP_PS_CTRL_WB_SWAP(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_WB_SWAP_SHIFT)) & PXP_PS_CTRL_WB_SWAP_MASK)
#define | PXP_PS_CTRL_RSVD0_MASK (0xC0U)
#define | PXP_PS_CTRL_RSVD0_SHIFT (6U)
#define | PXP_PS_CTRL_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_RSVD0_SHIFT)) & PXP_PS_CTRL_RSVD0_MASK)
#define | PXP_PS_CTRL_DECY_MASK (0x300U)
#define | PXP_PS_CTRL_DECY_SHIFT (8U)
#define | PXP_PS_CTRL_DECY(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_DECY_SHIFT)) & PXP_PS_CTRL_DECY_MASK)
#define | PXP_PS_CTRL_DECX_MASK (0xC00U)
#define | PXP_PS_CTRL_DECX_SHIFT (10U)
#define | PXP_PS_CTRL_DECX(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_DECX_SHIFT)) & PXP_PS_CTRL_DECX_MASK)
#define | PXP_PS_CTRL_RSVD1_MASK (0xFFFFF000U)
#define | PXP_PS_CTRL_RSVD1_SHIFT (12U)
#define | PXP_PS_CTRL_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_RSVD1_SHIFT)) & PXP_PS_CTRL_RSVD1_MASK)

## PS_CTRL_SET - Processed Surface (PS) Control Register

#define | PXP_PS_CTRL_SET_FORMAT_MASK (0x1FU)
#define | PXP_PS_CTRL_SET_FORMAT_SHIFT (0U)
#define | PXP_PS_CTRL_SET_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_FORMAT_SHIFT)) & PXP_PS_CTRL_SET_FORMAT_MASK)
#define | PXP_PS_CTRL_SET_WB_SWAP_MASK (0x20U)
#define | PXP_PS_CTRL_SET_WB_SWAP_SHIFT (5U)
#define | PXP_PS_CTRL_SET_WB_SWAP(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_WB_SWAP_SHIFT)) & PXP_PS_CTRL_SET_WB_SWAP_MASK)
#define | PXP_PS_CTRL_SET_RSVD0_MASK (0xC0U)
#define | PXP_PS_CTRL_SET_RSVD0_SHIFT (6U)
#define | PXP_PS_CTRL_SET_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_RSVD0_SHIFT)) & PXP_PS_CTRL_SET_RSVD0_MASK)
#define | PXP_PS_CTRL_SET_DECY_MASK (0x300U)
#define | PXP_PS_CTRL_SET_DECY_SHIFT (8U)
#define | PXP_PS_CTRL_SET_DECY(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_DECY_SHIFT)) & PXP_PS_CTRL_SET_DECY_MASK)
#define | PXP_PS_CTRL_SET_DECX_MASK (0xC00U)
#define | PXP_PS_CTRL_SET_DECX_SHIFT (10U)
#define | PXP_PS_CTRL_SET_DECX(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_DECX_SHIFT)) & PXP_PS_CTRL_SET_DECX_MASK)
#define | PXP_PS_CTRL_SET_RSVD1_MASK (0xFFFFF000U)
#define | PXP_PS_CTRL_SET_RSVD1_SHIFT (12U)
#define | PXP_PS_CTRL_SET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_RSVD1_SHIFT)) & PXP_PS_CTRL_SET_RSVD1_MASK)

## PS_CTRL_CLR - Processed Surface (PS) Control Register

#define | PXP_PS_CTRL_CLR_FORMAT_MASK (0x1FU)
#define | PXP_PS_CTRL_CLR_FORMAT_SHIFT (0U)
#define | PXP_PS_CTRL_CLR_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_FORMAT_SHIFT)) & PXP_PS_CTRL_CLR_FORMAT_MASK)
#define | PXP_PS_CTRL_CLR_WB_SWAP_MASK (0x20U)
#define | PXP_PS_CTRL_CLR_WB_SWAP_SHIFT (5U)
#define | PXP_PS_CTRL_CLR_WB_SWAP(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_WB_SWAP_SHIFT)) & PXP_PS_CTRL_CLR_WB_SWAP_MASK)
#define | PXP_PS_CTRL_CLR_RSVD0_MASK (0xC0U)
#define | PXP_PS_CTRL_CLR_RSVD0_SHIFT (6U)
#define | PXP_PS_CTRL_CLR_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_RSVD0_SHIFT)) & PXP_PS_CTRL_CLR_RSVD0_MASK)
#define | PXP_PS_CTRL_CLR_DECY_MASK (0x300U)
#define | PXP_PS_CTRL_CLR_DECY_SHIFT (8U)
#define | PXP_PS_CTRL_CLR_DECY(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_DECY_SHIFT)) & PXP_PS_CTRL_CLR_DECY_MASK)
#define | PXP_PS_CTRL_CLR_DECX_MASK (0xC00U)
#define | PXP_PS_CTRL_CLR_DECX_SHIFT (10U)
#define | PXP_PS_CTRL_CLR_DECX(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_DECX_SHIFT)) & PXP_PS_CTRL_CLR_DECX_MASK)
#define | PXP_PS_CTRL_CLR_RSVD1_MASK (0xFFFFF000U)
#define | PXP_PS_CTRL_CLR_RSVD1_SHIFT (12U)
#define | PXP_PS_CTRL_CLR_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_RSVD1_SHIFT)) & PXP_PS_CTRL_CLR_RSVD1_MASK)

## PS_CTRL_TOG - Processed Surface (PS) Control Register

#define | PXP_PS_CTRL_TOG_FORMAT_MASK (0x1FU)
#define | PXP_PS_CTRL_TOG_FORMAT_SHIFT (0U)
#define | PXP_PS_CTRL_TOG_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_FORMAT_SHIFT)) & PXP_PS_CTRL_TOG_FORMAT_MASK)
#define | PXP_PS_CTRL_TOG_WB_SWAP_MASK (0x20U)
#define | PXP_PS_CTRL_TOG_WB_SWAP_SHIFT (5U)
#define | PXP_PS_CTRL_TOG_WB_SWAP(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_WB_SWAP_SHIFT)) & PXP_PS_CTRL_TOG_WB_SWAP_MASK)
#define | PXP_PS_CTRL_TOG_RSVD0_MASK (0xC0U)
#define | PXP_PS_CTRL_TOG_RSVD0_SHIFT (6U)
#define | PXP_PS_CTRL_TOG_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_RSVD0_SHIFT)) & PXP_PS_CTRL_TOG_RSVD0_MASK)
#define | PXP_PS_CTRL_TOG_DECY_MASK (0x300U)
#define | PXP_PS_CTRL_TOG_DECY_SHIFT (8U)
#define | PXP_PS_CTRL_TOG_DECY(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_DECY_SHIFT)) & PXP_PS_CTRL_TOG_DECY_MASK)
#define | PXP_PS_CTRL_TOG_DECX_MASK (0xC00U)
#define | PXP_PS_CTRL_TOG_DECX_SHIFT (10U)
#define | PXP_PS_CTRL_TOG_DECX(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_DECX_SHIFT)) & PXP_PS_CTRL_TOG_DECX_MASK)
#define | PXP_PS_CTRL_TOG_RSVD1_MASK (0xFFFFF000U)
#define | PXP_PS_CTRL_TOG_RSVD1_SHIFT (12U)
#define | PXP_PS_CTRL_TOG_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_RSVD1_SHIFT)) & PXP_PS_CTRL_TOG_RSVD1_MASK)

## PS_BUF - PS Input Buffer Address

#define | PXP_PS_BUF_ADDR_MASK (0xFFFFFFFFU)
#define | PXP_PS_BUF_ADDR_SHIFT (0U)
#define | PXP_PS_BUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_BUF_ADDR_SHIFT)) & PXP_PS_BUF_ADDR_MASK)

## PS_UBUF - PS U/Cb or 2 Plane UV Input Buffer Address

#define | PXP_PS_UBUF_ADDR_MASK (0xFFFFFFFFU)
#define | PXP_PS_UBUF_ADDR_SHIFT (0U)
#define | PXP_PS_UBUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_UBUF_ADDR_SHIFT)) & PXP_PS_UBUF_ADDR_MASK)

## PS_VBUF - PS V/Cr Input Buffer Address

#define | PXP_PS_VBUF_ADDR_MASK (0xFFFFFFFFU)
#define | PXP_PS_VBUF_ADDR_SHIFT (0U)
#define | PXP_PS_VBUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_VBUF_ADDR_SHIFT)) & PXP_PS_VBUF_ADDR_MASK)

## PS_PITCH - Processed Surface Pitch

#define | PXP_PS_PITCH_PITCH_MASK (0xFFFFU)
#define | PXP_PS_PITCH_PITCH_SHIFT (0U)
#define | PXP_PS_PITCH_PITCH(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_PITCH_PITCH_SHIFT)) & PXP_PS_PITCH_PITCH_MASK)
#define | PXP_PS_PITCH_RSVD_MASK (0xFFFF0000U)
#define | PXP_PS_PITCH_RSVD_SHIFT (16U)
#define | PXP_PS_PITCH_RSVD(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_PITCH_RSVD_SHIFT)) & PXP_PS_PITCH_RSVD_MASK)

## PS_BACKGROUND - PS Background Color

#define | PXP_PS_BACKGROUND_COLOR_MASK (0xFFFFFFU)
#define | PXP_PS_BACKGROUND_COLOR_SHIFT (0U)
#define | PXP_PS_BACKGROUND_COLOR(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_BACKGROUND_COLOR_SHIFT)) & PXP_PS_BACKGROUND_COLOR_MASK)
#define | PXP_PS_BACKGROUND_RSVD_MASK (0xFF000000U)
#define | PXP_PS_BACKGROUND_RSVD_SHIFT (24U)
#define | PXP_PS_BACKGROUND_RSVD(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_BACKGROUND_RSVD_SHIFT)) & PXP_PS_BACKGROUND_RSVD_MASK)

## PS_SCALE - PS Scale Factor Register

#define | PXP_PS_SCALE_XSCALE_MASK (0x7FFFU)
#define | PXP_PS_SCALE_XSCALE_SHIFT (0U)
#define | PXP_PS_SCALE_XSCALE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_XSCALE_SHIFT)) & PXP_PS_SCALE_XSCALE_MASK)
#define | PXP_PS_SCALE_RSVD1_MASK (0x8000U)
#define | PXP_PS_SCALE_RSVD1_SHIFT (15U)
#define | PXP_PS_SCALE_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_RSVD1_SHIFT)) & PXP_PS_SCALE_RSVD1_MASK)
#define | PXP_PS_SCALE_YSCALE_MASK (0x7FFF0000U)
#define | PXP_PS_SCALE_YSCALE_SHIFT (16U)
#define | PXP_PS_SCALE_YSCALE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_YSCALE_SHIFT)) & PXP_PS_SCALE_YSCALE_MASK)
#define | PXP_PS_SCALE_RSVD2_MASK (0x80000000U)
#define | PXP_PS_SCALE_RSVD2_SHIFT (31U)
#define | PXP_PS_SCALE_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_RSVD2_SHIFT)) & PXP_PS_SCALE_RSVD2_MASK)

## PS_OFFSET - PS Scale Offset Register

#define | PXP_PS_OFFSET_XOFFSET_MASK (0xFFFU)
#define | PXP_PS_OFFSET_XOFFSET_SHIFT (0U)
#define | PXP_PS_OFFSET_XOFFSET(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_XOFFSET_SHIFT)) & PXP_PS_OFFSET_XOFFSET_MASK)
#define | PXP_PS_OFFSET_RSVD1_MASK (0xF000U)
#define | PXP_PS_OFFSET_RSVD1_SHIFT (12U)
#define | PXP_PS_OFFSET_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_RSVD1_SHIFT)) & PXP_PS_OFFSET_RSVD1_MASK)
#define | PXP_PS_OFFSET_YOFFSET_MASK (0xFFF0000U)
#define | PXP_PS_OFFSET_YOFFSET_SHIFT (16U)
#define | PXP_PS_OFFSET_YOFFSET(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_YOFFSET_SHIFT)) & PXP_PS_OFFSET_YOFFSET_MASK)
#define | PXP_PS_OFFSET_RSVD2_MASK (0xF0000000U)
#define | PXP_PS_OFFSET_RSVD2_SHIFT (28U)
#define | PXP_PS_OFFSET_RSVD2(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_RSVD2_SHIFT)) & PXP_PS_OFFSET_RSVD2_MASK)

## PS_CLRKEYLOW - PS Color Key Low

#define | PXP_PS_CLRKEYLOW_PIXEL_MASK (0xFFFFFFU)
#define | PXP_PS_CLRKEYLOW_PIXEL_SHIFT (0U)
#define | PXP_PS_CLRKEYLOW_PIXEL(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYLOW_PIXEL_SHIFT)) & PXP_PS_CLRKEYLOW_PIXEL_MASK)
#define | PXP_PS_CLRKEYLOW_RSVD1_MASK (0xFF000000U)
#define | PXP_PS_CLRKEYLOW_RSVD1_SHIFT (24U)
#define | PXP_PS_CLRKEYLOW_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYLOW_RSVD1_SHIFT)) & PXP_PS_CLRKEYLOW_RSVD1_MASK)

## PS_CLRKEYHIGH - PS Color Key High

#define | PXP_PS_CLRKEYHIGH_PIXEL_MASK (0xFFFFFFU)
#define | PXP_PS_CLRKEYHIGH_PIXEL_SHIFT (0U)
#define | PXP_PS_CLRKEYHIGH_PIXEL(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYHIGH_PIXEL_SHIFT)) & PXP_PS_CLRKEYHIGH_PIXEL_MASK)
#define | PXP_PS_CLRKEYHIGH_RSVD1_MASK (0xFF000000U)
#define | PXP_PS_CLRKEYHIGH_RSVD1_SHIFT (24U)
#define | PXP_PS_CLRKEYHIGH_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYHIGH_RSVD1_SHIFT)) & PXP_PS_CLRKEYHIGH_RSVD1_MASK)

## AS_CTRL - Alpha Surface Control

#define | PXP_AS_CTRL_RSVD0_MASK (0x1U)
#define | PXP_AS_CTRL_RSVD0_SHIFT (0U)
#define | PXP_AS_CTRL_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_RSVD0_SHIFT)) & PXP_AS_CTRL_RSVD0_MASK)
#define | PXP_AS_CTRL_ALPHA_CTRL_MASK (0x6U)
#define | PXP_AS_CTRL_ALPHA_CTRL_SHIFT (1U)
#define | PXP_AS_CTRL_ALPHA_CTRL(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ALPHA_CTRL_SHIFT)) & PXP_AS_CTRL_ALPHA_CTRL_MASK)
#define | PXP_AS_CTRL_ENABLE_COLORKEY_MASK (0x8U)
#define | PXP_AS_CTRL_ENABLE_COLORKEY_SHIFT (3U)
#define | PXP_AS_CTRL_ENABLE_COLORKEY(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ENABLE_COLORKEY_SHIFT)) & PXP_AS_CTRL_ENABLE_COLORKEY_MASK)
#define | PXP_AS_CTRL_FORMAT_MASK (0xF0U)
#define | PXP_AS_CTRL_FORMAT_SHIFT (4U)
#define | PXP_AS_CTRL_FORMAT(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_FORMAT_SHIFT)) & PXP_AS_CTRL_FORMAT_MASK)
#define | PXP_AS_CTRL_ALPHA_MASK (0xFF00U)
#define | PXP_AS_CTRL_ALPHA_SHIFT (8U)
#define | PXP_AS_CTRL_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ALPHA_SHIFT)) & PXP_AS_CTRL_ALPHA_MASK)
#define | PXP_AS_CTRL_ROP_MASK (0xF0000U)
#define | PXP_AS_CTRL_ROP_SHIFT (16U)
#define | PXP_AS_CTRL_ROP(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ROP_SHIFT)) & PXP_AS_CTRL_ROP_MASK)
#define | PXP_AS_CTRL_ALPHA_INVERT_MASK (0x100000U)
#define | PXP_AS_CTRL_ALPHA_INVERT_SHIFT (20U)
#define | PXP_AS_CTRL_ALPHA_INVERT(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ALPHA_INVERT_SHIFT)) & PXP_AS_CTRL_ALPHA_INVERT_MASK)
#define | PXP_AS_CTRL_RSVD1_MASK (0xFFE00000U)
#define | PXP_AS_CTRL_RSVD1_SHIFT (21U)
#define | PXP_AS_CTRL_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_RSVD1_SHIFT)) & PXP_AS_CTRL_RSVD1_MASK)

## AS_BUF - Alpha Surface Buffer Pointer

#define | PXP_AS_BUF_ADDR_MASK (0xFFFFFFFFU)
#define | PXP_AS_BUF_ADDR_SHIFT (0U)
#define | PXP_AS_BUF_ADDR(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_BUF_ADDR_SHIFT)) & PXP_AS_BUF_ADDR_MASK)

## AS_PITCH - Alpha Surface Pitch

#define | PXP_AS_PITCH_PITCH_MASK (0xFFFFU)
#define | PXP_AS_PITCH_PITCH_SHIFT (0U)
#define | PXP_AS_PITCH_PITCH(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_PITCH_PITCH_SHIFT)) & PXP_AS_PITCH_PITCH_MASK)
#define | PXP_AS_PITCH_RSVD_MASK (0xFFFF0000U)
#define | PXP_AS_PITCH_RSVD_SHIFT (16U)
#define | PXP_AS_PITCH_RSVD(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_PITCH_RSVD_SHIFT)) & PXP_AS_PITCH_RSVD_MASK)

## AS_CLRKEYLOW - Overlay Color Key Low

#define | PXP_AS_CLRKEYLOW_PIXEL_MASK (0xFFFFFFU)
#define | PXP_AS_CLRKEYLOW_PIXEL_SHIFT (0U)
#define | PXP_AS_CLRKEYLOW_PIXEL(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYLOW_PIXEL_SHIFT)) & PXP_AS_CLRKEYLOW_PIXEL_MASK)
#define | PXP_AS_CLRKEYLOW_RSVD1_MASK (0xFF000000U)
#define | PXP_AS_CLRKEYLOW_RSVD1_SHIFT (24U)
#define | PXP_AS_CLRKEYLOW_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYLOW_RSVD1_SHIFT)) & PXP_AS_CLRKEYLOW_RSVD1_MASK)

## AS_CLRKEYHIGH - Overlay Color Key High

#define | PXP_AS_CLRKEYHIGH_PIXEL_MASK (0xFFFFFFU)
#define | PXP_AS_CLRKEYHIGH_PIXEL_SHIFT (0U)
#define | PXP_AS_CLRKEYHIGH_PIXEL(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYHIGH_PIXEL_SHIFT)) & PXP_AS_CLRKEYHIGH_PIXEL_MASK)
#define | PXP_AS_CLRKEYHIGH_RSVD1_MASK (0xFF000000U)
#define | PXP_AS_CLRKEYHIGH_RSVD1_SHIFT (24U)
#define | PXP_AS_CLRKEYHIGH_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYHIGH_RSVD1_SHIFT)) & PXP_AS_CLRKEYHIGH_RSVD1_MASK)

## CSC1_COEF0 - Color Space Conversion Coefficient Register 0

#define | PXP_CSC1_COEF0_Y_OFFSET_MASK (0x1FFU)
#define | PXP_CSC1_COEF0_Y_OFFSET_SHIFT (0U)
#define | PXP_CSC1_COEF0_Y_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_Y_OFFSET_SHIFT)) & PXP_CSC1_COEF0_Y_OFFSET_MASK)
#define | PXP_CSC1_COEF0_UV_OFFSET_MASK (0x3FE00U)
#define | PXP_CSC1_COEF0_UV_OFFSET_SHIFT (9U)
#define | PXP_CSC1_COEF0_UV_OFFSET(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_UV_OFFSET_SHIFT)) & PXP_CSC1_COEF0_UV_OFFSET_MASK)
#define | PXP_CSC1_COEF0_C0_MASK (0x1FFC0000U)
#define | PXP_CSC1_COEF0_C0_SHIFT (18U)
#define | PXP_CSC1_COEF0_C0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_C0_SHIFT)) & PXP_CSC1_COEF0_C0_MASK)
#define | PXP_CSC1_COEF0_RSVD1_MASK (0x20000000U)
#define | PXP_CSC1_COEF0_RSVD1_SHIFT (29U)
#define | PXP_CSC1_COEF0_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_RSVD1_SHIFT)) & PXP_CSC1_COEF0_RSVD1_MASK)
#define | PXP_CSC1_COEF0_BYPASS_MASK (0x40000000U)
#define | PXP_CSC1_COEF0_BYPASS_SHIFT (30U)
#define | PXP_CSC1_COEF0_BYPASS(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_BYPASS_SHIFT)) & PXP_CSC1_COEF0_BYPASS_MASK)
#define | PXP_CSC1_COEF0_YCBCR_MODE_MASK (0x80000000U)
#define | PXP_CSC1_COEF0_YCBCR_MODE_SHIFT (31U)
#define | PXP_CSC1_COEF0_YCBCR_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_YCBCR_MODE_SHIFT)) & PXP_CSC1_COEF0_YCBCR_MODE_MASK)

## CSC1_COEF1 - Color Space Conversion Coefficient Register 1

#define | PXP_CSC1_COEF1_C4_MASK (0x7FFU)
#define | PXP_CSC1_COEF1_C4_SHIFT (0U)
#define | PXP_CSC1_COEF1_C4(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_C4_SHIFT)) & PXP_CSC1_COEF1_C4_MASK)
#define | PXP_CSC1_COEF1_RSVD0_MASK (0xF800U)
#define | PXP_CSC1_COEF1_RSVD0_SHIFT (11U)
#define | PXP_CSC1_COEF1_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_RSVD0_SHIFT)) & PXP_CSC1_COEF1_RSVD0_MASK)
#define | PXP_CSC1_COEF1_C1_MASK (0x7FF0000U)
#define | PXP_CSC1_COEF1_C1_SHIFT (16U)
#define | PXP_CSC1_COEF1_C1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_C1_SHIFT)) & PXP_CSC1_COEF1_C1_MASK)
#define | PXP_CSC1_COEF1_RSVD1_MASK (0xF8000000U)
#define | PXP_CSC1_COEF1_RSVD1_SHIFT (27U)
#define | PXP_CSC1_COEF1_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_RSVD1_SHIFT)) & PXP_CSC1_COEF1_RSVD1_MASK)

## CSC1_COEF2 - Color Space Conversion Coefficient Register 2

#define | PXP_CSC1_COEF2_C3_MASK (0x7FFU)
#define | PXP_CSC1_COEF2_C3_SHIFT (0U)
#define | PXP_CSC1_COEF2_C3(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_C3_SHIFT)) & PXP_CSC1_COEF2_C3_MASK)
#define | PXP_CSC1_COEF2_RSVD0_MASK (0xF800U)
#define | PXP_CSC1_COEF2_RSVD0_SHIFT (11U)
#define | PXP_CSC1_COEF2_RSVD0(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_RSVD0_SHIFT)) & PXP_CSC1_COEF2_RSVD0_MASK)
#define | PXP_CSC1_COEF2_C2_MASK (0x7FF0000U)
#define | PXP_CSC1_COEF2_C2_SHIFT (16U)
#define | PXP_CSC1_COEF2_C2(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_C2_SHIFT)) & PXP_CSC1_COEF2_C2_MASK)
#define | PXP_CSC1_COEF2_RSVD1_MASK (0xF8000000U)
#define | PXP_CSC1_COEF2_RSVD1_SHIFT (27U)
#define | PXP_CSC1_COEF2_RSVD1(x) (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_RSVD1_SHIFT)) & PXP_CSC1_COEF2_RSVD1_MASK)

## POWER - PXP Power Control Register

#define | PXP_POWER_ROT_MEM_LP_STATE_MASK (0xE00U)
#define | PXP_POWER_ROT_MEM_LP_STATE_SHIFT (9U)
#define | PXP_POWER_ROT_MEM_LP_STATE(x) (((uint32_t)(((uint32_t)(x)) << PXP_POWER_ROT_MEM_LP_STATE_SHIFT)) & PXP_POWER_ROT_MEM_LP_STATE_MASK)
#define | PXP_POWER_CTRL_MASK (0xFFFFF000U)
#define | PXP_POWER_CTRL_SHIFT (12U)
#define | PXP_POWER_CTRL(x) (((uint32_t)(((uint32_t)(x)) << PXP_POWER_CTRL_SHIFT)) & PXP_POWER_CTRL_MASK)

## NEXT - Next Frame Pointer

#define | PXP_NEXT_ENABLED_MASK (0x1U)
#define | PXP_NEXT_ENABLED_SHIFT (0U)
#define | PXP_NEXT_ENABLED(x) (((uint32_t)(((uint32_t)(x)) << PXP_NEXT_ENABLED_SHIFT)) & PXP_NEXT_ENABLED_MASK)
#define | PXP_NEXT_RSVD_MASK (0x2U)
#define | PXP_NEXT_RSVD_SHIFT (1U)
#define | PXP_NEXT_RSVD(x) (((uint32_t)(((uint32_t)(x)) << PXP_NEXT_RSVD_SHIFT)) & PXP_NEXT_RSVD_MASK)
#define | PXP_NEXT_POINTER_MASK (0xFFFFFFFCU)
#define | PXP_NEXT_POINTER_SHIFT (2U)
#define | PXP_NEXT_POINTER(x) (((uint32_t)(((uint32_t)(x)) << PXP_NEXT_POINTER_SHIFT)) & PXP_NEXT_POINTER_MASK)

## PORTER_DUFF_CTRL - PXP Alpha Engine A Control Register.

#define | PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_MASK (0x1U)
#define | PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_SHIFT (0U)
#define | PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_SHIFT)) & PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_MASK (0x6U)
#define | PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_SHIFT (1U)
#define | PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_MASK (0x18U)
#define | PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_SHIFT (3U)
#define | PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_MASK (0x20U)
#define | PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_SHIFT (5U)
#define | PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_MASK (0x40U)
#define | PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_SHIFT (6U)
#define | PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_MASK (0x300U)
#define | PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_SHIFT (8U)
#define | PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_MASK (0xC00U)
#define | PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_SHIFT (10U)
#define | PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_MASK (0x1000U)
#define | PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_SHIFT (12U)
#define | PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_MASK (0x2000U)
#define | PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_SHIFT (13U)
#define | PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_MASK)
#define | PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MASK (0xFF0000U)
#define | PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_SHIFT (16U)
#define | PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MASK)
#define | PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MASK (0xFF000000U)
#define | PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_SHIFT (24U)
#define | PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA(x) (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MASK)

## Detailed Description

## Macro Definition Documentation

## ◆ PXP_AS_BUF_ADDR

#define PXP_AS_BUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_BUF_ADDR_SHIFT)) & PXP_AS_BUF_ADDR_MASK)

Definition at line 35832 of file MIMXRT1062.h.

## ◆ PXP_AS_BUF_ADDR_MASK

#define PXP_AS_BUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 35830 of file MIMXRT1062.h.

## ◆ PXP_AS_BUF_ADDR_SHIFT

#define PXP_AS_BUF_ADDR_SHIFT (0U)

Definition at line 35831 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYHIGH_PIXEL

#define PXP_AS_CLRKEYHIGH_PIXEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYHIGH_PIXEL_SHIFT)) & PXP_AS_CLRKEYHIGH_PIXEL_MASK)

Definition at line 35859 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYHIGH_PIXEL_MASK

#define PXP_AS_CLRKEYHIGH_PIXEL_MASK (0xFFFFFFU)

Definition at line 35857 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYHIGH_PIXEL_SHIFT

#define PXP_AS_CLRKEYHIGH_PIXEL_SHIFT (0U)

Definition at line 35858 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYHIGH_RSVD1

#define PXP_AS_CLRKEYHIGH_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYHIGH_RSVD1_SHIFT)) & PXP_AS_CLRKEYHIGH_RSVD1_MASK)

Definition at line 35862 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYHIGH_RSVD1_MASK

#define PXP_AS_CLRKEYHIGH_RSVD1_MASK (0xFF000000U)

Definition at line 35860 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYHIGH_RSVD1_SHIFT

#define PXP_AS_CLRKEYHIGH_RSVD1_SHIFT (24U)

Definition at line 35861 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYLOW_PIXEL

#define PXP_AS_CLRKEYLOW_PIXEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYLOW_PIXEL_SHIFT)) & PXP_AS_CLRKEYLOW_PIXEL_MASK)

Definition at line 35849 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYLOW_PIXEL_MASK

#define PXP_AS_CLRKEYLOW_PIXEL_MASK (0xFFFFFFU)

Definition at line 35847 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYLOW_PIXEL_SHIFT

#define PXP_AS_CLRKEYLOW_PIXEL_SHIFT (0U)

Definition at line 35848 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYLOW_RSVD1

#define PXP_AS_CLRKEYLOW_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CLRKEYLOW_RSVD1_SHIFT)) & PXP_AS_CLRKEYLOW_RSVD1_MASK)

Definition at line 35852 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYLOW_RSVD1_MASK

#define PXP_AS_CLRKEYLOW_RSVD1_MASK (0xFF000000U)

Definition at line 35850 of file MIMXRT1062.h.

## ◆ PXP_AS_CLRKEYLOW_RSVD1_SHIFT

#define PXP_AS_CLRKEYLOW_RSVD1_SHIFT (24U)

Definition at line 35851 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA

#define PXP_AS_CTRL_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ALPHA_SHIFT)) & PXP_AS_CTRL_ALPHA_MASK)

Definition at line 35802 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_CTRL

#define PXP_AS_CTRL_ALPHA_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ALPHA_CTRL_SHIFT)) & PXP_AS_CTRL_ALPHA_CTRL_MASK)

ALPHA_CTRL 0b00..Indicates that the AS pixel alpha value will be used to blend the AS with PS. The ALPHA field is ignored. 0b01..Indicates that the value in the ALPHA field should be used instead of the alpha values present in the input pixels. 0b10..Indicates that the value in the ALPHA field should be used to scale all pixel alpha values. Each pixel alpha is multiplied by the value in the ALPHA field. 0b11..Enable ROPs. The ROP field indicates an operation to be performed on the alpha surface and PS pixels.

Definition at line 35784 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_CTRL_MASK

#define PXP_AS_CTRL_ALPHA_CTRL_MASK (0x6U)

Definition at line 35775 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_CTRL_SHIFT

#define PXP_AS_CTRL_ALPHA_CTRL_SHIFT (1U)

Definition at line 35776 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_INVERT

#define PXP_AS_CTRL_ALPHA_INVERT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ALPHA_INVERT_SHIFT)) & PXP_AS_CTRL_ALPHA_INVERT_MASK)

Definition at line 35822 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_INVERT_MASK

#define PXP_AS_CTRL_ALPHA_INVERT_MASK (0x100000U)

Definition at line 35820 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_INVERT_SHIFT

#define PXP_AS_CTRL_ALPHA_INVERT_SHIFT (20U)

Definition at line 35821 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_MASK

#define PXP_AS_CTRL_ALPHA_MASK (0xFF00U)

Definition at line 35800 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ALPHA_SHIFT

#define PXP_AS_CTRL_ALPHA_SHIFT (8U)

Definition at line 35801 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ENABLE_COLORKEY

#define PXP_AS_CTRL_ENABLE_COLORKEY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ENABLE_COLORKEY_SHIFT)) & PXP_AS_CTRL_ENABLE_COLORKEY_MASK)

Definition at line 35787 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ENABLE_COLORKEY_MASK

#define PXP_AS_CTRL_ENABLE_COLORKEY_MASK (0x8U)

Definition at line 35785 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ENABLE_COLORKEY_SHIFT

#define PXP_AS_CTRL_ENABLE_COLORKEY_SHIFT (3U)

Definition at line 35786 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_FORMAT

#define PXP_AS_CTRL_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_FORMAT_SHIFT)) & PXP_AS_CTRL_FORMAT_MASK)

FORMAT 0b0000..32-bit pixels with alpha 0b0100..32-bit pixels without alpha (unpacked 24-bit format) 0b1000..16-bit pixels with alpha 0b1001..16-bit pixels with alpha 0b1100..16-bit pixels without alpha 0b1101..16-bit pixels without alpha 0b1110..16-bit pixels without alpha

Definition at line 35799 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_FORMAT_MASK

#define PXP_AS_CTRL_FORMAT_MASK (0xF0U)

Definition at line 35788 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_FORMAT_SHIFT

#define PXP_AS_CTRL_FORMAT_SHIFT (4U)

Definition at line 35789 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ROP

#define PXP_AS_CTRL_ROP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_ROP_SHIFT)) & PXP_AS_CTRL_ROP_MASK)

ROP 0b0000..AS AND PS 0b0001..nAS AND PS 0b0010..AS AND nPS 0b0011..AS OR PS 0b0100..nAS OR PS 0b0101..AS OR nPS 0b0110..nAS 0b0111..nPS 0b1000..AS NAND PS 0b1001..AS NOR PS 0b1010..AS XOR PS 0b1011..AS XNOR PS

Definition at line 35819 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ROP_MASK

#define PXP_AS_CTRL_ROP_MASK (0xF0000U)

Definition at line 35803 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_ROP_SHIFT

#define PXP_AS_CTRL_ROP_SHIFT (16U)

Definition at line 35804 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_RSVD0

#define PXP_AS_CTRL_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_RSVD0_SHIFT)) & PXP_AS_CTRL_RSVD0_MASK)

Definition at line 35774 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_RSVD0_MASK

#define PXP_AS_CTRL_RSVD0_MASK (0x1U)

Definition at line 35772 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_RSVD0_SHIFT

#define PXP_AS_CTRL_RSVD0_SHIFT (0U)

Definition at line 35773 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_RSVD1

#define PXP_AS_CTRL_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_CTRL_RSVD1_SHIFT)) & PXP_AS_CTRL_RSVD1_MASK)

Definition at line 35825 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_RSVD1_MASK

#define PXP_AS_CTRL_RSVD1_MASK (0xFFE00000U)

Definition at line 35823 of file MIMXRT1062.h.

## ◆ PXP_AS_CTRL_RSVD1_SHIFT

#define PXP_AS_CTRL_RSVD1_SHIFT (21U)

Definition at line 35824 of file MIMXRT1062.h.

## ◆ PXP_AS_PITCH_PITCH

#define PXP_AS_PITCH_PITCH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_PITCH_PITCH_SHIFT)) & PXP_AS_PITCH_PITCH_MASK)

Definition at line 35839 of file MIMXRT1062.h.

## ◆ PXP_AS_PITCH_PITCH_MASK

#define PXP_AS_PITCH_PITCH_MASK (0xFFFFU)

Definition at line 35837 of file MIMXRT1062.h.

## ◆ PXP_AS_PITCH_PITCH_SHIFT

#define PXP_AS_PITCH_PITCH_SHIFT (0U)

Definition at line 35838 of file MIMXRT1062.h.

## ◆ PXP_AS_PITCH_RSVD

#define PXP_AS_PITCH_RSVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_AS_PITCH_RSVD_SHIFT)) & PXP_AS_PITCH_RSVD_MASK)

Definition at line 35842 of file MIMXRT1062.h.

## ◆ PXP_AS_PITCH_RSVD_MASK

#define PXP_AS_PITCH_RSVD_MASK (0xFFFF0000U)

Definition at line 35840 of file MIMXRT1062.h.

## ◆ PXP_AS_PITCH_RSVD_SHIFT

#define PXP_AS_PITCH_RSVD_SHIFT (16U)

Definition at line 35841 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_BYPASS

#define PXP_CSC1_COEF0_BYPASS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_BYPASS_SHIFT)) & PXP_CSC1_COEF0_BYPASS_MASK)

Definition at line 35881 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_BYPASS_MASK

#define PXP_CSC1_COEF0_BYPASS_MASK (0x40000000U)

Definition at line 35879 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_BYPASS_SHIFT

#define PXP_CSC1_COEF0_BYPASS_SHIFT (30U)

Definition at line 35880 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_C0

#define PXP_CSC1_COEF0_C0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_C0_SHIFT)) & PXP_CSC1_COEF0_C0_MASK)

Definition at line 35875 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_C0_MASK

#define PXP_CSC1_COEF0_C0_MASK (0x1FFC0000U)

Definition at line 35873 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_C0_SHIFT

#define PXP_CSC1_COEF0_C0_SHIFT (18U)

Definition at line 35874 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_RSVD1

#define PXP_CSC1_COEF0_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_RSVD1_SHIFT)) & PXP_CSC1_COEF0_RSVD1_MASK)

Definition at line 35878 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_RSVD1_MASK

#define PXP_CSC1_COEF0_RSVD1_MASK (0x20000000U)

Definition at line 35876 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_RSVD1_SHIFT

#define PXP_CSC1_COEF0_RSVD1_SHIFT (29U)

Definition at line 35877 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_UV_OFFSET

#define PXP_CSC1_COEF0_UV_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_UV_OFFSET_SHIFT)) & PXP_CSC1_COEF0_UV_OFFSET_MASK)

Definition at line 35872 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_UV_OFFSET_MASK

#define PXP_CSC1_COEF0_UV_OFFSET_MASK (0x3FE00U)

Definition at line 35870 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_UV_OFFSET_SHIFT

#define PXP_CSC1_COEF0_UV_OFFSET_SHIFT (9U)

Definition at line 35871 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_Y_OFFSET

#define PXP_CSC1_COEF0_Y_OFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_Y_OFFSET_SHIFT)) & PXP_CSC1_COEF0_Y_OFFSET_MASK)

Definition at line 35869 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_Y_OFFSET_MASK

#define PXP_CSC1_COEF0_Y_OFFSET_MASK (0x1FFU)

Definition at line 35867 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_Y_OFFSET_SHIFT

#define PXP_CSC1_COEF0_Y_OFFSET_SHIFT (0U)

Definition at line 35868 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_YCBCR_MODE

#define PXP_CSC1_COEF0_YCBCR_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF0_YCBCR_MODE_SHIFT)) & PXP_CSC1_COEF0_YCBCR_MODE_MASK)

Definition at line 35884 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_YCBCR_MODE_MASK

#define PXP_CSC1_COEF0_YCBCR_MODE_MASK (0x80000000U)

Definition at line 35882 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF0_YCBCR_MODE_SHIFT

#define PXP_CSC1_COEF0_YCBCR_MODE_SHIFT (31U)

Definition at line 35883 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_C1

#define PXP_CSC1_COEF1_C1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_C1_SHIFT)) & PXP_CSC1_COEF1_C1_MASK)

Definition at line 35897 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_C1_MASK

#define PXP_CSC1_COEF1_C1_MASK (0x7FF0000U)

Definition at line 35895 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_C1_SHIFT

#define PXP_CSC1_COEF1_C1_SHIFT (16U)

Definition at line 35896 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_C4

#define PXP_CSC1_COEF1_C4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_C4_SHIFT)) & PXP_CSC1_COEF1_C4_MASK)

Definition at line 35891 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_C4_MASK

#define PXP_CSC1_COEF1_C4_MASK (0x7FFU)

Definition at line 35889 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_C4_SHIFT

#define PXP_CSC1_COEF1_C4_SHIFT (0U)

Definition at line 35890 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_RSVD0

#define PXP_CSC1_COEF1_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_RSVD0_SHIFT)) & PXP_CSC1_COEF1_RSVD0_MASK)

Definition at line 35894 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_RSVD0_MASK

#define PXP_CSC1_COEF1_RSVD0_MASK (0xF800U)

Definition at line 35892 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_RSVD0_SHIFT

#define PXP_CSC1_COEF1_RSVD0_SHIFT (11U)

Definition at line 35893 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_RSVD1

#define PXP_CSC1_COEF1_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF1_RSVD1_SHIFT)) & PXP_CSC1_COEF1_RSVD1_MASK)

Definition at line 35900 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_RSVD1_MASK

#define PXP_CSC1_COEF1_RSVD1_MASK (0xF8000000U)

Definition at line 35898 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF1_RSVD1_SHIFT

#define PXP_CSC1_COEF1_RSVD1_SHIFT (27U)

Definition at line 35899 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_C2

#define PXP_CSC1_COEF2_C2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_C2_SHIFT)) & PXP_CSC1_COEF2_C2_MASK)

Definition at line 35913 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_C2_MASK

#define PXP_CSC1_COEF2_C2_MASK (0x7FF0000U)

Definition at line 35911 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_C2_SHIFT

#define PXP_CSC1_COEF2_C2_SHIFT (16U)

Definition at line 35912 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_C3

#define PXP_CSC1_COEF2_C3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_C3_SHIFT)) & PXP_CSC1_COEF2_C3_MASK)

Definition at line 35907 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_C3_MASK

#define PXP_CSC1_COEF2_C3_MASK (0x7FFU)

Definition at line 35905 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_C3_SHIFT

#define PXP_CSC1_COEF2_C3_SHIFT (0U)

Definition at line 35906 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_RSVD0

#define PXP_CSC1_COEF2_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_RSVD0_SHIFT)) & PXP_CSC1_COEF2_RSVD0_MASK)

Definition at line 35910 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_RSVD0_MASK

#define PXP_CSC1_COEF2_RSVD0_MASK (0xF800U)

Definition at line 35908 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_RSVD0_SHIFT

#define PXP_CSC1_COEF2_RSVD0_SHIFT (11U)

Definition at line 35909 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_RSVD1

#define PXP_CSC1_COEF2_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CSC1_COEF2_RSVD1_SHIFT)) & PXP_CSC1_COEF2_RSVD1_MASK)

Definition at line 35916 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_RSVD1_MASK

#define PXP_CSC1_COEF2_RSVD1_MASK (0xF8000000U)

Definition at line 35914 of file MIMXRT1062.h.

## ◆ PXP_CSC1_COEF2_RSVD1_SHIFT

#define PXP_CSC1_COEF2_RSVD1_SHIFT (27U)

Definition at line 35915 of file MIMXRT1062.h.

## ◆ PXP_CTRL_BLOCK_SIZE

#define PXP_CTRL_BLOCK_SIZE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_BLOCK_SIZE_SHIFT)) & PXP_CTRL_BLOCK_SIZE_MASK)

BLOCK_SIZE 0b0..Process 8x8 pixel blocks. 0b1..Process 16x16 pixel blocks.

Definition at line 34853 of file MIMXRT1062.h.

## ◆ PXP_CTRL_BLOCK_SIZE_MASK

#define PXP_CTRL_BLOCK_SIZE_MASK (0x800000U)

Definition at line 34847 of file MIMXRT1062.h.

## ◆ PXP_CTRL_BLOCK_SIZE_SHIFT

#define PXP_CTRL_BLOCK_SIZE_SHIFT (23U)

Definition at line 34848 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLKGATE

#define PXP_CTRL_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLKGATE_SHIFT)) & PXP_CTRL_CLKGATE_MASK)

Definition at line 34865 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLKGATE_MASK

#define PXP_CTRL_CLKGATE_MASK (0x40000000U)

Definition at line 34863 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLKGATE_SHIFT

#define PXP_CTRL_CLKGATE_SHIFT (30U)

Definition at line 34864 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_BLOCK_SIZE

#define PXP_CTRL_CLR_BLOCK_SIZE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_BLOCK_SIZE_SHIFT)) & PXP_CTRL_CLR_BLOCK_SIZE_MASK)

BLOCK_SIZE 0b0..Process 8x8 pixel blocks. 0b1..Process 16x16 pixel blocks.

Definition at line 34977 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_BLOCK_SIZE_MASK

#define PXP_CTRL_CLR_BLOCK_SIZE_MASK (0x800000U)

Definition at line 34971 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_BLOCK_SIZE_SHIFT

#define PXP_CTRL_CLR_BLOCK_SIZE_SHIFT (23U)

Definition at line 34972 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_CLKGATE

#define PXP_CTRL_CLR_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_CLKGATE_SHIFT)) & PXP_CTRL_CLR_CLKGATE_MASK)

Definition at line 34989 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_CLKGATE_MASK

#define PXP_CTRL_CLR_CLKGATE_MASK (0x40000000U)

Definition at line 34987 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_CLKGATE_SHIFT

#define PXP_CTRL_CLR_CLKGATE_SHIFT (30U)

Definition at line 34988 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_EN_REPEAT

#define PXP_CTRL_CLR_EN_REPEAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_EN_REPEAT_SHIFT)) & PXP_CTRL_CLR_EN_REPEAT_MASK)

Definition at line 34983 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_EN_REPEAT_MASK

#define PXP_CTRL_CLR_EN_REPEAT_MASK (0x10000000U)

Definition at line 34981 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_EN_REPEAT_SHIFT

#define PXP_CTRL_CLR_EN_REPEAT_SHIFT (28U)

Definition at line 34982 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ENABLE

#define PXP_CTRL_CLR_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ENABLE_SHIFT)) & PXP_CTRL_CLR_ENABLE_MASK)

Definition at line 34937 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE

#define PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_MASK)

Definition at line 34946 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_MASK

#define PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_MASK (0x10U)

Definition at line 34944 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_SHIFT

#define PXP_CTRL_CLR_ENABLE_LCD_HANDSHAKE_SHIFT (4U)

Definition at line 34945 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ENABLE_MASK

#define PXP_CTRL_CLR_ENABLE_MASK (0x1U)

Definition at line 34935 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ENABLE_SHIFT

#define PXP_CTRL_CLR_ENABLE_SHIFT (0U)

Definition at line 34936 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_HFLIP

#define PXP_CTRL_CLR_HFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_HFLIP_SHIFT)) & PXP_CTRL_CLR_HFLIP_MASK)

Definition at line 34961 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_HFLIP_MASK

#define PXP_CTRL_CLR_HFLIP_MASK (0x400U)

Definition at line 34959 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_HFLIP_SHIFT

#define PXP_CTRL_CLR_HFLIP_SHIFT (10U)

Definition at line 34960 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_IRQ_ENABLE

#define PXP_CTRL_CLR_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_IRQ_ENABLE_SHIFT)) & PXP_CTRL_CLR_IRQ_ENABLE_MASK)

Definition at line 34940 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_IRQ_ENABLE_MASK

#define PXP_CTRL_CLR_IRQ_ENABLE_MASK (0x2U)

Definition at line 34938 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_IRQ_ENABLE_SHIFT

#define PXP_CTRL_CLR_IRQ_ENABLE_SHIFT (1U)

Definition at line 34939 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_NEXT_IRQ_ENABLE

#define PXP_CTRL_CLR_NEXT_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_CLR_NEXT_IRQ_ENABLE_MASK)

Definition at line 34943 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_NEXT_IRQ_ENABLE_MASK

#define PXP_CTRL_CLR_NEXT_IRQ_ENABLE_MASK (0x4U)

Definition at line 34941 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_NEXT_IRQ_ENABLE_SHIFT

#define PXP_CTRL_CLR_NEXT_IRQ_ENABLE_SHIFT (2U)

Definition at line 34942 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ROT_POS

#define PXP_CTRL_CLR_ROT_POS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ROT_POS_SHIFT)) & PXP_CTRL_CLR_ROT_POS_MASK)

Definition at line 34970 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ROT_POS_MASK

#define PXP_CTRL_CLR_ROT_POS_MASK (0x400000U)

Definition at line 34968 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ROT_POS_SHIFT

#define PXP_CTRL_CLR_ROT_POS_SHIFT (22U)

Definition at line 34969 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ROTATE

#define PXP_CTRL_CLR_ROTATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_ROTATE_SHIFT)) & PXP_CTRL_CLR_ROTATE_MASK)

ROTATE 0b00..ROT_0 0b01..ROT_90 0b10..ROT_180 0b11..ROT_270

Definition at line 34958 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ROTATE_MASK

#define PXP_CTRL_CLR_ROTATE_MASK (0x300U)

Definition at line 34950 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_ROTATE_SHIFT

#define PXP_CTRL_CLR_ROTATE_SHIFT (8U)

Definition at line 34951 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD0

#define PXP_CTRL_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD0_SHIFT)) & PXP_CTRL_CLR_RSVD0_MASK)

Definition at line 34949 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD0_MASK

#define PXP_CTRL_CLR_RSVD0_MASK (0xE0U)

Definition at line 34947 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD0_SHIFT

#define PXP_CTRL_CLR_RSVD0_SHIFT (5U)

Definition at line 34948 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD1

#define PXP_CTRL_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD1_SHIFT)) & PXP_CTRL_CLR_RSVD1_MASK)

Definition at line 34967 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD1_MASK

#define PXP_CTRL_CLR_RSVD1_MASK (0x3FF000U)

Definition at line 34965 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD1_SHIFT

#define PXP_CTRL_CLR_RSVD1_SHIFT (12U)

Definition at line 34966 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD3

#define PXP_CTRL_CLR_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD3_SHIFT)) & PXP_CTRL_CLR_RSVD3_MASK)

Definition at line 34980 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD3_MASK

#define PXP_CTRL_CLR_RSVD3_MASK (0xF000000U)

Definition at line 34978 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD3_SHIFT

#define PXP_CTRL_CLR_RSVD3_SHIFT (24U)

Definition at line 34979 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD4

#define PXP_CTRL_CLR_RSVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_RSVD4_SHIFT)) & PXP_CTRL_CLR_RSVD4_MASK)

Definition at line 34986 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD4_MASK

#define PXP_CTRL_CLR_RSVD4_MASK (0x20000000U)

Definition at line 34984 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_RSVD4_SHIFT

#define PXP_CTRL_CLR_RSVD4_SHIFT (29U)

Definition at line 34985 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_SFTRST

#define PXP_CTRL_CLR_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_SFTRST_SHIFT)) & PXP_CTRL_CLR_SFTRST_MASK)

Definition at line 34992 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_SFTRST_MASK

#define PXP_CTRL_CLR_SFTRST_MASK (0x80000000U)

Definition at line 34990 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_SFTRST_SHIFT

#define PXP_CTRL_CLR_SFTRST_SHIFT (31U)

Definition at line 34991 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_VFLIP

#define PXP_CTRL_CLR_VFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_CLR_VFLIP_SHIFT)) & PXP_CTRL_CLR_VFLIP_MASK)

Definition at line 34964 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_VFLIP_MASK

#define PXP_CTRL_CLR_VFLIP_MASK (0x800U)

Definition at line 34962 of file MIMXRT1062.h.

## ◆ PXP_CTRL_CLR_VFLIP_SHIFT

#define PXP_CTRL_CLR_VFLIP_SHIFT (11U)

Definition at line 34963 of file MIMXRT1062.h.

## ◆ PXP_CTRL_EN_REPEAT

#define PXP_CTRL_EN_REPEAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_EN_REPEAT_SHIFT)) & PXP_CTRL_EN_REPEAT_MASK)

Definition at line 34859 of file MIMXRT1062.h.

## ◆ PXP_CTRL_EN_REPEAT_MASK

#define PXP_CTRL_EN_REPEAT_MASK (0x10000000U)

Definition at line 34857 of file MIMXRT1062.h.

## ◆ PXP_CTRL_EN_REPEAT_SHIFT

#define PXP_CTRL_EN_REPEAT_SHIFT (28U)

Definition at line 34858 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ENABLE

#define PXP_CTRL_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ENABLE_SHIFT)) & PXP_CTRL_ENABLE_MASK)

Definition at line 34813 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ENABLE_LCD_HANDSHAKE

#define PXP_CTRL_ENABLE_LCD_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_ENABLE_LCD_HANDSHAKE_MASK)

Definition at line 34822 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ENABLE_LCD_HANDSHAKE_MASK

#define PXP_CTRL_ENABLE_LCD_HANDSHAKE_MASK (0x10U)

Definition at line 34820 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ENABLE_LCD_HANDSHAKE_SHIFT

#define PXP_CTRL_ENABLE_LCD_HANDSHAKE_SHIFT (4U)

Definition at line 34821 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ENABLE_MASK

#define PXP_CTRL_ENABLE_MASK (0x1U)

Definition at line 34811 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ENABLE_SHIFT

#define PXP_CTRL_ENABLE_SHIFT (0U)

Definition at line 34812 of file MIMXRT1062.h.

## ◆ PXP_CTRL_HFLIP

#define PXP_CTRL_HFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_HFLIP_SHIFT)) & PXP_CTRL_HFLIP_MASK)

Definition at line 34837 of file MIMXRT1062.h.

## ◆ PXP_CTRL_HFLIP_MASK

#define PXP_CTRL_HFLIP_MASK (0x400U)

Definition at line 34835 of file MIMXRT1062.h.

## ◆ PXP_CTRL_HFLIP_SHIFT

#define PXP_CTRL_HFLIP_SHIFT (10U)

Definition at line 34836 of file MIMXRT1062.h.

## ◆ PXP_CTRL_IRQ_ENABLE

#define PXP_CTRL_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_IRQ_ENABLE_SHIFT)) & PXP_CTRL_IRQ_ENABLE_MASK)

Definition at line 34816 of file MIMXRT1062.h.

## ◆ PXP_CTRL_IRQ_ENABLE_MASK

#define PXP_CTRL_IRQ_ENABLE_MASK (0x2U)

Definition at line 34814 of file MIMXRT1062.h.

## ◆ PXP_CTRL_IRQ_ENABLE_SHIFT

#define PXP_CTRL_IRQ_ENABLE_SHIFT (1U)

Definition at line 34815 of file MIMXRT1062.h.

## ◆ PXP_CTRL_NEXT_IRQ_ENABLE

#define PXP_CTRL_NEXT_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_NEXT_IRQ_ENABLE_MASK)

Definition at line 34819 of file MIMXRT1062.h.

## ◆ PXP_CTRL_NEXT_IRQ_ENABLE_MASK

#define PXP_CTRL_NEXT_IRQ_ENABLE_MASK (0x4U)

Definition at line 34817 of file MIMXRT1062.h.

## ◆ PXP_CTRL_NEXT_IRQ_ENABLE_SHIFT

#define PXP_CTRL_NEXT_IRQ_ENABLE_SHIFT (2U)

Definition at line 34818 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ROT_POS

#define PXP_CTRL_ROT_POS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ROT_POS_SHIFT)) & PXP_CTRL_ROT_POS_MASK)

Definition at line 34846 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ROT_POS_MASK

#define PXP_CTRL_ROT_POS_MASK (0x400000U)

Definition at line 34844 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ROT_POS_SHIFT

#define PXP_CTRL_ROT_POS_SHIFT (22U)

Definition at line 34845 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ROTATE

#define PXP_CTRL_ROTATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_ROTATE_SHIFT)) & PXP_CTRL_ROTATE_MASK)

ROTATE 0b00..ROT_0 0b01..ROT_90 0b10..ROT_180 0b11..ROT_270

Definition at line 34834 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ROTATE_MASK

#define PXP_CTRL_ROTATE_MASK (0x300U)

Definition at line 34826 of file MIMXRT1062.h.

## ◆ PXP_CTRL_ROTATE_SHIFT

#define PXP_CTRL_ROTATE_SHIFT (8U)

Definition at line 34827 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD0

#define PXP_CTRL_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD0_SHIFT)) & PXP_CTRL_RSVD0_MASK)

Definition at line 34825 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD0_MASK

#define PXP_CTRL_RSVD0_MASK (0xE0U)

Definition at line 34823 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD0_SHIFT

#define PXP_CTRL_RSVD0_SHIFT (5U)

Definition at line 34824 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD1

#define PXP_CTRL_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD1_SHIFT)) & PXP_CTRL_RSVD1_MASK)

Definition at line 34843 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD1_MASK

#define PXP_CTRL_RSVD1_MASK (0x3FF000U)

Definition at line 34841 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD1_SHIFT

#define PXP_CTRL_RSVD1_SHIFT (12U)

Definition at line 34842 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD3

#define PXP_CTRL_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD3_SHIFT)) & PXP_CTRL_RSVD3_MASK)

Definition at line 34856 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD3_MASK

#define PXP_CTRL_RSVD3_MASK (0xF000000U)

Definition at line 34854 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD3_SHIFT

#define PXP_CTRL_RSVD3_SHIFT (24U)

Definition at line 34855 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD4

#define PXP_CTRL_RSVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_RSVD4_SHIFT)) & PXP_CTRL_RSVD4_MASK)

Definition at line 34862 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD4_MASK

#define PXP_CTRL_RSVD4_MASK (0x20000000U)

Definition at line 34860 of file MIMXRT1062.h.

## ◆ PXP_CTRL_RSVD4_SHIFT

#define PXP_CTRL_RSVD4_SHIFT (29U)

Definition at line 34861 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_BLOCK_SIZE

#define PXP_CTRL_SET_BLOCK_SIZE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_BLOCK_SIZE_SHIFT)) & PXP_CTRL_SET_BLOCK_SIZE_MASK)

BLOCK_SIZE 0b0..Process 8x8 pixel blocks. 0b1..Process 16x16 pixel blocks.

Definition at line 34915 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_BLOCK_SIZE_MASK

#define PXP_CTRL_SET_BLOCK_SIZE_MASK (0x800000U)

Definition at line 34909 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_BLOCK_SIZE_SHIFT

#define PXP_CTRL_SET_BLOCK_SIZE_SHIFT (23U)

Definition at line 34910 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_CLKGATE

#define PXP_CTRL_SET_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_CLKGATE_SHIFT)) & PXP_CTRL_SET_CLKGATE_MASK)

Definition at line 34927 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_CLKGATE_MASK

#define PXP_CTRL_SET_CLKGATE_MASK (0x40000000U)

Definition at line 34925 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_CLKGATE_SHIFT

#define PXP_CTRL_SET_CLKGATE_SHIFT (30U)

Definition at line 34926 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_EN_REPEAT

#define PXP_CTRL_SET_EN_REPEAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_EN_REPEAT_SHIFT)) & PXP_CTRL_SET_EN_REPEAT_MASK)

Definition at line 34921 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_EN_REPEAT_MASK

#define PXP_CTRL_SET_EN_REPEAT_MASK (0x10000000U)

Definition at line 34919 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_EN_REPEAT_SHIFT

#define PXP_CTRL_SET_EN_REPEAT_SHIFT (28U)

Definition at line 34920 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ENABLE

#define PXP_CTRL_SET_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ENABLE_SHIFT)) & PXP_CTRL_SET_ENABLE_MASK)

Definition at line 34875 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE

#define PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_MASK)

Definition at line 34884 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_MASK

#define PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_MASK (0x10U)

Definition at line 34882 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_SHIFT

#define PXP_CTRL_SET_ENABLE_LCD_HANDSHAKE_SHIFT (4U)

Definition at line 34883 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ENABLE_MASK

#define PXP_CTRL_SET_ENABLE_MASK (0x1U)

Definition at line 34873 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ENABLE_SHIFT

#define PXP_CTRL_SET_ENABLE_SHIFT (0U)

Definition at line 34874 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_HFLIP

#define PXP_CTRL_SET_HFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_HFLIP_SHIFT)) & PXP_CTRL_SET_HFLIP_MASK)

Definition at line 34899 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_HFLIP_MASK

#define PXP_CTRL_SET_HFLIP_MASK (0x400U)

Definition at line 34897 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_HFLIP_SHIFT

#define PXP_CTRL_SET_HFLIP_SHIFT (10U)

Definition at line 34898 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_IRQ_ENABLE

#define PXP_CTRL_SET_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_IRQ_ENABLE_SHIFT)) & PXP_CTRL_SET_IRQ_ENABLE_MASK)

Definition at line 34878 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_IRQ_ENABLE_MASK

#define PXP_CTRL_SET_IRQ_ENABLE_MASK (0x2U)

Definition at line 34876 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_IRQ_ENABLE_SHIFT

#define PXP_CTRL_SET_IRQ_ENABLE_SHIFT (1U)

Definition at line 34877 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_NEXT_IRQ_ENABLE

#define PXP_CTRL_SET_NEXT_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_SET_NEXT_IRQ_ENABLE_MASK)

Definition at line 34881 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_NEXT_IRQ_ENABLE_MASK

#define PXP_CTRL_SET_NEXT_IRQ_ENABLE_MASK (0x4U)

Definition at line 34879 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_NEXT_IRQ_ENABLE_SHIFT

#define PXP_CTRL_SET_NEXT_IRQ_ENABLE_SHIFT (2U)

Definition at line 34880 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ROT_POS

#define PXP_CTRL_SET_ROT_POS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ROT_POS_SHIFT)) & PXP_CTRL_SET_ROT_POS_MASK)

Definition at line 34908 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ROT_POS_MASK

#define PXP_CTRL_SET_ROT_POS_MASK (0x400000U)

Definition at line 34906 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ROT_POS_SHIFT

#define PXP_CTRL_SET_ROT_POS_SHIFT (22U)

Definition at line 34907 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ROTATE

#define PXP_CTRL_SET_ROTATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_ROTATE_SHIFT)) & PXP_CTRL_SET_ROTATE_MASK)

ROTATE 0b00..ROT_0 0b01..ROT_90 0b10..ROT_180 0b11..ROT_270

Definition at line 34896 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ROTATE_MASK

#define PXP_CTRL_SET_ROTATE_MASK (0x300U)

Definition at line 34888 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_ROTATE_SHIFT

#define PXP_CTRL_SET_ROTATE_SHIFT (8U)

Definition at line 34889 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD0

#define PXP_CTRL_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD0_SHIFT)) & PXP_CTRL_SET_RSVD0_MASK)

Definition at line 34887 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD0_MASK

#define PXP_CTRL_SET_RSVD0_MASK (0xE0U)

Definition at line 34885 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD0_SHIFT

#define PXP_CTRL_SET_RSVD0_SHIFT (5U)

Definition at line 34886 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD1

#define PXP_CTRL_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD1_SHIFT)) & PXP_CTRL_SET_RSVD1_MASK)

Definition at line 34905 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD1_MASK

#define PXP_CTRL_SET_RSVD1_MASK (0x3FF000U)

Definition at line 34903 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD1_SHIFT

#define PXP_CTRL_SET_RSVD1_SHIFT (12U)

Definition at line 34904 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD3

#define PXP_CTRL_SET_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD3_SHIFT)) & PXP_CTRL_SET_RSVD3_MASK)

Definition at line 34918 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD3_MASK

#define PXP_CTRL_SET_RSVD3_MASK (0xF000000U)

Definition at line 34916 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD3_SHIFT

#define PXP_CTRL_SET_RSVD3_SHIFT (24U)

Definition at line 34917 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD4

#define PXP_CTRL_SET_RSVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_RSVD4_SHIFT)) & PXP_CTRL_SET_RSVD4_MASK)

Definition at line 34924 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD4_MASK

#define PXP_CTRL_SET_RSVD4_MASK (0x20000000U)

Definition at line 34922 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_RSVD4_SHIFT

#define PXP_CTRL_SET_RSVD4_SHIFT (29U)

Definition at line 34923 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_SFTRST

#define PXP_CTRL_SET_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_SFTRST_SHIFT)) & PXP_CTRL_SET_SFTRST_MASK)

Definition at line 34930 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_SFTRST_MASK

#define PXP_CTRL_SET_SFTRST_MASK (0x80000000U)

Definition at line 34928 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_SFTRST_SHIFT

#define PXP_CTRL_SET_SFTRST_SHIFT (31U)

Definition at line 34929 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_VFLIP

#define PXP_CTRL_SET_VFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SET_VFLIP_SHIFT)) & PXP_CTRL_SET_VFLIP_MASK)

Definition at line 34902 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_VFLIP_MASK

#define PXP_CTRL_SET_VFLIP_MASK (0x800U)

Definition at line 34900 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SET_VFLIP_SHIFT

#define PXP_CTRL_SET_VFLIP_SHIFT (11U)

Definition at line 34901 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SFTRST

#define PXP_CTRL_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_SFTRST_SHIFT)) & PXP_CTRL_SFTRST_MASK)

Definition at line 34868 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SFTRST_MASK

#define PXP_CTRL_SFTRST_MASK (0x80000000U)

Definition at line 34866 of file MIMXRT1062.h.

## ◆ PXP_CTRL_SFTRST_SHIFT

#define PXP_CTRL_SFTRST_SHIFT (31U)

Definition at line 34867 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_BLOCK_SIZE

#define PXP_CTRL_TOG_BLOCK_SIZE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_BLOCK_SIZE_SHIFT)) & PXP_CTRL_TOG_BLOCK_SIZE_MASK)

BLOCK_SIZE 0b0..Process 8x8 pixel blocks. 0b1..Process 16x16 pixel blocks.

Definition at line 35039 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_BLOCK_SIZE_MASK

#define PXP_CTRL_TOG_BLOCK_SIZE_MASK (0x800000U)

Definition at line 35033 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_BLOCK_SIZE_SHIFT

#define PXP_CTRL_TOG_BLOCK_SIZE_SHIFT (23U)

Definition at line 35034 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_CLKGATE

#define PXP_CTRL_TOG_CLKGATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_CLKGATE_SHIFT)) & PXP_CTRL_TOG_CLKGATE_MASK)

Definition at line 35051 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_CLKGATE_MASK

#define PXP_CTRL_TOG_CLKGATE_MASK (0x40000000U)

Definition at line 35049 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_CLKGATE_SHIFT

#define PXP_CTRL_TOG_CLKGATE_SHIFT (30U)

Definition at line 35050 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_EN_REPEAT

#define PXP_CTRL_TOG_EN_REPEAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_EN_REPEAT_SHIFT)) & PXP_CTRL_TOG_EN_REPEAT_MASK)

Definition at line 35045 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_EN_REPEAT_MASK

#define PXP_CTRL_TOG_EN_REPEAT_MASK (0x10000000U)

Definition at line 35043 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_EN_REPEAT_SHIFT

#define PXP_CTRL_TOG_EN_REPEAT_SHIFT (28U)

Definition at line 35044 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ENABLE

#define PXP_CTRL_TOG_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ENABLE_SHIFT)) & PXP_CTRL_TOG_ENABLE_MASK)

Definition at line 34999 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE

#define PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_SHIFT)) & PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_MASK)

Definition at line 35008 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_MASK

#define PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_MASK (0x10U)

Definition at line 35006 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_SHIFT

#define PXP_CTRL_TOG_ENABLE_LCD_HANDSHAKE_SHIFT (4U)

Definition at line 35007 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ENABLE_MASK

#define PXP_CTRL_TOG_ENABLE_MASK (0x1U)

Definition at line 34997 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ENABLE_SHIFT

#define PXP_CTRL_TOG_ENABLE_SHIFT (0U)

Definition at line 34998 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_HFLIP

#define PXP_CTRL_TOG_HFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_HFLIP_SHIFT)) & PXP_CTRL_TOG_HFLIP_MASK)

Definition at line 35023 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_HFLIP_MASK

#define PXP_CTRL_TOG_HFLIP_MASK (0x400U)

Definition at line 35021 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_HFLIP_SHIFT

#define PXP_CTRL_TOG_HFLIP_SHIFT (10U)

Definition at line 35022 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_IRQ_ENABLE

#define PXP_CTRL_TOG_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_IRQ_ENABLE_SHIFT)) & PXP_CTRL_TOG_IRQ_ENABLE_MASK)

Definition at line 35002 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_IRQ_ENABLE_MASK

#define PXP_CTRL_TOG_IRQ_ENABLE_MASK (0x2U)

Definition at line 35000 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_IRQ_ENABLE_SHIFT

#define PXP_CTRL_TOG_IRQ_ENABLE_SHIFT (1U)

Definition at line 35001 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_NEXT_IRQ_ENABLE

#define PXP_CTRL_TOG_NEXT_IRQ_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_NEXT_IRQ_ENABLE_SHIFT)) & PXP_CTRL_TOG_NEXT_IRQ_ENABLE_MASK)

Definition at line 35005 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_NEXT_IRQ_ENABLE_MASK

#define PXP_CTRL_TOG_NEXT_IRQ_ENABLE_MASK (0x4U)

Definition at line 35003 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_NEXT_IRQ_ENABLE_SHIFT

#define PXP_CTRL_TOG_NEXT_IRQ_ENABLE_SHIFT (2U)

Definition at line 35004 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ROT_POS

#define PXP_CTRL_TOG_ROT_POS | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ROT_POS_SHIFT)) & PXP_CTRL_TOG_ROT_POS_MASK)

Definition at line 35032 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ROT_POS_MASK

#define PXP_CTRL_TOG_ROT_POS_MASK (0x400000U)

Definition at line 35030 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ROT_POS_SHIFT

#define PXP_CTRL_TOG_ROT_POS_SHIFT (22U)

Definition at line 35031 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ROTATE

#define PXP_CTRL_TOG_ROTATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_ROTATE_SHIFT)) & PXP_CTRL_TOG_ROTATE_MASK)

ROTATE 0b00..ROT_0 0b01..ROT_90 0b10..ROT_180 0b11..ROT_270

Definition at line 35020 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ROTATE_MASK

#define PXP_CTRL_TOG_ROTATE_MASK (0x300U)

Definition at line 35012 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_ROTATE_SHIFT

#define PXP_CTRL_TOG_ROTATE_SHIFT (8U)

Definition at line 35013 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD0

#define PXP_CTRL_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD0_SHIFT)) & PXP_CTRL_TOG_RSVD0_MASK)

Definition at line 35011 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD0_MASK

#define PXP_CTRL_TOG_RSVD0_MASK (0xE0U)

Definition at line 35009 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD0_SHIFT

#define PXP_CTRL_TOG_RSVD0_SHIFT (5U)

Definition at line 35010 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD1

#define PXP_CTRL_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD1_SHIFT)) & PXP_CTRL_TOG_RSVD1_MASK)

Definition at line 35029 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD1_MASK

#define PXP_CTRL_TOG_RSVD1_MASK (0x3FF000U)

Definition at line 35027 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD1_SHIFT

#define PXP_CTRL_TOG_RSVD1_SHIFT (12U)

Definition at line 35028 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD3

#define PXP_CTRL_TOG_RSVD3 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD3_SHIFT)) & PXP_CTRL_TOG_RSVD3_MASK)

Definition at line 35042 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD3_MASK

#define PXP_CTRL_TOG_RSVD3_MASK (0xF000000U)

Definition at line 35040 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD3_SHIFT

#define PXP_CTRL_TOG_RSVD3_SHIFT (24U)

Definition at line 35041 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD4

#define PXP_CTRL_TOG_RSVD4 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_RSVD4_SHIFT)) & PXP_CTRL_TOG_RSVD4_MASK)

Definition at line 35048 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD4_MASK

#define PXP_CTRL_TOG_RSVD4_MASK (0x20000000U)

Definition at line 35046 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_RSVD4_SHIFT

#define PXP_CTRL_TOG_RSVD4_SHIFT (29U)

Definition at line 35047 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_SFTRST

#define PXP_CTRL_TOG_SFTRST | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_SFTRST_SHIFT)) & PXP_CTRL_TOG_SFTRST_MASK)

Definition at line 35054 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_SFTRST_MASK

#define PXP_CTRL_TOG_SFTRST_MASK (0x80000000U)

Definition at line 35052 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_SFTRST_SHIFT

#define PXP_CTRL_TOG_SFTRST_SHIFT (31U)

Definition at line 35053 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_VFLIP

#define PXP_CTRL_TOG_VFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_TOG_VFLIP_SHIFT)) & PXP_CTRL_TOG_VFLIP_MASK)

Definition at line 35026 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_VFLIP_MASK

#define PXP_CTRL_TOG_VFLIP_MASK (0x800U)

Definition at line 35024 of file MIMXRT1062.h.

## ◆ PXP_CTRL_TOG_VFLIP_SHIFT

#define PXP_CTRL_TOG_VFLIP_SHIFT (11U)

Definition at line 35025 of file MIMXRT1062.h.

## ◆ PXP_CTRL_VFLIP

#define PXP_CTRL_VFLIP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_CTRL_VFLIP_SHIFT)) & PXP_CTRL_VFLIP_MASK)

Definition at line 34840 of file MIMXRT1062.h.

## ◆ PXP_CTRL_VFLIP_MASK

#define PXP_CTRL_VFLIP_MASK (0x800U)

Definition at line 34838 of file MIMXRT1062.h.

## ◆ PXP_CTRL_VFLIP_SHIFT

#define PXP_CTRL_VFLIP_SHIFT (11U)

Definition at line 34839 of file MIMXRT1062.h.

## ◆ PXP_NEXT_ENABLED

#define PXP_NEXT_ENABLED | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_NEXT_ENABLED_SHIFT)) & PXP_NEXT_ENABLED_MASK)

Definition at line 35939 of file MIMXRT1062.h.

## ◆ PXP_NEXT_ENABLED_MASK

#define PXP_NEXT_ENABLED_MASK (0x1U)

Definition at line 35937 of file MIMXRT1062.h.

## ◆ PXP_NEXT_ENABLED_SHIFT

#define PXP_NEXT_ENABLED_SHIFT (0U)

Definition at line 35938 of file MIMXRT1062.h.

## ◆ PXP_NEXT_POINTER

#define PXP_NEXT_POINTER | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_NEXT_POINTER_SHIFT)) & PXP_NEXT_POINTER_MASK)

Definition at line 35945 of file MIMXRT1062.h.

## ◆ PXP_NEXT_POINTER_MASK

#define PXP_NEXT_POINTER_MASK (0xFFFFFFFCU)

Definition at line 35943 of file MIMXRT1062.h.

## ◆ PXP_NEXT_POINTER_SHIFT

#define PXP_NEXT_POINTER_SHIFT (2U)

Definition at line 35944 of file MIMXRT1062.h.

## ◆ PXP_NEXT_RSVD

#define PXP_NEXT_RSVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_NEXT_RSVD_SHIFT)) & PXP_NEXT_RSVD_MASK)

Definition at line 35942 of file MIMXRT1062.h.

## ◆ PXP_NEXT_RSVD_MASK

#define PXP_NEXT_RSVD_MASK (0x2U)

Definition at line 35940 of file MIMXRT1062.h.

## ◆ PXP_NEXT_RSVD_SHIFT

#define PXP_NEXT_RSVD_SHIFT (1U)

Definition at line 35941 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_RSVD0

#define PXP_OUT_AS_LRC_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_RSVD0_SHIFT)) & PXP_OUT_AS_LRC_RSVD0_MASK)

Definition at line 35464 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_RSVD0_MASK

#define PXP_OUT_AS_LRC_RSVD0_MASK (0xC000U)

Definition at line 35462 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_RSVD0_SHIFT

#define PXP_OUT_AS_LRC_RSVD0_SHIFT (14U)

Definition at line 35463 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_RSVD1

#define PXP_OUT_AS_LRC_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_RSVD1_SHIFT)) & PXP_OUT_AS_LRC_RSVD1_MASK)

Definition at line 35470 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_RSVD1_MASK

#define PXP_OUT_AS_LRC_RSVD1_MASK (0xC0000000U)

Definition at line 35468 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_RSVD1_SHIFT

#define PXP_OUT_AS_LRC_RSVD1_SHIFT (30U)

Definition at line 35469 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_X

#define PXP_OUT_AS_LRC_X | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_X_SHIFT)) & PXP_OUT_AS_LRC_X_MASK)

Definition at line 35467 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_X_MASK

#define PXP_OUT_AS_LRC_X_MASK (0x3FFF0000U)

Definition at line 35465 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_X_SHIFT

#define PXP_OUT_AS_LRC_X_SHIFT (16U)

Definition at line 35466 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_Y

#define PXP_OUT_AS_LRC_Y | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_LRC_Y_SHIFT)) & PXP_OUT_AS_LRC_Y_MASK)

Definition at line 35461 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_Y_MASK

#define PXP_OUT_AS_LRC_Y_MASK (0x3FFFU)

Definition at line 35459 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_LRC_Y_SHIFT

#define PXP_OUT_AS_LRC_Y_SHIFT (0U)

Definition at line 35460 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_RSVD0

#define PXP_OUT_AS_ULC_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_RSVD0_SHIFT)) & PXP_OUT_AS_ULC_RSVD0_MASK)

Definition at line 35448 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_RSVD0_MASK

#define PXP_OUT_AS_ULC_RSVD0_MASK (0xC000U)

Definition at line 35446 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_RSVD0_SHIFT

#define PXP_OUT_AS_ULC_RSVD0_SHIFT (14U)

Definition at line 35447 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_RSVD1

#define PXP_OUT_AS_ULC_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_RSVD1_SHIFT)) & PXP_OUT_AS_ULC_RSVD1_MASK)

Definition at line 35454 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_RSVD1_MASK

#define PXP_OUT_AS_ULC_RSVD1_MASK (0xC0000000U)

Definition at line 35452 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_RSVD1_SHIFT

#define PXP_OUT_AS_ULC_RSVD1_SHIFT (30U)

Definition at line 35453 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_X

#define PXP_OUT_AS_ULC_X | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_X_SHIFT)) & PXP_OUT_AS_ULC_X_MASK)

Definition at line 35451 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_X_MASK

#define PXP_OUT_AS_ULC_X_MASK (0x3FFF0000U)

Definition at line 35449 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_X_SHIFT

#define PXP_OUT_AS_ULC_X_SHIFT (16U)

Definition at line 35450 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_Y

#define PXP_OUT_AS_ULC_Y | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_AS_ULC_Y_SHIFT)) & PXP_OUT_AS_ULC_Y_MASK)

Definition at line 35445 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_Y_MASK

#define PXP_OUT_AS_ULC_Y_MASK (0x3FFFU)

Definition at line 35443 of file MIMXRT1062.h.

## ◆ PXP_OUT_AS_ULC_Y_SHIFT

#define PXP_OUT_AS_ULC_Y_SHIFT (0U)

Definition at line 35444 of file MIMXRT1062.h.

## ◆ PXP_OUT_BUF2_ADDR

#define PXP_OUT_BUF2_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_BUF2_ADDR_SHIFT)) & PXP_OUT_BUF2_ADDR_MASK)

Definition at line 35380 of file MIMXRT1062.h.

## ◆ PXP_OUT_BUF2_ADDR_MASK

#define PXP_OUT_BUF2_ADDR_MASK (0xFFFFFFFFU)

Definition at line 35378 of file MIMXRT1062.h.

## ◆ PXP_OUT_BUF2_ADDR_SHIFT

#define PXP_OUT_BUF2_ADDR_SHIFT (0U)

Definition at line 35379 of file MIMXRT1062.h.

## ◆ PXP_OUT_BUF_ADDR

#define PXP_OUT_BUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_BUF_ADDR_SHIFT)) & PXP_OUT_BUF_ADDR_MASK)

Definition at line 35373 of file MIMXRT1062.h.

## ◆ PXP_OUT_BUF_ADDR_MASK

#define PXP_OUT_BUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 35371 of file MIMXRT1062.h.

## ◆ PXP_OUT_BUF_ADDR_SHIFT

#define PXP_OUT_BUF_ADDR_SHIFT (0U)

Definition at line 35372 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_ALPHA

#define PXP_OUT_CTRL_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_ALPHA_SHIFT)) & PXP_OUT_CTRL_ALPHA_MASK)

Definition at line 35225 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_ALPHA_MASK

#define PXP_OUT_CTRL_ALPHA_MASK (0xFF000000U)

Definition at line 35223 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_ALPHA_OUTPUT

#define PXP_OUT_CTRL_ALPHA_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_ALPHA_OUTPUT_MASK)

Definition at line 35222 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_ALPHA_OUTPUT_MASK

#define PXP_OUT_CTRL_ALPHA_OUTPUT_MASK (0x800000U)

Definition at line 35220 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_ALPHA_OUTPUT_SHIFT

#define PXP_OUT_CTRL_ALPHA_OUTPUT_SHIFT (23U)

Definition at line 35221 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_ALPHA_SHIFT

#define PXP_OUT_CTRL_ALPHA_SHIFT (24U)

Definition at line 35224 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_ALPHA

#define PXP_OUT_CTRL_CLR_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_ALPHA_SHIFT)) & PXP_OUT_CTRL_CLR_ALPHA_MASK)

Definition at line 35319 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_ALPHA_MASK

#define PXP_OUT_CTRL_CLR_ALPHA_MASK (0xFF000000U)

Definition at line 35317 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_ALPHA_OUTPUT

#define PXP_OUT_CTRL_CLR_ALPHA_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_MASK)

Definition at line 35316 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_MASK

#define PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_MASK (0x800000U)

Definition at line 35314 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_SHIFT

#define PXP_OUT_CTRL_CLR_ALPHA_OUTPUT_SHIFT (23U)

Definition at line 35315 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_ALPHA_SHIFT

#define PXP_OUT_CTRL_CLR_ALPHA_SHIFT (24U)

Definition at line 35318 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_FORMAT

#define PXP_OUT_CTRL_CLR_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_FORMAT_SHIFT)) & PXP_OUT_CTRL_CLR_FORMAT_MASK)

FORMAT 0b00000..32-bit pixels 0b00100..32-bit pixels (unpacked 24-bit pixel in 32 bit DWORD.) 0b00101..24-bit pixels (packed 24-bit format) 0b01000..16-bit pixels 0b01001..16-bit pixels 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU)

Definition at line 35298 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_FORMAT_MASK

#define PXP_OUT_CTRL_CLR_FORMAT_MASK (0x1FU)

Definition at line 35277 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_FORMAT_SHIFT

#define PXP_OUT_CTRL_CLR_FORMAT_SHIFT (0U)

Definition at line 35278 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT

#define PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_MASK)

INTERLACED_OUTPUT 0b00..All data written in progressive format to the OUTBUF Pointer. 0b01..Interlaced output: only data for field 0 is written to the OUTBUF Pointer. 0b10..Interlaced output: only data for field 1 is written to the OUTBUF2 Pointer. 0b11..Interlaced output: data for field 0 is written to OUTBUF and data for field 1 is written to OUTBUF2.

Definition at line 35310 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_MASK

#define PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_MASK (0x300U)

Definition at line 35302 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_SHIFT

#define PXP_OUT_CTRL_CLR_INTERLACED_OUTPUT_SHIFT (8U)

Definition at line 35303 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_RSVD0

#define PXP_OUT_CTRL_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_RSVD0_SHIFT)) & PXP_OUT_CTRL_CLR_RSVD0_MASK)

Definition at line 35301 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_RSVD0_MASK

#define PXP_OUT_CTRL_CLR_RSVD0_MASK (0xE0U)

Definition at line 35299 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_RSVD0_SHIFT

#define PXP_OUT_CTRL_CLR_RSVD0_SHIFT (5U)

Definition at line 35300 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_RSVD1

#define PXP_OUT_CTRL_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_CLR_RSVD1_SHIFT)) & PXP_OUT_CTRL_CLR_RSVD1_MASK)

Definition at line 35313 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_RSVD1_MASK

#define PXP_OUT_CTRL_CLR_RSVD1_MASK (0x7FFC00U)

Definition at line 35311 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_CLR_RSVD1_SHIFT

#define PXP_OUT_CTRL_CLR_RSVD1_SHIFT (10U)

Definition at line 35312 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_FORMAT

#define PXP_OUT_CTRL_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_FORMAT_SHIFT)) & PXP_OUT_CTRL_FORMAT_MASK)

FORMAT 0b00000..32-bit pixels 0b00100..32-bit pixels (unpacked 24-bit pixel in 32 bit DWORD.) 0b00101..24-bit pixels (packed 24-bit format) 0b01000..16-bit pixels 0b01001..16-bit pixels 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU)

Definition at line 35204 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_FORMAT_MASK

#define PXP_OUT_CTRL_FORMAT_MASK (0x1FU)

Definition at line 35183 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_FORMAT_SHIFT

#define PXP_OUT_CTRL_FORMAT_SHIFT (0U)

Definition at line 35184 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_INTERLACED_OUTPUT

#define PXP_OUT_CTRL_INTERLACED_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_INTERLACED_OUTPUT_MASK)

INTERLACED_OUTPUT 0b00..All data written in progressive format to the OUTBUF Pointer. 0b01..Interlaced output: only data for field 0 is written to the OUTBUF Pointer. 0b10..Interlaced output: only data for field 1 is written to the OUTBUF2 Pointer. 0b11..Interlaced output: data for field 0 is written to OUTBUF and data for field 1 is written to OUTBUF2.

Definition at line 35216 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_INTERLACED_OUTPUT_MASK

#define PXP_OUT_CTRL_INTERLACED_OUTPUT_MASK (0x300U)

Definition at line 35208 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_INTERLACED_OUTPUT_SHIFT

#define PXP_OUT_CTRL_INTERLACED_OUTPUT_SHIFT (8U)

Definition at line 35209 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_RSVD0

#define PXP_OUT_CTRL_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_RSVD0_SHIFT)) & PXP_OUT_CTRL_RSVD0_MASK)

Definition at line 35207 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_RSVD0_MASK

#define PXP_OUT_CTRL_RSVD0_MASK (0xE0U)

Definition at line 35205 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_RSVD0_SHIFT

#define PXP_OUT_CTRL_RSVD0_SHIFT (5U)

Definition at line 35206 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_RSVD1

#define PXP_OUT_CTRL_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_RSVD1_SHIFT)) & PXP_OUT_CTRL_RSVD1_MASK)

Definition at line 35219 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_RSVD1_MASK

#define PXP_OUT_CTRL_RSVD1_MASK (0x7FFC00U)

Definition at line 35217 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_RSVD1_SHIFT

#define PXP_OUT_CTRL_RSVD1_SHIFT (10U)

Definition at line 35218 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_ALPHA

#define PXP_OUT_CTRL_SET_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_ALPHA_SHIFT)) & PXP_OUT_CTRL_SET_ALPHA_MASK)

Definition at line 35272 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_ALPHA_MASK

#define PXP_OUT_CTRL_SET_ALPHA_MASK (0xFF000000U)

Definition at line 35270 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_ALPHA_OUTPUT

#define PXP_OUT_CTRL_SET_ALPHA_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_SET_ALPHA_OUTPUT_MASK)

Definition at line 35269 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_ALPHA_OUTPUT_MASK

#define PXP_OUT_CTRL_SET_ALPHA_OUTPUT_MASK (0x800000U)

Definition at line 35267 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_ALPHA_OUTPUT_SHIFT

#define PXP_OUT_CTRL_SET_ALPHA_OUTPUT_SHIFT (23U)

Definition at line 35268 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_ALPHA_SHIFT

#define PXP_OUT_CTRL_SET_ALPHA_SHIFT (24U)

Definition at line 35271 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_FORMAT

#define PXP_OUT_CTRL_SET_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_FORMAT_SHIFT)) & PXP_OUT_CTRL_SET_FORMAT_MASK)

FORMAT 0b00000..32-bit pixels 0b00100..32-bit pixels (unpacked 24-bit pixel in 32 bit DWORD.) 0b00101..24-bit pixels (packed 24-bit format) 0b01000..16-bit pixels 0b01001..16-bit pixels 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU)

Definition at line 35251 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_FORMAT_MASK

#define PXP_OUT_CTRL_SET_FORMAT_MASK (0x1FU)

Definition at line 35230 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_FORMAT_SHIFT

#define PXP_OUT_CTRL_SET_FORMAT_SHIFT (0U)

Definition at line 35231 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_INTERLACED_OUTPUT

#define PXP_OUT_CTRL_SET_INTERLACED_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_MASK)

INTERLACED_OUTPUT 0b00..All data written in progressive format to the OUTBUF Pointer. 0b01..Interlaced output: only data for field 0 is written to the OUTBUF Pointer. 0b10..Interlaced output: only data for field 1 is written to the OUTBUF2 Pointer. 0b11..Interlaced output: data for field 0 is written to OUTBUF and data for field 1 is written to OUTBUF2.

Definition at line 35263 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_MASK

#define PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_MASK (0x300U)

Definition at line 35255 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_SHIFT

#define PXP_OUT_CTRL_SET_INTERLACED_OUTPUT_SHIFT (8U)

Definition at line 35256 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_RSVD0

#define PXP_OUT_CTRL_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_RSVD0_SHIFT)) & PXP_OUT_CTRL_SET_RSVD0_MASK)

Definition at line 35254 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_RSVD0_MASK

#define PXP_OUT_CTRL_SET_RSVD0_MASK (0xE0U)

Definition at line 35252 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_RSVD0_SHIFT

#define PXP_OUT_CTRL_SET_RSVD0_SHIFT (5U)

Definition at line 35253 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_RSVD1

#define PXP_OUT_CTRL_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_SET_RSVD1_SHIFT)) & PXP_OUT_CTRL_SET_RSVD1_MASK)

Definition at line 35266 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_RSVD1_MASK

#define PXP_OUT_CTRL_SET_RSVD1_MASK (0x7FFC00U)

Definition at line 35264 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_SET_RSVD1_SHIFT

#define PXP_OUT_CTRL_SET_RSVD1_SHIFT (10U)

Definition at line 35265 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_ALPHA

#define PXP_OUT_CTRL_TOG_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_ALPHA_SHIFT)) & PXP_OUT_CTRL_TOG_ALPHA_MASK)

Definition at line 35366 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_ALPHA_MASK

#define PXP_OUT_CTRL_TOG_ALPHA_MASK (0xFF000000U)

Definition at line 35364 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_ALPHA_OUTPUT

#define PXP_OUT_CTRL_TOG_ALPHA_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_SHIFT)) & PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_MASK)

Definition at line 35363 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_MASK

#define PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_MASK (0x800000U)

Definition at line 35361 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_SHIFT

#define PXP_OUT_CTRL_TOG_ALPHA_OUTPUT_SHIFT (23U)

Definition at line 35362 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_ALPHA_SHIFT

#define PXP_OUT_CTRL_TOG_ALPHA_SHIFT (24U)

Definition at line 35365 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_FORMAT

#define PXP_OUT_CTRL_TOG_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_FORMAT_SHIFT)) & PXP_OUT_CTRL_TOG_FORMAT_MASK)

FORMAT 0b00000..32-bit pixels 0b00100..32-bit pixels (unpacked 24-bit pixel in 32 bit DWORD.) 0b00101..24-bit pixels (packed 24-bit format) 0b01000..16-bit pixels 0b01001..16-bit pixels 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU)

Definition at line 35345 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_FORMAT_MASK

#define PXP_OUT_CTRL_TOG_FORMAT_MASK (0x1FU)

Definition at line 35324 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_FORMAT_SHIFT

#define PXP_OUT_CTRL_TOG_FORMAT_SHIFT (0U)

Definition at line 35325 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT

#define PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_SHIFT)) & PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_MASK)

INTERLACED_OUTPUT 0b00..All data written in progressive format to the OUTBUF Pointer. 0b01..Interlaced output: only data for field 0 is written to the OUTBUF Pointer. 0b10..Interlaced output: only data for field 1 is written to the OUTBUF2 Pointer. 0b11..Interlaced output: data for field 0 is written to OUTBUF and data for field 1 is written to OUTBUF2.

Definition at line 35357 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_MASK

#define PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_MASK (0x300U)

Definition at line 35349 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_SHIFT

#define PXP_OUT_CTRL_TOG_INTERLACED_OUTPUT_SHIFT (8U)

Definition at line 35350 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_RSVD0

#define PXP_OUT_CTRL_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_RSVD0_SHIFT)) & PXP_OUT_CTRL_TOG_RSVD0_MASK)

Definition at line 35348 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_RSVD0_MASK

#define PXP_OUT_CTRL_TOG_RSVD0_MASK (0xE0U)

Definition at line 35346 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_RSVD0_SHIFT

#define PXP_OUT_CTRL_TOG_RSVD0_SHIFT (5U)

Definition at line 35347 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_RSVD1

#define PXP_OUT_CTRL_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_CTRL_TOG_RSVD1_SHIFT)) & PXP_OUT_CTRL_TOG_RSVD1_MASK)

Definition at line 35360 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_RSVD1_MASK

#define PXP_OUT_CTRL_TOG_RSVD1_MASK (0x7FFC00U)

Definition at line 35358 of file MIMXRT1062.h.

## ◆ PXP_OUT_CTRL_TOG_RSVD1_SHIFT

#define PXP_OUT_CTRL_TOG_RSVD1_SHIFT (10U)

Definition at line 35359 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_RSVD0

#define PXP_OUT_LRC_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_RSVD0_SHIFT)) & PXP_OUT_LRC_RSVD0_MASK)

Definition at line 35400 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_RSVD0_MASK

#define PXP_OUT_LRC_RSVD0_MASK (0xC000U)

Definition at line 35398 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_RSVD0_SHIFT

#define PXP_OUT_LRC_RSVD0_SHIFT (14U)

Definition at line 35399 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_RSVD1

#define PXP_OUT_LRC_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_RSVD1_SHIFT)) & PXP_OUT_LRC_RSVD1_MASK)

Definition at line 35406 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_RSVD1_MASK

#define PXP_OUT_LRC_RSVD1_MASK (0xC0000000U)

Definition at line 35404 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_RSVD1_SHIFT

#define PXP_OUT_LRC_RSVD1_SHIFT (30U)

Definition at line 35405 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_X

#define PXP_OUT_LRC_X | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_X_SHIFT)) & PXP_OUT_LRC_X_MASK)

Definition at line 35403 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_X_MASK

#define PXP_OUT_LRC_X_MASK (0x3FFF0000U)

Definition at line 35401 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_X_SHIFT

#define PXP_OUT_LRC_X_SHIFT (16U)

Definition at line 35402 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_Y

#define PXP_OUT_LRC_Y | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_LRC_Y_SHIFT)) & PXP_OUT_LRC_Y_MASK)

Definition at line 35397 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_Y_MASK

#define PXP_OUT_LRC_Y_MASK (0x3FFFU)

Definition at line 35395 of file MIMXRT1062.h.

## ◆ PXP_OUT_LRC_Y_SHIFT

#define PXP_OUT_LRC_Y_SHIFT (0U)

Definition at line 35396 of file MIMXRT1062.h.

## ◆ PXP_OUT_PITCH_PITCH

#define PXP_OUT_PITCH_PITCH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PITCH_PITCH_SHIFT)) & PXP_OUT_PITCH_PITCH_MASK)

Definition at line 35387 of file MIMXRT1062.h.

## ◆ PXP_OUT_PITCH_PITCH_MASK

#define PXP_OUT_PITCH_PITCH_MASK (0xFFFFU)

Definition at line 35385 of file MIMXRT1062.h.

## ◆ PXP_OUT_PITCH_PITCH_SHIFT

#define PXP_OUT_PITCH_PITCH_SHIFT (0U)

Definition at line 35386 of file MIMXRT1062.h.

## ◆ PXP_OUT_PITCH_RSVD

#define PXP_OUT_PITCH_RSVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PITCH_RSVD_SHIFT)) & PXP_OUT_PITCH_RSVD_MASK)

Definition at line 35390 of file MIMXRT1062.h.

## ◆ PXP_OUT_PITCH_RSVD_MASK

#define PXP_OUT_PITCH_RSVD_MASK (0xFFFF0000U)

Definition at line 35388 of file MIMXRT1062.h.

## ◆ PXP_OUT_PITCH_RSVD_SHIFT

#define PXP_OUT_PITCH_RSVD_SHIFT (16U)

Definition at line 35389 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_RSVD0

#define PXP_OUT_PS_LRC_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_RSVD0_SHIFT)) & PXP_OUT_PS_LRC_RSVD0_MASK)

Definition at line 35432 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_RSVD0_MASK

#define PXP_OUT_PS_LRC_RSVD0_MASK (0xC000U)

Definition at line 35430 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_RSVD0_SHIFT

#define PXP_OUT_PS_LRC_RSVD0_SHIFT (14U)

Definition at line 35431 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_RSVD1

#define PXP_OUT_PS_LRC_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_RSVD1_SHIFT)) & PXP_OUT_PS_LRC_RSVD1_MASK)

Definition at line 35438 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_RSVD1_MASK

#define PXP_OUT_PS_LRC_RSVD1_MASK (0xC0000000U)

Definition at line 35436 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_RSVD1_SHIFT

#define PXP_OUT_PS_LRC_RSVD1_SHIFT (30U)

Definition at line 35437 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_X

#define PXP_OUT_PS_LRC_X | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_X_SHIFT)) & PXP_OUT_PS_LRC_X_MASK)

Definition at line 35435 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_X_MASK

#define PXP_OUT_PS_LRC_X_MASK (0x3FFF0000U)

Definition at line 35433 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_X_SHIFT

#define PXP_OUT_PS_LRC_X_SHIFT (16U)

Definition at line 35434 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_Y

#define PXP_OUT_PS_LRC_Y | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_LRC_Y_SHIFT)) & PXP_OUT_PS_LRC_Y_MASK)

Definition at line 35429 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_Y_MASK

#define PXP_OUT_PS_LRC_Y_MASK (0x3FFFU)

Definition at line 35427 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_LRC_Y_SHIFT

#define PXP_OUT_PS_LRC_Y_SHIFT (0U)

Definition at line 35428 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_RSVD0

#define PXP_OUT_PS_ULC_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_RSVD0_SHIFT)) & PXP_OUT_PS_ULC_RSVD0_MASK)

Definition at line 35416 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_RSVD0_MASK

#define PXP_OUT_PS_ULC_RSVD0_MASK (0xC000U)

Definition at line 35414 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_RSVD0_SHIFT

#define PXP_OUT_PS_ULC_RSVD0_SHIFT (14U)

Definition at line 35415 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_RSVD1

#define PXP_OUT_PS_ULC_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_RSVD1_SHIFT)) & PXP_OUT_PS_ULC_RSVD1_MASK)

Definition at line 35422 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_RSVD1_MASK

#define PXP_OUT_PS_ULC_RSVD1_MASK (0xC0000000U)

Definition at line 35420 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_RSVD1_SHIFT

#define PXP_OUT_PS_ULC_RSVD1_SHIFT (30U)

Definition at line 35421 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_X

#define PXP_OUT_PS_ULC_X | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_X_SHIFT)) & PXP_OUT_PS_ULC_X_MASK)

Definition at line 35419 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_X_MASK

#define PXP_OUT_PS_ULC_X_MASK (0x3FFF0000U)

Definition at line 35417 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_X_SHIFT

#define PXP_OUT_PS_ULC_X_SHIFT (16U)

Definition at line 35418 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_Y

#define PXP_OUT_PS_ULC_Y | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_OUT_PS_ULC_Y_SHIFT)) & PXP_OUT_PS_ULC_Y_MASK)

Definition at line 35413 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_Y_MASK

#define PXP_OUT_PS_ULC_Y_MASK (0x3FFFU)

Definition at line 35411 of file MIMXRT1062.h.

## ◆ PXP_OUT_PS_ULC_Y_SHIFT

#define PXP_OUT_PS_ULC_Y_SHIFT (0U)

Definition at line 35412 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE

#define PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_SHIFT)) & PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_MASK)

Definition at line 35952 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_MASK

#define PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_MASK (0x1U)

Definition at line 35950 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_SHIFT

#define PXP_PORTER_DUFF_CTRL_POTER_DUFF_ENABLE_SHIFT (0U)

Definition at line 35951 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE

#define PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_MASK)

Definition at line 35961 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_MASK (0x20U)

Definition at line 35959 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S0_ALPHA_MODE_SHIFT (5U)

Definition at line 35960 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE

#define PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_MASK)

Definition at line 35964 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_MASK (0x40U)

Definition at line 35962 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S0_COLOR_MODE_SHIFT (6U)

Definition at line 35963 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA

#define PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MASK)

Definition at line 35979 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MASK

#define PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MASK (0xFF0000U)

Definition at line 35977 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE

#define PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_MASK)

Definition at line 35958 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_MASK (0x18U)

Definition at line 35956 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_MODE_SHIFT (3U)

Definition at line 35957 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_SHIFT

#define PXP_PORTER_DUFF_CTRL_S0_GLOBAL_ALPHA_SHIFT (16U)

Definition at line 35978 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE

#define PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_MASK)

Definition at line 35955 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_MASK (0x6U)

Definition at line 35953 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S0_S1_FACTOR_MODE_SHIFT (1U)

Definition at line 35954 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE

#define PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_MASK)

Definition at line 35973 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_MASK (0x1000U)

Definition at line 35971 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S1_ALPHA_MODE_SHIFT (12U)

Definition at line 35972 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE

#define PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_MASK)

Definition at line 35976 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_MASK (0x2000U)

Definition at line 35974 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S1_COLOR_MODE_SHIFT (13U)

Definition at line 35975 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA

#define PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MASK)

Definition at line 35982 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MASK

#define PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MASK (0xFF000000U)

Definition at line 35980 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE

#define PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_MASK)

Definition at line 35970 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_MASK (0xC00U)

Definition at line 35968 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_MODE_SHIFT (10U)

Definition at line 35969 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_SHIFT

#define PXP_PORTER_DUFF_CTRL_S1_GLOBAL_ALPHA_SHIFT (24U)

Definition at line 35981 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE

#define PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_SHIFT)) & PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_MASK)

Definition at line 35967 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_MASK

#define PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_MASK (0x300U)

Definition at line 35965 of file MIMXRT1062.h.

## ◆ PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_SHIFT

#define PXP_PORTER_DUFF_CTRL_S1_S0_FACTOR_MODE_SHIFT (8U)

Definition at line 35966 of file MIMXRT1062.h.

## ◆ PXP_POWER_CTRL

#define PXP_POWER_CTRL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_POWER_CTRL_SHIFT)) & PXP_POWER_CTRL_MASK)

Definition at line 35932 of file MIMXRT1062.h.

## ◆ PXP_POWER_CTRL_MASK

#define PXP_POWER_CTRL_MASK (0xFFFFF000U)

Definition at line 35930 of file MIMXRT1062.h.

## ◆ PXP_POWER_CTRL_SHIFT

#define PXP_POWER_CTRL_SHIFT (12U)

Definition at line 35931 of file MIMXRT1062.h.

## ◆ PXP_POWER_ROT_MEM_LP_STATE

#define PXP_POWER_ROT_MEM_LP_STATE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_POWER_ROT_MEM_LP_STATE_SHIFT)) & PXP_POWER_ROT_MEM_LP_STATE_MASK)

ROT_MEM_LP_STATE 0b000..Memory is not in low power state. 0b001..Light Sleep Mode. Low leakage mode, maintain memory contents. 0b010..Deep Sleep Mode. Low leakage mode, maintain memory contents. 0b100..Shut Down Mode. Shut Down periphery and core, no memory retention.

Definition at line 35929 of file MIMXRT1062.h.

## ◆ PXP_POWER_ROT_MEM_LP_STATE_MASK

#define PXP_POWER_ROT_MEM_LP_STATE_MASK (0xE00U)

Definition at line 35921 of file MIMXRT1062.h.

## ◆ PXP_POWER_ROT_MEM_LP_STATE_SHIFT

#define PXP_POWER_ROT_MEM_LP_STATE_SHIFT (9U)

Definition at line 35922 of file MIMXRT1062.h.

## ◆ PXP_PS_BACKGROUND_COLOR

#define PXP_PS_BACKGROUND_COLOR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_BACKGROUND_COLOR_SHIFT)) & PXP_PS_BACKGROUND_COLOR_MASK)

Definition at line 35712 of file MIMXRT1062.h.

## ◆ PXP_PS_BACKGROUND_COLOR_MASK

#define PXP_PS_BACKGROUND_COLOR_MASK (0xFFFFFFU)

Definition at line 35710 of file MIMXRT1062.h.

## ◆ PXP_PS_BACKGROUND_COLOR_SHIFT

#define PXP_PS_BACKGROUND_COLOR_SHIFT (0U)

Definition at line 35711 of file MIMXRT1062.h.

## ◆ PXP_PS_BACKGROUND_RSVD

#define PXP_PS_BACKGROUND_RSVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_BACKGROUND_RSVD_SHIFT)) & PXP_PS_BACKGROUND_RSVD_MASK)

Definition at line 35715 of file MIMXRT1062.h.

## ◆ PXP_PS_BACKGROUND_RSVD_MASK

#define PXP_PS_BACKGROUND_RSVD_MASK (0xFF000000U)

Definition at line 35713 of file MIMXRT1062.h.

## ◆ PXP_PS_BACKGROUND_RSVD_SHIFT

#define PXP_PS_BACKGROUND_RSVD_SHIFT (24U)

Definition at line 35714 of file MIMXRT1062.h.

## ◆ PXP_PS_BUF_ADDR

#define PXP_PS_BUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_BUF_ADDR_SHIFT)) & PXP_PS_BUF_ADDR_MASK)

Definition at line 35681 of file MIMXRT1062.h.

## ◆ PXP_PS_BUF_ADDR_MASK

#define PXP_PS_BUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 35679 of file MIMXRT1062.h.

## ◆ PXP_PS_BUF_ADDR_SHIFT

#define PXP_PS_BUF_ADDR_SHIFT (0U)

Definition at line 35680 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYHIGH_PIXEL

#define PXP_PS_CLRKEYHIGH_PIXEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYHIGH_PIXEL_SHIFT)) & PXP_PS_CLRKEYHIGH_PIXEL_MASK)

Definition at line 35764 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYHIGH_PIXEL_MASK

#define PXP_PS_CLRKEYHIGH_PIXEL_MASK (0xFFFFFFU)

Definition at line 35762 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYHIGH_PIXEL_SHIFT

#define PXP_PS_CLRKEYHIGH_PIXEL_SHIFT (0U)

Definition at line 35763 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYHIGH_RSVD1

#define PXP_PS_CLRKEYHIGH_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYHIGH_RSVD1_SHIFT)) & PXP_PS_CLRKEYHIGH_RSVD1_MASK)

Definition at line 35767 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYHIGH_RSVD1_MASK

#define PXP_PS_CLRKEYHIGH_RSVD1_MASK (0xFF000000U)

Definition at line 35765 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYHIGH_RSVD1_SHIFT

#define PXP_PS_CLRKEYHIGH_RSVD1_SHIFT (24U)

Definition at line 35766 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYLOW_PIXEL

#define PXP_PS_CLRKEYLOW_PIXEL | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYLOW_PIXEL_SHIFT)) & PXP_PS_CLRKEYLOW_PIXEL_MASK)

Definition at line 35754 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYLOW_PIXEL_MASK

#define PXP_PS_CLRKEYLOW_PIXEL_MASK (0xFFFFFFU)

Definition at line 35752 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYLOW_PIXEL_SHIFT

#define PXP_PS_CLRKEYLOW_PIXEL_SHIFT (0U)

Definition at line 35753 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYLOW_RSVD1

#define PXP_PS_CLRKEYLOW_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CLRKEYLOW_RSVD1_SHIFT)) & PXP_PS_CLRKEYLOW_RSVD1_MASK)

Definition at line 35757 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYLOW_RSVD1_MASK

#define PXP_PS_CLRKEYLOW_RSVD1_MASK (0xFF000000U)

Definition at line 35755 of file MIMXRT1062.h.

## ◆ PXP_PS_CLRKEYLOW_RSVD1_SHIFT

#define PXP_PS_CLRKEYLOW_RSVD1_SHIFT (24U)

Definition at line 35756 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_DECX

#define PXP_PS_CTRL_CLR_DECX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_DECX_SHIFT)) & PXP_PS_CTRL_CLR_DECX_MASK)

DECX 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35620 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_DECX_MASK

#define PXP_PS_CTRL_CLR_DECX_MASK (0xC00U)

Definition at line 35612 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_DECX_SHIFT

#define PXP_PS_CTRL_CLR_DECX_SHIFT (10U)

Definition at line 35613 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_DECY

#define PXP_PS_CTRL_CLR_DECY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_DECY_SHIFT)) & PXP_PS_CTRL_CLR_DECY_MASK)

DECY 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35611 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_DECY_MASK

#define PXP_PS_CTRL_CLR_DECY_MASK (0x300U)

Definition at line 35603 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_DECY_SHIFT

#define PXP_PS_CTRL_CLR_DECY_SHIFT (8U)

Definition at line 35604 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_FORMAT

#define PXP_PS_CTRL_CLR_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_FORMAT_SHIFT)) & PXP_PS_CTRL_CLR_FORMAT_MASK)

FORMAT 0b00100..32-bit pixels (unpacked 24-bit format) 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU) 0b11110..16-bit pixels (3-plane format) 0b11111..16-bit pixels (3-plane format)

Definition at line 35596 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_FORMAT_MASK

#define PXP_PS_CTRL_CLR_FORMAT_MASK (0x1FU)

Definition at line 35577 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_FORMAT_SHIFT

#define PXP_PS_CTRL_CLR_FORMAT_SHIFT (0U)

Definition at line 35578 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_RSVD0

#define PXP_PS_CTRL_CLR_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_RSVD0_SHIFT)) & PXP_PS_CTRL_CLR_RSVD0_MASK)

Definition at line 35602 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_RSVD0_MASK

#define PXP_PS_CTRL_CLR_RSVD0_MASK (0xC0U)

Definition at line 35600 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_RSVD0_SHIFT

#define PXP_PS_CTRL_CLR_RSVD0_SHIFT (6U)

Definition at line 35601 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_RSVD1

#define PXP_PS_CTRL_CLR_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_RSVD1_SHIFT)) & PXP_PS_CTRL_CLR_RSVD1_MASK)

Definition at line 35623 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_RSVD1_MASK

#define PXP_PS_CTRL_CLR_RSVD1_MASK (0xFFFFF000U)

Definition at line 35621 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_RSVD1_SHIFT

#define PXP_PS_CTRL_CLR_RSVD1_SHIFT (12U)

Definition at line 35622 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_WB_SWAP

#define PXP_PS_CTRL_CLR_WB_SWAP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_CLR_WB_SWAP_SHIFT)) & PXP_PS_CTRL_CLR_WB_SWAP_MASK)

Definition at line 35599 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_WB_SWAP_MASK

#define PXP_PS_CTRL_CLR_WB_SWAP_MASK (0x20U)

Definition at line 35597 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_CLR_WB_SWAP_SHIFT

#define PXP_PS_CTRL_CLR_WB_SWAP_SHIFT (5U)

Definition at line 35598 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_DECX

#define PXP_PS_CTRL_DECX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_DECX_SHIFT)) & PXP_PS_CTRL_DECX_MASK)

DECX 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35518 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_DECX_MASK

#define PXP_PS_CTRL_DECX_MASK (0xC00U)

Definition at line 35510 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_DECX_SHIFT

#define PXP_PS_CTRL_DECX_SHIFT (10U)

Definition at line 35511 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_DECY

#define PXP_PS_CTRL_DECY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_DECY_SHIFT)) & PXP_PS_CTRL_DECY_MASK)

DECY 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35509 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_DECY_MASK

#define PXP_PS_CTRL_DECY_MASK (0x300U)

Definition at line 35501 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_DECY_SHIFT

#define PXP_PS_CTRL_DECY_SHIFT (8U)

Definition at line 35502 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_FORMAT

#define PXP_PS_CTRL_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_FORMAT_SHIFT)) & PXP_PS_CTRL_FORMAT_MASK)

FORMAT 0b00100..32-bit pixels (unpacked 24-bit format) 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU) 0b11110..16-bit pixels (3-plane format) 0b11111..16-bit pixels (3-plane format)

Definition at line 35494 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_FORMAT_MASK

#define PXP_PS_CTRL_FORMAT_MASK (0x1FU)

Definition at line 35475 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_FORMAT_SHIFT

#define PXP_PS_CTRL_FORMAT_SHIFT (0U)

Definition at line 35476 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_RSVD0

#define PXP_PS_CTRL_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_RSVD0_SHIFT)) & PXP_PS_CTRL_RSVD0_MASK)

Definition at line 35500 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_RSVD0_MASK

#define PXP_PS_CTRL_RSVD0_MASK (0xC0U)

Definition at line 35498 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_RSVD0_SHIFT

#define PXP_PS_CTRL_RSVD0_SHIFT (6U)

Definition at line 35499 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_RSVD1

#define PXP_PS_CTRL_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_RSVD1_SHIFT)) & PXP_PS_CTRL_RSVD1_MASK)

Definition at line 35521 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_RSVD1_MASK

#define PXP_PS_CTRL_RSVD1_MASK (0xFFFFF000U)

Definition at line 35519 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_RSVD1_SHIFT

#define PXP_PS_CTRL_RSVD1_SHIFT (12U)

Definition at line 35520 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_DECX

#define PXP_PS_CTRL_SET_DECX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_DECX_SHIFT)) & PXP_PS_CTRL_SET_DECX_MASK)

DECX 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35569 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_DECX_MASK

#define PXP_PS_CTRL_SET_DECX_MASK (0xC00U)

Definition at line 35561 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_DECX_SHIFT

#define PXP_PS_CTRL_SET_DECX_SHIFT (10U)

Definition at line 35562 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_DECY

#define PXP_PS_CTRL_SET_DECY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_DECY_SHIFT)) & PXP_PS_CTRL_SET_DECY_MASK)

DECY 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35560 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_DECY_MASK

#define PXP_PS_CTRL_SET_DECY_MASK (0x300U)

Definition at line 35552 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_DECY_SHIFT

#define PXP_PS_CTRL_SET_DECY_SHIFT (8U)

Definition at line 35553 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_FORMAT

#define PXP_PS_CTRL_SET_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_FORMAT_SHIFT)) & PXP_PS_CTRL_SET_FORMAT_MASK)

FORMAT 0b00100..32-bit pixels (unpacked 24-bit format) 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU) 0b11110..16-bit pixels (3-plane format) 0b11111..16-bit pixels (3-plane format)

Definition at line 35545 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_FORMAT_MASK

#define PXP_PS_CTRL_SET_FORMAT_MASK (0x1FU)

Definition at line 35526 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_FORMAT_SHIFT

#define PXP_PS_CTRL_SET_FORMAT_SHIFT (0U)

Definition at line 35527 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_RSVD0

#define PXP_PS_CTRL_SET_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_RSVD0_SHIFT)) & PXP_PS_CTRL_SET_RSVD0_MASK)

Definition at line 35551 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_RSVD0_MASK

#define PXP_PS_CTRL_SET_RSVD0_MASK (0xC0U)

Definition at line 35549 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_RSVD0_SHIFT

#define PXP_PS_CTRL_SET_RSVD0_SHIFT (6U)

Definition at line 35550 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_RSVD1

#define PXP_PS_CTRL_SET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_RSVD1_SHIFT)) & PXP_PS_CTRL_SET_RSVD1_MASK)

Definition at line 35572 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_RSVD1_MASK

#define PXP_PS_CTRL_SET_RSVD1_MASK (0xFFFFF000U)

Definition at line 35570 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_RSVD1_SHIFT

#define PXP_PS_CTRL_SET_RSVD1_SHIFT (12U)

Definition at line 35571 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_WB_SWAP

#define PXP_PS_CTRL_SET_WB_SWAP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_SET_WB_SWAP_SHIFT)) & PXP_PS_CTRL_SET_WB_SWAP_MASK)

Definition at line 35548 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_WB_SWAP_MASK

#define PXP_PS_CTRL_SET_WB_SWAP_MASK (0x20U)

Definition at line 35546 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_SET_WB_SWAP_SHIFT

#define PXP_PS_CTRL_SET_WB_SWAP_SHIFT (5U)

Definition at line 35547 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_DECX

#define PXP_PS_CTRL_TOG_DECX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_DECX_SHIFT)) & PXP_PS_CTRL_TOG_DECX_MASK)

DECX 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35671 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_DECX_MASK

#define PXP_PS_CTRL_TOG_DECX_MASK (0xC00U)

Definition at line 35663 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_DECX_SHIFT

#define PXP_PS_CTRL_TOG_DECX_SHIFT (10U)

Definition at line 35664 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_DECY

#define PXP_PS_CTRL_TOG_DECY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_DECY_SHIFT)) & PXP_PS_CTRL_TOG_DECY_MASK)

DECY 0b00..Disable pre-decimation filter. 0b01..Decimate PS by 2. 0b10..Decimate PS by 4. 0b11..Decimate PS by 8.

Definition at line 35662 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_DECY_MASK

#define PXP_PS_CTRL_TOG_DECY_MASK (0x300U)

Definition at line 35654 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_DECY_SHIFT

#define PXP_PS_CTRL_TOG_DECY_SHIFT (8U)

Definition at line 35655 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_FORMAT

#define PXP_PS_CTRL_TOG_FORMAT | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_FORMAT_SHIFT)) & PXP_PS_CTRL_TOG_FORMAT_MASK)

FORMAT 0b00100..32-bit pixels (unpacked 24-bit format) 0b01100..16-bit pixels 0b01101..16-bit pixels 0b01110..16-bit pixels 0b10000..32-bit pixels (1-plane XYUV unpacked) 0b10010..16-bit pixels (1-plane U0,Y0,V0,Y1 interleaved bytes) 0b10011..16-bit pixels (1-plane V0,Y0,U0,Y1 interleaved bytes) 0b10100..8-bit monochrome pixels (1-plane Y luma output) 0b10101..4-bit monochrome pixels (1-plane Y luma, 4 bit truncation) 0b11000..16-bit pixels (2-plane UV interleaved bytes) 0b11001..16-bit pixels (2-plane UV) 0b11010..16-bit pixels (2-plane VU interleaved bytes) 0b11011..16-bit pixels (2-plane VU) 0b11110..16-bit pixels (3-plane format) 0b11111..16-bit pixels (3-plane format)

Definition at line 35647 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_FORMAT_MASK

#define PXP_PS_CTRL_TOG_FORMAT_MASK (0x1FU)

Definition at line 35628 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_FORMAT_SHIFT

#define PXP_PS_CTRL_TOG_FORMAT_SHIFT (0U)

Definition at line 35629 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_RSVD0

#define PXP_PS_CTRL_TOG_RSVD0 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_RSVD0_SHIFT)) & PXP_PS_CTRL_TOG_RSVD0_MASK)

Definition at line 35653 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_RSVD0_MASK

#define PXP_PS_CTRL_TOG_RSVD0_MASK (0xC0U)

Definition at line 35651 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_RSVD0_SHIFT

#define PXP_PS_CTRL_TOG_RSVD0_SHIFT (6U)

Definition at line 35652 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_RSVD1

#define PXP_PS_CTRL_TOG_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_RSVD1_SHIFT)) & PXP_PS_CTRL_TOG_RSVD1_MASK)

Definition at line 35674 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_RSVD1_MASK

#define PXP_PS_CTRL_TOG_RSVD1_MASK (0xFFFFF000U)

Definition at line 35672 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_RSVD1_SHIFT

#define PXP_PS_CTRL_TOG_RSVD1_SHIFT (12U)

Definition at line 35673 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_WB_SWAP

#define PXP_PS_CTRL_TOG_WB_SWAP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_TOG_WB_SWAP_SHIFT)) & PXP_PS_CTRL_TOG_WB_SWAP_MASK)

Definition at line 35650 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_WB_SWAP_MASK

#define PXP_PS_CTRL_TOG_WB_SWAP_MASK (0x20U)

Definition at line 35648 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_TOG_WB_SWAP_SHIFT

#define PXP_PS_CTRL_TOG_WB_SWAP_SHIFT (5U)

Definition at line 35649 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_WB_SWAP

#define PXP_PS_CTRL_WB_SWAP | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_CTRL_WB_SWAP_SHIFT)) & PXP_PS_CTRL_WB_SWAP_MASK)

Definition at line 35497 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_WB_SWAP_MASK

#define PXP_PS_CTRL_WB_SWAP_MASK (0x20U)

Definition at line 35495 of file MIMXRT1062.h.

## ◆ PXP_PS_CTRL_WB_SWAP_SHIFT

#define PXP_PS_CTRL_WB_SWAP_SHIFT (5U)

Definition at line 35496 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_RSVD1

#define PXP_PS_OFFSET_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_RSVD1_SHIFT)) & PXP_PS_OFFSET_RSVD1_MASK)

Definition at line 35741 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_RSVD1_MASK

#define PXP_PS_OFFSET_RSVD1_MASK (0xF000U)

Definition at line 35739 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_RSVD1_SHIFT

#define PXP_PS_OFFSET_RSVD1_SHIFT (12U)

Definition at line 35740 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_RSVD2

#define PXP_PS_OFFSET_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_RSVD2_SHIFT)) & PXP_PS_OFFSET_RSVD2_MASK)

Definition at line 35747 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_RSVD2_MASK

#define PXP_PS_OFFSET_RSVD2_MASK (0xF0000000U)

Definition at line 35745 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_RSVD2_SHIFT

#define PXP_PS_OFFSET_RSVD2_SHIFT (28U)

Definition at line 35746 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_XOFFSET

#define PXP_PS_OFFSET_XOFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_XOFFSET_SHIFT)) & PXP_PS_OFFSET_XOFFSET_MASK)

Definition at line 35738 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_XOFFSET_MASK

#define PXP_PS_OFFSET_XOFFSET_MASK (0xFFFU)

Definition at line 35736 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_XOFFSET_SHIFT

#define PXP_PS_OFFSET_XOFFSET_SHIFT (0U)

Definition at line 35737 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_YOFFSET

#define PXP_PS_OFFSET_YOFFSET | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_OFFSET_YOFFSET_SHIFT)) & PXP_PS_OFFSET_YOFFSET_MASK)

Definition at line 35744 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_YOFFSET_MASK

#define PXP_PS_OFFSET_YOFFSET_MASK (0xFFF0000U)

Definition at line 35742 of file MIMXRT1062.h.

## ◆ PXP_PS_OFFSET_YOFFSET_SHIFT

#define PXP_PS_OFFSET_YOFFSET_SHIFT (16U)

Definition at line 35743 of file MIMXRT1062.h.

## ◆ PXP_PS_PITCH_PITCH

#define PXP_PS_PITCH_PITCH | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_PITCH_PITCH_SHIFT)) & PXP_PS_PITCH_PITCH_MASK)

Definition at line 35702 of file MIMXRT1062.h.

## ◆ PXP_PS_PITCH_PITCH_MASK

#define PXP_PS_PITCH_PITCH_MASK (0xFFFFU)

Definition at line 35700 of file MIMXRT1062.h.

## ◆ PXP_PS_PITCH_PITCH_SHIFT

#define PXP_PS_PITCH_PITCH_SHIFT (0U)

Definition at line 35701 of file MIMXRT1062.h.

## ◆ PXP_PS_PITCH_RSVD

#define PXP_PS_PITCH_RSVD | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_PITCH_RSVD_SHIFT)) & PXP_PS_PITCH_RSVD_MASK)

Definition at line 35705 of file MIMXRT1062.h.

## ◆ PXP_PS_PITCH_RSVD_MASK

#define PXP_PS_PITCH_RSVD_MASK (0xFFFF0000U)

Definition at line 35703 of file MIMXRT1062.h.

## ◆ PXP_PS_PITCH_RSVD_SHIFT

#define PXP_PS_PITCH_RSVD_SHIFT (16U)

Definition at line 35704 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_RSVD1

#define PXP_PS_SCALE_RSVD1 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_RSVD1_SHIFT)) & PXP_PS_SCALE_RSVD1_MASK)

Definition at line 35725 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_RSVD1_MASK

#define PXP_PS_SCALE_RSVD1_MASK (0x8000U)

Definition at line 35723 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_RSVD1_SHIFT

#define PXP_PS_SCALE_RSVD1_SHIFT (15U)

Definition at line 35724 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_RSVD2

#define PXP_PS_SCALE_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_RSVD2_SHIFT)) & PXP_PS_SCALE_RSVD2_MASK)

Definition at line 35731 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_RSVD2_MASK

#define PXP_PS_SCALE_RSVD2_MASK (0x80000000U)

Definition at line 35729 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_RSVD2_SHIFT

#define PXP_PS_SCALE_RSVD2_SHIFT (31U)

Definition at line 35730 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_XSCALE

#define PXP_PS_SCALE_XSCALE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_XSCALE_SHIFT)) & PXP_PS_SCALE_XSCALE_MASK)

Definition at line 35722 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_XSCALE_MASK

#define PXP_PS_SCALE_XSCALE_MASK (0x7FFFU)

Definition at line 35720 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_XSCALE_SHIFT

#define PXP_PS_SCALE_XSCALE_SHIFT (0U)

Definition at line 35721 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_YSCALE

#define PXP_PS_SCALE_YSCALE | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_SCALE_YSCALE_SHIFT)) & PXP_PS_SCALE_YSCALE_MASK)

Definition at line 35728 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_YSCALE_MASK

#define PXP_PS_SCALE_YSCALE_MASK (0x7FFF0000U)

Definition at line 35726 of file MIMXRT1062.h.

## ◆ PXP_PS_SCALE_YSCALE_SHIFT

#define PXP_PS_SCALE_YSCALE_SHIFT (16U)

Definition at line 35727 of file MIMXRT1062.h.

## ◆ PXP_PS_UBUF_ADDR

#define PXP_PS_UBUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_UBUF_ADDR_SHIFT)) & PXP_PS_UBUF_ADDR_MASK)

Definition at line 35688 of file MIMXRT1062.h.

## ◆ PXP_PS_UBUF_ADDR_MASK

#define PXP_PS_UBUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 35686 of file MIMXRT1062.h.

## ◆ PXP_PS_UBUF_ADDR_SHIFT

#define PXP_PS_UBUF_ADDR_SHIFT (0U)

Definition at line 35687 of file MIMXRT1062.h.

## ◆ PXP_PS_VBUF_ADDR

#define PXP_PS_VBUF_ADDR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_PS_VBUF_ADDR_SHIFT)) & PXP_PS_VBUF_ADDR_MASK)

Definition at line 35695 of file MIMXRT1062.h.

## ◆ PXP_PS_VBUF_ADDR_MASK

#define PXP_PS_VBUF_ADDR_MASK (0xFFFFFFFFU)

Definition at line 35693 of file MIMXRT1062.h.

## ◆ PXP_PS_VBUF_ADDR_SHIFT

#define PXP_PS_VBUF_ADDR_SHIFT (0U)

Definition at line 35694 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_ERROR_ID

#define PXP_STAT_AXI_ERROR_ID | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_AXI_ERROR_ID_SHIFT)) & PXP_STAT_AXI_ERROR_ID_MASK)

Definition at line 35073 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_ERROR_ID_MASK

#define PXP_STAT_AXI_ERROR_ID_MASK (0xF0U)

Definition at line 35071 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_ERROR_ID_SHIFT

#define PXP_STAT_AXI_ERROR_ID_SHIFT (4U)

Definition at line 35072 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_READ_ERROR

#define PXP_STAT_AXI_READ_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_AXI_READ_ERROR_SHIFT)) & PXP_STAT_AXI_READ_ERROR_MASK)

Definition at line 35067 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_READ_ERROR_MASK

#define PXP_STAT_AXI_READ_ERROR_MASK (0x4U)

Definition at line 35065 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_READ_ERROR_SHIFT

#define PXP_STAT_AXI_READ_ERROR_SHIFT (2U)

Definition at line 35066 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_WRITE_ERROR

#define PXP_STAT_AXI_WRITE_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_AXI_WRITE_ERROR_MASK)

Definition at line 35064 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_WRITE_ERROR_MASK

#define PXP_STAT_AXI_WRITE_ERROR_MASK (0x2U)

Definition at line 35062 of file MIMXRT1062.h.

## ◆ PXP_STAT_AXI_WRITE_ERROR_SHIFT

#define PXP_STAT_AXI_WRITE_ERROR_SHIFT (1U)

Definition at line 35063 of file MIMXRT1062.h.

## ◆ PXP_STAT_BLOCKX

#define PXP_STAT_BLOCKX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_BLOCKX_SHIFT)) & PXP_STAT_BLOCKX_MASK)

Definition at line 35085 of file MIMXRT1062.h.

## ◆ PXP_STAT_BLOCKX_MASK

#define PXP_STAT_BLOCKX_MASK (0xFF000000U)

Definition at line 35083 of file MIMXRT1062.h.

## ◆ PXP_STAT_BLOCKX_SHIFT

#define PXP_STAT_BLOCKX_SHIFT (24U)

Definition at line 35084 of file MIMXRT1062.h.

## ◆ PXP_STAT_BLOCKY

#define PXP_STAT_BLOCKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_BLOCKY_SHIFT)) & PXP_STAT_BLOCKY_MASK)

Definition at line 35082 of file MIMXRT1062.h.

## ◆ PXP_STAT_BLOCKY_MASK

#define PXP_STAT_BLOCKY_MASK (0xFF0000U)

Definition at line 35080 of file MIMXRT1062.h.

## ◆ PXP_STAT_BLOCKY_SHIFT

#define PXP_STAT_BLOCKY_SHIFT (16U)

Definition at line 35081 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_ERROR_ID

#define PXP_STAT_CLR_AXI_ERROR_ID | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_AXI_ERROR_ID_SHIFT)) & PXP_STAT_CLR_AXI_ERROR_ID_MASK)

Definition at line 35135 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_ERROR_ID_MASK

#define PXP_STAT_CLR_AXI_ERROR_ID_MASK (0xF0U)

Definition at line 35133 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_ERROR_ID_SHIFT

#define PXP_STAT_CLR_AXI_ERROR_ID_SHIFT (4U)

Definition at line 35134 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_READ_ERROR

#define PXP_STAT_CLR_AXI_READ_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_AXI_READ_ERROR_SHIFT)) & PXP_STAT_CLR_AXI_READ_ERROR_MASK)

Definition at line 35129 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_READ_ERROR_MASK

#define PXP_STAT_CLR_AXI_READ_ERROR_MASK (0x4U)

Definition at line 35127 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_READ_ERROR_SHIFT

#define PXP_STAT_CLR_AXI_READ_ERROR_SHIFT (2U)

Definition at line 35128 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_WRITE_ERROR

#define PXP_STAT_CLR_AXI_WRITE_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_CLR_AXI_WRITE_ERROR_MASK)

Definition at line 35126 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_WRITE_ERROR_MASK

#define PXP_STAT_CLR_AXI_WRITE_ERROR_MASK (0x2U)

Definition at line 35124 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_AXI_WRITE_ERROR_SHIFT

#define PXP_STAT_CLR_AXI_WRITE_ERROR_SHIFT (1U)

Definition at line 35125 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_BLOCKX

#define PXP_STAT_CLR_BLOCKX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_BLOCKX_SHIFT)) & PXP_STAT_CLR_BLOCKX_MASK)

Definition at line 35147 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_BLOCKX_MASK

#define PXP_STAT_CLR_BLOCKX_MASK (0xFF000000U)

Definition at line 35145 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_BLOCKX_SHIFT

#define PXP_STAT_CLR_BLOCKX_SHIFT (24U)

Definition at line 35146 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_BLOCKY

#define PXP_STAT_CLR_BLOCKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_BLOCKY_SHIFT)) & PXP_STAT_CLR_BLOCKY_MASK)

Definition at line 35144 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_BLOCKY_MASK

#define PXP_STAT_CLR_BLOCKY_MASK (0xFF0000U)

Definition at line 35142 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_BLOCKY_SHIFT

#define PXP_STAT_CLR_BLOCKY_SHIFT (16U)

Definition at line 35143 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_IRQ

#define PXP_STAT_CLR_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_IRQ_SHIFT)) & PXP_STAT_CLR_IRQ_MASK)

Definition at line 35123 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_IRQ_MASK

#define PXP_STAT_CLR_IRQ_MASK (0x1U)

Definition at line 35121 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_IRQ_SHIFT

#define PXP_STAT_CLR_IRQ_SHIFT (0U)

Definition at line 35122 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ

#define PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_MASK)

Definition at line 35138 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_MASK

#define PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)

Definition at line 35136 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_SHIFT

#define PXP_STAT_CLR_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)

Definition at line 35137 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_NEXT_IRQ

#define PXP_STAT_CLR_NEXT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_NEXT_IRQ_SHIFT)) & PXP_STAT_CLR_NEXT_IRQ_MASK)

Definition at line 35132 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_NEXT_IRQ_MASK

#define PXP_STAT_CLR_NEXT_IRQ_MASK (0x8U)

Definition at line 35130 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_NEXT_IRQ_SHIFT

#define PXP_STAT_CLR_NEXT_IRQ_SHIFT (3U)

Definition at line 35131 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_RSVD2

#define PXP_STAT_CLR_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_CLR_RSVD2_SHIFT)) & PXP_STAT_CLR_RSVD2_MASK)

Definition at line 35141 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_RSVD2_MASK

#define PXP_STAT_CLR_RSVD2_MASK (0xFE00U)

Definition at line 35139 of file MIMXRT1062.h.

## ◆ PXP_STAT_CLR_RSVD2_SHIFT

#define PXP_STAT_CLR_RSVD2_SHIFT (9U)

Definition at line 35140 of file MIMXRT1062.h.

## ◆ PXP_STAT_IRQ

#define PXP_STAT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_IRQ_SHIFT)) & PXP_STAT_IRQ_MASK)

Definition at line 35061 of file MIMXRT1062.h.

## ◆ PXP_STAT_IRQ_MASK

#define PXP_STAT_IRQ_MASK (0x1U)

Definition at line 35059 of file MIMXRT1062.h.

## ◆ PXP_STAT_IRQ_SHIFT

#define PXP_STAT_IRQ_SHIFT (0U)

Definition at line 35060 of file MIMXRT1062.h.

## ◆ PXP_STAT_LUT_DMA_LOAD_DONE_IRQ

#define PXP_STAT_LUT_DMA_LOAD_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_MASK)

Definition at line 35076 of file MIMXRT1062.h.

## ◆ PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_MASK

#define PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)

Definition at line 35074 of file MIMXRT1062.h.

## ◆ PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_SHIFT

#define PXP_STAT_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)

Definition at line 35075 of file MIMXRT1062.h.

## ◆ PXP_STAT_NEXT_IRQ

#define PXP_STAT_NEXT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_NEXT_IRQ_SHIFT)) & PXP_STAT_NEXT_IRQ_MASK)

Definition at line 35070 of file MIMXRT1062.h.

## ◆ PXP_STAT_NEXT_IRQ_MASK

#define PXP_STAT_NEXT_IRQ_MASK (0x8U)

Definition at line 35068 of file MIMXRT1062.h.

## ◆ PXP_STAT_NEXT_IRQ_SHIFT

#define PXP_STAT_NEXT_IRQ_SHIFT (3U)

Definition at line 35069 of file MIMXRT1062.h.

## ◆ PXP_STAT_RSVD2

#define PXP_STAT_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_RSVD2_SHIFT)) & PXP_STAT_RSVD2_MASK)

Definition at line 35079 of file MIMXRT1062.h.

## ◆ PXP_STAT_RSVD2_MASK

#define PXP_STAT_RSVD2_MASK (0xFE00U)

Definition at line 35077 of file MIMXRT1062.h.

## ◆ PXP_STAT_RSVD2_SHIFT

#define PXP_STAT_RSVD2_SHIFT (9U)

Definition at line 35078 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_ERROR_ID

#define PXP_STAT_SET_AXI_ERROR_ID | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_AXI_ERROR_ID_SHIFT)) & PXP_STAT_SET_AXI_ERROR_ID_MASK)

Definition at line 35104 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_ERROR_ID_MASK

#define PXP_STAT_SET_AXI_ERROR_ID_MASK (0xF0U)

Definition at line 35102 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_ERROR_ID_SHIFT

#define PXP_STAT_SET_AXI_ERROR_ID_SHIFT (4U)

Definition at line 35103 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_READ_ERROR

#define PXP_STAT_SET_AXI_READ_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_AXI_READ_ERROR_SHIFT)) & PXP_STAT_SET_AXI_READ_ERROR_MASK)

Definition at line 35098 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_READ_ERROR_MASK

#define PXP_STAT_SET_AXI_READ_ERROR_MASK (0x4U)

Definition at line 35096 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_READ_ERROR_SHIFT

#define PXP_STAT_SET_AXI_READ_ERROR_SHIFT (2U)

Definition at line 35097 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_WRITE_ERROR

#define PXP_STAT_SET_AXI_WRITE_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_SET_AXI_WRITE_ERROR_MASK)

Definition at line 35095 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_WRITE_ERROR_MASK

#define PXP_STAT_SET_AXI_WRITE_ERROR_MASK (0x2U)

Definition at line 35093 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_AXI_WRITE_ERROR_SHIFT

#define PXP_STAT_SET_AXI_WRITE_ERROR_SHIFT (1U)

Definition at line 35094 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_BLOCKX

#define PXP_STAT_SET_BLOCKX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_BLOCKX_SHIFT)) & PXP_STAT_SET_BLOCKX_MASK)

Definition at line 35116 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_BLOCKX_MASK

#define PXP_STAT_SET_BLOCKX_MASK (0xFF000000U)

Definition at line 35114 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_BLOCKX_SHIFT

#define PXP_STAT_SET_BLOCKX_SHIFT (24U)

Definition at line 35115 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_BLOCKY

#define PXP_STAT_SET_BLOCKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_BLOCKY_SHIFT)) & PXP_STAT_SET_BLOCKY_MASK)

Definition at line 35113 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_BLOCKY_MASK

#define PXP_STAT_SET_BLOCKY_MASK (0xFF0000U)

Definition at line 35111 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_BLOCKY_SHIFT

#define PXP_STAT_SET_BLOCKY_SHIFT (16U)

Definition at line 35112 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_IRQ

#define PXP_STAT_SET_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_IRQ_SHIFT)) & PXP_STAT_SET_IRQ_MASK)

Definition at line 35092 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_IRQ_MASK

#define PXP_STAT_SET_IRQ_MASK (0x1U)

Definition at line 35090 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_IRQ_SHIFT

#define PXP_STAT_SET_IRQ_SHIFT (0U)

Definition at line 35091 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ

#define PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_MASK)

Definition at line 35107 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_MASK

#define PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)

Definition at line 35105 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_SHIFT

#define PXP_STAT_SET_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)

Definition at line 35106 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_NEXT_IRQ

#define PXP_STAT_SET_NEXT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_NEXT_IRQ_SHIFT)) & PXP_STAT_SET_NEXT_IRQ_MASK)

Definition at line 35101 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_NEXT_IRQ_MASK

#define PXP_STAT_SET_NEXT_IRQ_MASK (0x8U)

Definition at line 35099 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_NEXT_IRQ_SHIFT

#define PXP_STAT_SET_NEXT_IRQ_SHIFT (3U)

Definition at line 35100 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_RSVD2

#define PXP_STAT_SET_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_SET_RSVD2_SHIFT)) & PXP_STAT_SET_RSVD2_MASK)

Definition at line 35110 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_RSVD2_MASK

#define PXP_STAT_SET_RSVD2_MASK (0xFE00U)

Definition at line 35108 of file MIMXRT1062.h.

## ◆ PXP_STAT_SET_RSVD2_SHIFT

#define PXP_STAT_SET_RSVD2_SHIFT (9U)

Definition at line 35109 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_ERROR_ID

#define PXP_STAT_TOG_AXI_ERROR_ID | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_AXI_ERROR_ID_SHIFT)) & PXP_STAT_TOG_AXI_ERROR_ID_MASK)

Definition at line 35166 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_ERROR_ID_MASK

#define PXP_STAT_TOG_AXI_ERROR_ID_MASK (0xF0U)

Definition at line 35164 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_ERROR_ID_SHIFT

#define PXP_STAT_TOG_AXI_ERROR_ID_SHIFT (4U)

Definition at line 35165 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_READ_ERROR

#define PXP_STAT_TOG_AXI_READ_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_AXI_READ_ERROR_SHIFT)) & PXP_STAT_TOG_AXI_READ_ERROR_MASK)

Definition at line 35160 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_READ_ERROR_MASK

#define PXP_STAT_TOG_AXI_READ_ERROR_MASK (0x4U)

Definition at line 35158 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_READ_ERROR_SHIFT

#define PXP_STAT_TOG_AXI_READ_ERROR_SHIFT (2U)

Definition at line 35159 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_WRITE_ERROR

#define PXP_STAT_TOG_AXI_WRITE_ERROR | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_AXI_WRITE_ERROR_SHIFT)) & PXP_STAT_TOG_AXI_WRITE_ERROR_MASK)

Definition at line 35157 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_WRITE_ERROR_MASK

#define PXP_STAT_TOG_AXI_WRITE_ERROR_MASK (0x2U)

Definition at line 35155 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_AXI_WRITE_ERROR_SHIFT

#define PXP_STAT_TOG_AXI_WRITE_ERROR_SHIFT (1U)

Definition at line 35156 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_BLOCKX

#define PXP_STAT_TOG_BLOCKX | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_BLOCKX_SHIFT)) & PXP_STAT_TOG_BLOCKX_MASK)

Definition at line 35178 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_BLOCKX_MASK

#define PXP_STAT_TOG_BLOCKX_MASK (0xFF000000U)

Definition at line 35176 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_BLOCKX_SHIFT

#define PXP_STAT_TOG_BLOCKX_SHIFT (24U)

Definition at line 35177 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_BLOCKY

#define PXP_STAT_TOG_BLOCKY | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_BLOCKY_SHIFT)) & PXP_STAT_TOG_BLOCKY_MASK)

Definition at line 35175 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_BLOCKY_MASK

#define PXP_STAT_TOG_BLOCKY_MASK (0xFF0000U)

Definition at line 35173 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_BLOCKY_SHIFT

#define PXP_STAT_TOG_BLOCKY_SHIFT (16U)

Definition at line 35174 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_IRQ

#define PXP_STAT_TOG_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_IRQ_SHIFT)) & PXP_STAT_TOG_IRQ_MASK)

Definition at line 35154 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_IRQ_MASK

#define PXP_STAT_TOG_IRQ_MASK (0x1U)

Definition at line 35152 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_IRQ_SHIFT

#define PXP_STAT_TOG_IRQ_SHIFT (0U)

Definition at line 35153 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ

#define PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_SHIFT)) & PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_MASK)

Definition at line 35169 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_MASK

#define PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_MASK (0x100U)

Definition at line 35167 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_SHIFT

#define PXP_STAT_TOG_LUT_DMA_LOAD_DONE_IRQ_SHIFT (8U)

Definition at line 35168 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_NEXT_IRQ

#define PXP_STAT_TOG_NEXT_IRQ | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_NEXT_IRQ_SHIFT)) & PXP_STAT_TOG_NEXT_IRQ_MASK)

Definition at line 35163 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_NEXT_IRQ_MASK

#define PXP_STAT_TOG_NEXT_IRQ_MASK (0x8U)

Definition at line 35161 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_NEXT_IRQ_SHIFT

#define PXP_STAT_TOG_NEXT_IRQ_SHIFT (3U)

Definition at line 35162 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_RSVD2

#define PXP_STAT_TOG_RSVD2 | ( |  | x | ) | (((uint32_t)(((uint32_t)(x)) << PXP_STAT_TOG_RSVD2_SHIFT)) & PXP_STAT_TOG_RSVD2_MASK)

Definition at line 35172 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_RSVD2_MASK

#define PXP_STAT_TOG_RSVD2_MASK (0xFE00U)

Definition at line 35170 of file MIMXRT1062.h.

## ◆ PXP_STAT_TOG_RSVD2_SHIFT

#define PXP_STAT_TOG_RSVD2_SHIFT (9U)

Definition at line 35171 of file MIMXRT1062.h.