Callisto4Bootloader: serialNOR_t Struct Reference

Callisto4Bootloader

Data Fields
serialNOR_t Struct Reference

Serial NOR configuration block Contains FlexSPIheader common block and NOR specific configuration. More...

`#include <bootloader_types.h>`

## Data Fields

FlexSPI_Header_t | memCfg
uint32_t | pageSize
uint32_t | sectorSize
uint32_t | ipCmdSerialClkFreq
| Chip specific value, not used by ROM 0 – No change, keep current serial clock unchanged 1 – 30 MHz 2 – 50 MHz 3 – 60 MHz 4 – 75 MHz 5 – 80 MHz 6 – 100 MHz 7 – 120 MHz 8 – 133 MHz 9 – 166 MHz. More...
uint8_t | reserved [52]

## Detailed Description

Serial NOR configuration block Contains FlexSPIheader common block and NOR specific configuration.

Definition at line 150 of file bootloader_types.h.

## Field Documentation

## ◆ ipCmdSerialClkFreq

uint32_t serialNOR_t::ipCmdSerialClkFreq

Chip specific value, not used by ROM 0 – No change, keep current serial clock unchanged 1 – 30 MHz 2 – 50 MHz 3 – 60 MHz 4 – 75 MHz 5 – 80 MHz 6 – 100 MHz 7 – 120 MHz 8 – 133 MHz 9 – 166 MHz.

Definition at line 155 of file bootloader_types.h.

## ◆ memCfg

FlexSPI_Header_t serialNOR_t::memCfg

Common header.

Definition at line 152 of file bootloader_types.h.

## ◆ pageSize

uint32_t serialNOR_t::pageSize

Page size in terms of bytes, not used by ROM.

Definition at line 153 of file bootloader_types.h.

## ◆ reserved

uint8_t serialNOR_t::reserved[52]

Reserved for future use.

Definition at line 166 of file bootloader_types.h.

## ◆ sectorSize

uint32_t serialNOR_t::sectorSize

Sector size in terms of bytes, not used by ROM.

Definition at line 154 of file bootloader_types.h.

The documentation for this struct was generated from the following file:

- src/bootloader_types.h