Callisto4Bootloader: TRNG_Type Struct Reference

Callisto4Bootloader

Data Fields
TRNG_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » TRNG Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | MCTL
__IO uint32_t | SCMISC
__IO uint32_t | PKRRNG
union {
__IO uint32_t TRNG_Type::PKRMAX
__I uint32_t TRNG_Type::PKRSQ
}; |
__IO uint32_t | SDCTL
union {
__IO uint32_t TRNG_Type::SBLIM
__I uint32_t TRNG_Type::TOTSAM
}; |
__IO uint32_t | FRQMIN
union {
__I uint32_t TRNG_Type::FRQCNT
__IO uint32_t TRNG_Type::FRQMAX
}; |
union {
__I uint32_t TRNG_Type::SCMC
__IO uint32_t TRNG_Type::SCML
}; |
union {
__I uint32_t TRNG_Type::SCR1C
__IO uint32_t TRNG_Type::SCR1L
}; |
union {
__I uint32_t TRNG_Type::SCR2C
__IO uint32_t TRNG_Type::SCR2L
}; |
union {
__I uint32_t TRNG_Type::SCR3C
__IO uint32_t TRNG_Type::SCR3L
}; |
union {
__I uint32_t TRNG_Type::SCR4C
__IO uint32_t TRNG_Type::SCR4L
}; |
union {
__I uint32_t TRNG_Type::SCR5C
__IO uint32_t TRNG_Type::SCR5L
}; |
union {
__I uint32_t TRNG_Type::SCR6PC
__IO uint32_t TRNG_Type::SCR6PL
}; |
__I uint32_t | STATUS
__I uint32_t | ENT [16]
__I uint32_t | PKRCNT10
__I uint32_t | PKRCNT32
__I uint32_t | PKRCNT54
__I uint32_t | PKRCNT76
__I uint32_t | PKRCNT98
__I uint32_t | PKRCNTBA
__I uint32_t | PKRCNTDC
__I uint32_t | PKRCNTFE
__IO uint32_t | SEC_CFG
__IO uint32_t | INT_CTRL
__IO uint32_t | INT_MASK
__I uint32_t | INT_STATUS
uint8_t | RESERVED_0 [64]
__I uint32_t | VID1
__I uint32_t | VID2

## Detailed Description

TRNG - Register Layout Typedef

Definition at line 40259 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h