Callisto4Bootloader: CCM Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
CCM Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| CCM Register Masks

## Data Structures

struct | CCM_Type

## Macros

#define | CCM_BASE (0x400FC000u)
#define | CCM ((CCM_Type *)CCM_BASE)
#define | CCM_BASE_ADDRS { CCM_BASE }
#define | CCM_BASE_PTRS { CCM }
#define | CCM_IRQS { CCM_1_IRQn, CCM_2_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ CCM

#define CCM ((CCM_Type *)CCM_BASE)

Peripheral CCM base pointer

Definition at line 7229 of file MIMXRT1062.h.

## ◆ CCM_BASE

#define CCM_BASE (0x400FC000u)

Peripheral CCM base address

Definition at line 7227 of file MIMXRT1062.h.

## ◆ CCM_BASE_ADDRS

#define CCM_BASE_ADDRS { CCM_BASE }

Array initializer of CCM peripheral base addresses

Definition at line 7231 of file MIMXRT1062.h.

## ◆ CCM_BASE_PTRS

#define CCM_BASE_PTRS { CCM }

Array initializer of CCM peripheral base pointers

Definition at line 7233 of file MIMXRT1062.h.

## ◆ CCM_IRQS

#define CCM_IRQS { CCM_1_IRQn, CCM_2_IRQn }

Interrupt vectors for the CCM peripheral type

Definition at line 7235 of file MIMXRT1062.h.