Callisto4Bootloader: device/MIMXRT1062_features.h File Reference

Callisto4Bootloader

Macros
MIMXRT1062_features.h File Reference

Go to the source code of this file.

## Macros

#define | FSL_FEATURE_SOC_ADC_COUNT (2)
#define | FSL_FEATURE_SOC_AIPSTZ_COUNT (4)
#define | FSL_FEATURE_SOC_AOI_COUNT (2)
#define | FSL_FEATURE_SOC_CCM_COUNT (1)
#define | FSL_FEATURE_SOC_CCM_ANALOG_COUNT (1)
#define | FSL_FEATURE_SOC_CMP_COUNT (4)
#define | FSL_FEATURE_SOC_CSI_COUNT (1)
#define | FSL_FEATURE_SOC_DCDC_COUNT (1)
#define | FSL_FEATURE_SOC_DCP_COUNT (1)
#define | FSL_FEATURE_SOC_DMAMUX_COUNT (1)
#define | FSL_FEATURE_SOC_EDMA_COUNT (1)
#define | FSL_FEATURE_SOC_ENC_COUNT (4)
#define | FSL_FEATURE_SOC_ENET_COUNT (2)
#define | FSL_FEATURE_SOC_EWM_COUNT (1)
#define | FSL_FEATURE_SOC_FLEXCAN_COUNT (3)
#define | FSL_FEATURE_SOC_FLEXIO_COUNT (3)
#define | FSL_FEATURE_SOC_FLEXRAM_COUNT (1)
#define | FSL_FEATURE_SOC_FLEXSPI_COUNT (2)
#define | FSL_FEATURE_SOC_GPC_COUNT (1)
#define | FSL_FEATURE_SOC_GPT_COUNT (2)
#define | FSL_FEATURE_SOC_I2S_COUNT (3)
#define | FSL_FEATURE_SOC_IGPIO_COUNT (9)
#define | FSL_FEATURE_SOC_IOMUXC_COUNT (1)
#define | FSL_FEATURE_SOC_IOMUXC_GPR_COUNT (1)
#define | FSL_FEATURE_SOC_IOMUXC_SNVS_COUNT (1)
#define | FSL_FEATURE_SOC_KPP_COUNT (1)
#define | FSL_FEATURE_SOC_LCDIF_COUNT (1)
#define | FSL_FEATURE_SOC_LPI2C_COUNT (4)
#define | FSL_FEATURE_SOC_LPSPI_COUNT (4)
#define | FSL_FEATURE_SOC_LPUART_COUNT (8)
#define | FSL_FEATURE_SOC_OCOTP_COUNT (1)
#define | FSL_FEATURE_SOC_PIT_COUNT (1)
#define | FSL_FEATURE_SOC_PMU_COUNT (1)
#define | FSL_FEATURE_SOC_PWM_COUNT (4)
#define | FSL_FEATURE_SOC_PXP_COUNT (1)
#define | FSL_FEATURE_SOC_ROMC_COUNT (1)
#define | FSL_FEATURE_SOC_SEMC_COUNT (1)
#define | FSL_FEATURE_SOC_SNVS_COUNT (1)
#define | FSL_FEATURE_SOC_SPDIF_COUNT (1)
#define | FSL_FEATURE_SOC_SRC_COUNT (1)
#define | FSL_FEATURE_SOC_TEMPMON_COUNT (1)
#define | FSL_FEATURE_SOC_TMR_COUNT (4)
#define | FSL_FEATURE_SOC_TRNG_COUNT (1)
#define | FSL_FEATURE_SOC_TSC_COUNT (1)
#define | FSL_FEATURE_SOC_USBHS_COUNT (2)
#define | FSL_FEATURE_SOC_USBNC_COUNT (2)
#define | FSL_FEATURE_SOC_USBPHY_COUNT (2)
#define | FSL_FEATURE_SOC_USB_ANALOG_COUNT (1)
#define | FSL_FEATURE_SOC_USDHC_COUNT (2)
#define | FSL_FEATURE_SOC_WDOG_COUNT (2)
#define | FSL_FEATURE_SOC_XBARA_COUNT (1)
#define | FSL_FEATURE_SOC_XBARB_COUNT (2)
#define | FSL_FEATURE_SOC_XTALOSC24M_COUNT (1)
#define | FSL_FEATURE_ADC_SUPPORT_HARDWARE_TRIGGER_REMOVE (0)
#define | FSL_FEATURE_ADC_SUPPORT_ALTCLK_REMOVE (1)
#define | FSL_FEATURE_ADC_CONVERSION_CONTROL_COUNT (8)
#define | FSL_FEATURE_ADC_ETC_HAS_CTRL_DMA_MODE_SEL (1)
#define | FSL_FEATURE_AOI_MODULE_INPUTS (4)
#define | FSL_FEATURE_AOI_EVENT_COUNT (4)
#define | FSL_FEATURE_FLEXCAN_HAS_MESSAGE_BUFFER_MAX_NUMBERn(x) (64)
#define | FSL_FEATURE_FLEXCAN_HAS_DOZE_MODE_SUPPORT (1)
#define | FSL_FEATURE_FLEXCAN_INSTANCE_HAS_DOZE_MODE_SUPPORTn(x)
#define | FSL_FEATURE_FLEXCAN_HAS_GLITCH_FILTER (1)
#define | FSL_FEATURE_FLEXCAN_HAS_EXTENDED_FLAG_REGISTER (1)
#define | FSL_FEATURE_FLEXCAN_INSTANCE_HAS_EXTENDED_TIMING_REGISTERn(x)
#define | FSL_FEATURE_FLEXCAN_HAS_RX_FIFO_DMA (1)
#define | FSL_FEATURE_FLEXCAN_INSTANCE_HAS_RX_FIFO_DMAn(x)
#define | FSL_FEATURE_FLEXCAN_SUPPORT_ENGINE_CLK_SEL_REMOVE (1)
#define | FSL_FEATURE_FLEXCAN_INSTANCE_SUPPORT_ENGINE_CLK_SEL_REMOVEn(x)
#define | FSL_FEATURE_FLEXCAN_HAS_ERRATA_5641 (0)
#define | FSL_FEATURE_FLEXCAN_HAS_ERRATA_5829 (1)
#define | FSL_FEATURE_FLEXCAN_HAS_ERRATA_6032 (1)
#define | FSL_FEATURE_FLEXCAN_HAS_ERRATA_9595 (1)
#define | FSL_FEATURE_FLEXCAN_HAS_FLEXIBLE_DATA_RATE (1)
#define | FSL_FEATURE_FLEXCAN_INSTANCE_HAS_FLEXIBLE_DATA_RATEn(x)
#define | FSL_FEATURE_FLEXCAN_HAS_EXTRA_MB_INT (1)
#define | FSL_FEATURE_CCM_HAS_ERRATA_50235 (1)
#define | FSL_FEATURE_CMP_HAS_TRIGGER_MODE (0)
#define | FSL_FEATURE_CMP_HAS_WINDOW_MODE (1)
#define | FSL_FEATURE_CMP_HAS_EXTERNAL_SAMPLE_SUPPORT (1)
#define | FSL_FEATURE_CMP_HAS_DMA (1)
#define | FSL_FEATURE_CMP_HAS_PASS_THROUGH_MODE (0)
#define | FSL_FEATURE_CMP_HAS_DAC_TEST (0)
#define | FSL_FEATURE_EDMA_MODULE_CHANNEL (32)
#define | FSL_FEATURE_EDMA_DMAMUX_CHANNELS (32)
#define | FSL_FEATURE_EDMA_CHANNEL_GROUP_COUNT (1)
#define | FSL_FEATURE_EDMA_HAS_ERROR_IRQ (1)
#define | FSL_FEATURE_EDMA_ASYNCHRO_REQUEST_CHANNEL_COUNT (32)
#define | FSL_FEATURE_EDMA_MODULE_CHANNEL_IRQ_ENTRY_SHARED_OFFSET (16)
#define | FSL_FEATURE_EDMA_SUPPORT_8_BYTES_TRANSFER (1)
#define | FSL_FEATURE_EDMA_SUPPORT_16_BYTES_TRANSFER (0)
#define | FSL_FEATURE_DMAMUX_MODULE_CHANNEL (32)
#define | FSL_FEATURE_DMAMUX_DMAMUX_CHANNELS (FSL_FEATURE_SOC_DMAMUX_COUNT * 32)
#define | FSL_FEATURE_DMAMUX_HAS_TRIG (1)
#define | FSL_FEATURE_DMAMUX_HAS_A_ON (1)
#define | FSL_FEATURE_ENET_HAS_INTERRUPT_COALESCE (1)
#define | FSL_FEATURE_ENET_QUEUE (1)
#define | FSL_FEATURE_ENET_HAS_AVB (0)
#define | FSL_FEATURE_ENET_HAS_TIMER_PWCONTROL (1)
#define | FSL_FEATURE_ENET_HAS_EXTEND_MDIO (1)
#define | FSL_FEATURE_ENET_HAS_ADD_1588_TIMER_CHN_INT (0)
#define | FSL_FEATURE_EWM_HAS_CLOCK_SELECT (1)
#define | FSL_FEATURE_EWM_HAS_PRESCALER (1)
#define | FSL_FEATURE_FLEXIO_HAS_SHIFTER_STATUS (1)
#define | FSL_FEATURE_FLEXIO_HAS_PIN_STATUS (1)
#define | FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_NIBBLE_BYTE_SWAP (1)
#define | FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_HALF_WORD_SWAP (1)
#define | FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_NIBBLE_SWAP (1)
#define | FSL_FEATURE_FLEXIO_HAS_STATE_MODE (1)
#define | FSL_FEATURE_FLEXIO_HAS_LOGIC_MODE (1)
#define | FSL_FEATURE_FLEXIO_HAS_PARALLEL_WIDTH (1)
#define | FSL_FEATURE_FLEXIO_VERID_RESET_VALUE (0x1010001)
#define | FSL_FEATURE_FLEXIO_PARAM_RESET_VALUE (0x2200404)
#define | FSL_FEATURE_FLEXIO_DMA_REQUEST_BASE_CHANNEL (0)
#define | FSL_FEATURE_FLEXRAM_INTERNAL_RAM_BANK_SIZE (32768)
#define | FSL_FEATURE_FLEXRAM_INTERNAL_RAM_TOTAL_BANK_NUMBERS (16)
#define | FSL_FEATURE_FLEXRAM_HAS_MAGIC_ADDR (0)
#define | FSL_FEATURE_FLEXSPI_AHB_BUFFER_COUNTn(x) (4)
#define | FSL_FEATURE_FLEXSPI_HAS_NO_DATA_LEARN (1)
#define | FSL_FEATURE_FLEXSPI_HAS_INTEN_AHBBUSERROREN (0)
#define | FSL_FEATURE_GPC_HAS_CNTR_DVFS0CR (0)
#define | FSL_FEATURE_GPC_HAS_CNTR_GPCIRQM (0)
#define | FSL_FEATURE_GPC_HAS_CNTR_L2PGE (0)
#define | FSL_FEATURE_GPC_HAS_CNTR_PDRAM0PGE (1)
#define | FSL_FEATURE_GPC_HAS_CNTR_VADC (0)
#define | FSL_FEATURE_GPC_HAS_CNTR_DISPLAY (0)
#define | FSL_FEATURE_GPC_HAS_IRQ_0_31 (1)
#define | FSL_FEATURE_IGPIO_HAS_DR_SET (1)
#define | FSL_FEATURE_IGPIO_HAS_DR_CLEAR (1)
#define | FSL_FEATURE_IGPIO_HAS_DR_TOGGLE (1)
#define | FSL_FEATURE_LCDIF_HAS_NO_AS (1)
#define | FSL_FEATURE_LCDIF_HAS_NO_RESET_PIN (1)
#define | FSL_FEATURE_LCDIF_HAS_LUT (1)
#define | FSL_FEATURE_LPI2C_HAS_SEPARATE_DMA_RX_TX_REQn(x) (0)
#define | FSL_FEATURE_LPI2C_FIFO_SIZEn(x) (4)
#define | FSL_FEATURE_LPSPI_FIFO_SIZEn(x) (16)
#define | FSL_FEATURE_LPSPI_HAS_SEPARATE_DMA_RX_TX_REQn(x) (1)
#define | FSL_FEATURE_LPUART_HAS_IRQ_EXTENDED_FUNCTIONS (0)
#define | FSL_FEATURE_LPUART_HAS_LOW_POWER_UART_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_EXTENDED_DATA_REGISTER_FLAGS (1)
#define | FSL_FEATURE_LPUART_HAS_FIFO (1)
#define | FSL_FEATURE_LPUART_HAS_MODIR (1)
#define | FSL_FEATURE_LPUART_HAS_MODEM_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_IR_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_STOP_BIT_CONFIG_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_10BIT_DATA_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_7BIT_DATA_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_BAUD_RATE_FINE_ADJUST_SUPPORT (0)
#define | FSL_FEATURE_LPUART_HAS_BAUD_RATE_OVER_SAMPLING_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_RX_RESYNC_SUPPORT (1)
#define | FSL_FEATURE_LPUART_HAS_BOTH_EDGE_SAMPLING_SUPPORT (1)
#define | FSL_FEATURE_LPUART_IS_SCI (1)
#define | FSL_FEATURE_LPUART_FIFO_SIZEn(x) (4)
#define | FSL_FEATURE_LPUART_MAX_DATA_WIDTH_WITH_NO_PARITY (10)
#define | FSL_FEATURE_LPUART_MAX_DATA_WIDTH_WITH_PARITY (9)
#define | FSL_FEATURE_LPUART_HAS_ADDRESS_MATCHING (1)
#define | FSL_FEATURE_LPUART_HAS_DMA_ENABLE (1)
#define | FSL_FEATURE_LPUART_HAS_DMA_SELECT (0)
#define | FSL_FEATURE_LPUART_HAS_BIT_ORDER_SELECT (1)
#define | FSL_FEATURE_LPUART_HAS_SMART_CARD_SUPPORT (0)
#define | FSL_FEATURE_LPUART_HAS_IMPROVED_SMART_CARD_SUPPORT (0)
#define | FSL_FEATURE_LPUART_HAS_LOCAL_OPERATION_NETWORK_SUPPORT (0)
#define | FSL_FEATURE_LPUART_HAS_32BIT_REGISTERS (1)
#define | FSL_FEATURE_LPUART_HAS_LIN_BREAK_DETECT (1)
#define | FSL_FEATURE_LPUART_HAS_WAIT_MODE_OPERATION (0)
#define | FSL_FEATURE_LPUART_HAS_SEPARATE_DMA_RX_TX_REQn(x) (1)
#define | FSL_FEATURE_LPUART_HAS_SEPARATE_RX_TX_IRQ (0)
#define | FSL_FEATURE_LPUART_HAS_PARAM (1)
#define | FSL_FEATURE_LPUART_HAS_VERID (1)
#define | FSL_FEATURE_LPUART_HAS_GLOBAL (1)
#define | FSL_FEATURE_LPUART_HAS_PINCFG (1)
#define | FSL_FEATURE_INTERRUPT_IRQ_MIN (-14)
#define | FSL_FEATURE_INTERRUPT_IRQ_MAX (157)
#define | FSL_FEATURE_PIT_TIMER_COUNT (4)
#define | FSL_FEATURE_PIT_HAS_LIFETIME_TIMER (1)
#define | FSL_FEATURE_PIT_HAS_CHAIN_MODE (1)
#define | FSL_FEATURE_PIT_HAS_SHARED_IRQ_HANDLER (1)
#define | FSL_FEATURE_PIT_HAS_MDIS (1)
#define | FSL_FEATURE_PMU_HAS_LOWPWR_CTRL (0)
#define | FSL_FEATURE_PWM_CHANNEL_COUNT (12U)
#define | FSL_FEATURE_PWM_CHANNELA_COUNT (4U)
#define | FSL_FEATURE_PWM_CHANNELB_COUNT (4U)
#define | FSL_FEATURE_PWM_CHANNELX_COUNT (4U)
#define | FSL_FEATURE_PWM_CMP_INT_HANDLER_COUNT (4U)
#define | FSL_FEATURE_PWM_RELOAD_INT_HANDLER_COUNT (4U)
#define | FSL_FEATURE_PWM_CAP_INT_HANDLER_COUNT (1U)
#define | FSL_FEATURE_PWM_RERR_INT_HANDLER_COUNT (1U)
#define | FSL_FEATURE_PWM_FAULT_INT_HANDLER_COUNT (1U)
#define | FSL_FEATURE_PWM_SUBMODULE_COUNT (4U)
#define | FSL_FEATURE_PXP_HAS_DITHER (0)
#define | FSL_FEATURE_PXP_HAS_EN_REPEAT (1)
#define | FSL_FEATURE_PXP_HAS_NO_CSC2 (1)
#define | FSL_FEATURE_PXP_HAS_NO_LUT (1)
#define | FSL_FEATURE_RTWDOG_HAS_WATCHDOG (1)
#define | FSL_FEATURE_RTWDOG_HAS_32BIT_ACCESS (1)
#define | FSL_FEATURE_SAI_FIFO_COUNT (32)
#define | FSL_FEATURE_SAI_CHANNEL_COUNTn(x)
#define | FSL_FEATURE_SAI_MAX_WORDS_PER_FRAME (32)
#define | FSL_FEATURE_SAI_HAS_FIFO_COMBINE_MODE (1)
#define | FSL_FEATURE_SAI_HAS_FIFO_PACKING (1)
#define | FSL_FEATURE_SAI_HAS_FIFO_FUNCTION_AFTER_ERROR (1)
#define | FSL_FEATURE_SAI_HAS_ON_DEMAND_MODE (1)
#define | FSL_FEATURE_SAI_HAS_CLOCKING_MODE (0)
#define | FSL_FEATURE_SAI_HAS_MCLKDIV_REGISTER (0)
#define | FSL_FEATURE_SAI_INT_SOURCE_NUM (2)
#define | FSL_FEATURE_SAI_HAS_MCR (0)
#define | FSL_FEATURE_SAI_HAS_NO_MCR_MICS (1)
#define | FSL_FEATURE_SAI_HAS_MDR (0)
#define | FSL_FEATURE_SAI_HAS_BCLK_BYPASS (0)
#define | FSL_FEATURE_SAI_HAS_MCR_MCLK_POST_DIV (0)
#define | FSL_FEATURE_SAI_HAS_CHANNEL_MODE (1)
#define | FSL_FEATURE_SEMC_HAS_NOR_WDH_TIME (0)
#define | FSL_FEATURE_SEMC_HAS_NOR_WDS_TIME (0)
#define | FSL_FEATURE_SNVS_HAS_SRTC (1)
#define | FSL_FEATURE_SRC_HAS_SCR_MASK_WDOG3_RST (1)
#define | FSL_FEATURE_SRC_HAS_SCR_MIX_RST_STRCH (0)
#define | FSL_FEATURE_SRC_HAS_SCR_DBG_RST_MSK_PG (1)
#define | FSL_FEATURE_SRC_HAS_SCR_WDOG3_RST_OPTN (0)
#define | FSL_FEATURE_SRC_HAS_SCR_CORES_DBG_RST (0)
#define | FSL_FEATURE_SRC_HAS_SCR_MTSR (0)
#define | FSL_FEATURE_SRC_HAS_SCR_CORE0_DBG_RST (1)
#define | FSL_FEATURE_SRC_HAS_SCR_CORE0_RST (1)
#define | FSL_FEATURE_SRC_HAS_SCR_LOCKUP_RST (0)
#define | FSL_FEATURE_SRC_HAS_SCR_SWRC (0)
#define | FSL_FEATURE_SRC_HAS_SCR_EIM_RST (0)
#define | FSL_FEATURE_SRC_HAS_SCR_LUEN (0)
#define | FSL_FEATURE_SRC_HAS_NO_SCR_WRBC (1)
#define | FSL_FEATURE_SRC_HAS_NO_SCR_WRE (1)
#define | FSL_FEATURE_SRC_HAS_SISR (0)
#define | FSL_FEATURE_SRC_HAS_SRSR_RESET_OUT (0)
#define | FSL_FEATURE_SRC_HAS_SRSR_WDOG3_RST_B (1)
#define | FSL_FEATURE_SRC_HAS_SRSR_JTAG_SW_RST (1)
#define | FSL_FEATURE_SRC_HAS_SRSR_SW (0)
#define | FSL_FEATURE_SRC_HAS_SRSR_IPP_USER_RESET_B (1)
#define | FSL_FEATURE_SRC_HAS_SRSR_SNVS (0)
#define | FSL_FEATURE_SRC_HAS_SRSR_CSU_RESET_B (1)
#define | FSL_FEATURE_SRC_HAS_SRSR_LOCKUP (0)
#define | FSL_FEATURE_SRC_HAS_SRSR_LOCKUP_SYSRESETREQ (1)
#define | FSL_FEATURE_SRC_HAS_SRSR_POR (0)
#define | FSL_FEATURE_SRC_HAS_SRSR_IPP_RESET_B (1)
#define | FSL_FEATURE_SRC_HAS_NO_SRSR_WBI (1)
#define | FSL_FEATURE_L1ICACHE_LINESIZE_BYTE (32)
#define | FSL_FEATURE_L1DCACHE_LINESIZE_BYTE (32)
#define | FSL_FEATURE_TRNG_HAS_NO_TRNG_ACC (1)
#define | FSL_FEATURE_USBHS_EHCI_COUNT (2)
#define | FSL_FEATURE_USBHS_ENDPT_COUNT (8)
#define | FSL_FEATURE_USDHC_HAS_EXT_DMA (0)
#define | FSL_FEATURE_USDHC_HAS_HS400_MODE (0)
#define | FSL_FEATURE_USDHC_HAS_SDR50_MODE (1)
#define | FSL_FEATURE_USDHC_HAS_SDR104_MODE (1)
#define | FSL_FEATURE_USDHC_HAS_RESET (0)
#define | FSL_FEATURE_USDHC_HAS_NO_RW_BURST_LEN (0)
#define | FSL_FEATURE_XBARA_INTERRUPT_COUNT (4)

## Macro Definition Documentation

## ◆ FSL_FEATURE_ADC_CONVERSION_CONTROL_COUNT

#define FSL_FEATURE_ADC_CONVERSION_CONTROL_COUNT (8)

Definition at line 146 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ADC_ETC_HAS_CTRL_DMA_MODE_SEL

#define FSL_FEATURE_ADC_ETC_HAS_CTRL_DMA_MODE_SEL (1)

Definition at line 151 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ADC_SUPPORT_ALTCLK_REMOVE

#define FSL_FEATURE_ADC_SUPPORT_ALTCLK_REMOVE (1)

Definition at line 144 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ADC_SUPPORT_HARDWARE_TRIGGER_REMOVE

#define FSL_FEATURE_ADC_SUPPORT_HARDWARE_TRIGGER_REMOVE (0)

Definition at line 142 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_AOI_EVENT_COUNT

#define FSL_FEATURE_AOI_EVENT_COUNT (4)

Definition at line 158 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_AOI_MODULE_INPUTS

#define FSL_FEATURE_AOI_MODULE_INPUTS (4)

Definition at line 156 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CCM_HAS_ERRATA_50235

#define FSL_FEATURE_CCM_HAS_ERRATA_50235 (1)

Definition at line 215 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CMP_HAS_DAC_TEST

#define FSL_FEATURE_CMP_HAS_DAC_TEST (0)

Definition at line 230 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CMP_HAS_DMA

#define FSL_FEATURE_CMP_HAS_DMA (1)

Definition at line 226 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CMP_HAS_EXTERNAL_SAMPLE_SUPPORT

#define FSL_FEATURE_CMP_HAS_EXTERNAL_SAMPLE_SUPPORT (1)

Definition at line 224 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CMP_HAS_PASS_THROUGH_MODE

#define FSL_FEATURE_CMP_HAS_PASS_THROUGH_MODE (0)

Definition at line 228 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CMP_HAS_TRIGGER_MODE

#define FSL_FEATURE_CMP_HAS_TRIGGER_MODE (0)

Definition at line 220 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_CMP_HAS_WINDOW_MODE

#define FSL_FEATURE_CMP_HAS_WINDOW_MODE (1)

Definition at line 222 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_DMAMUX_DMAMUX_CHANNELS

#define FSL_FEATURE_DMAMUX_DMAMUX_CHANNELS (FSL_FEATURE_SOC_DMAMUX_COUNT * 32)

Definition at line 256 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_DMAMUX_HAS_A_ON

#define FSL_FEATURE_DMAMUX_HAS_A_ON (1)

Definition at line 260 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_DMAMUX_HAS_TRIG

#define FSL_FEATURE_DMAMUX_HAS_TRIG (1)

Definition at line 258 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_DMAMUX_MODULE_CHANNEL

#define FSL_FEATURE_DMAMUX_MODULE_CHANNEL (32)

Definition at line 254 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_ASYNCHRO_REQUEST_CHANNEL_COUNT

#define FSL_FEATURE_EDMA_ASYNCHRO_REQUEST_CHANNEL_COUNT (32)

Definition at line 243 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_CHANNEL_GROUP_COUNT

#define FSL_FEATURE_EDMA_CHANNEL_GROUP_COUNT (1)

Definition at line 239 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_DMAMUX_CHANNELS

#define FSL_FEATURE_EDMA_DMAMUX_CHANNELS (32)

Definition at line 237 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_HAS_ERROR_IRQ

#define FSL_FEATURE_EDMA_HAS_ERROR_IRQ (1)

Definition at line 241 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_MODULE_CHANNEL

#define FSL_FEATURE_EDMA_MODULE_CHANNEL (32)

Definition at line 235 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_MODULE_CHANNEL_IRQ_ENTRY_SHARED_OFFSET

#define FSL_FEATURE_EDMA_MODULE_CHANNEL_IRQ_ENTRY_SHARED_OFFSET (16)

Definition at line 245 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_SUPPORT_16_BYTES_TRANSFER

#define FSL_FEATURE_EDMA_SUPPORT_16_BYTES_TRANSFER (0)

Definition at line 249 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EDMA_SUPPORT_8_BYTES_TRANSFER

#define FSL_FEATURE_EDMA_SUPPORT_8_BYTES_TRANSFER (1)

Definition at line 247 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ENET_HAS_ADD_1588_TIMER_CHN_INT

#define FSL_FEATURE_ENET_HAS_ADD_1588_TIMER_CHN_INT (0)

Definition at line 275 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ENET_HAS_AVB

#define FSL_FEATURE_ENET_HAS_AVB (0)

Definition at line 269 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ENET_HAS_EXTEND_MDIO

#define FSL_FEATURE_ENET_HAS_EXTEND_MDIO (1)

Definition at line 273 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ENET_HAS_INTERRUPT_COALESCE

#define FSL_FEATURE_ENET_HAS_INTERRUPT_COALESCE (1)

Definition at line 265 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ENET_HAS_TIMER_PWCONTROL

#define FSL_FEATURE_ENET_HAS_TIMER_PWCONTROL (1)

Definition at line 271 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_ENET_QUEUE

#define FSL_FEATURE_ENET_QUEUE (1)

Definition at line 267 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EWM_HAS_CLOCK_SELECT

#define FSL_FEATURE_EWM_HAS_CLOCK_SELECT (1)

Definition at line 280 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_EWM_HAS_PRESCALER

#define FSL_FEATURE_EWM_HAS_PRESCALER (1)

Definition at line 282 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_DOZE_MODE_SUPPORT

#define FSL_FEATURE_FLEXCAN_HAS_DOZE_MODE_SUPPORT (1)

Definition at line 165 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_ERRATA_5641

#define FSL_FEATURE_FLEXCAN_HAS_ERRATA_5641 (0)

Definition at line 195 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_ERRATA_5829

#define FSL_FEATURE_FLEXCAN_HAS_ERRATA_5829 (1)

Definition at line 197 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_ERRATA_6032

#define FSL_FEATURE_FLEXCAN_HAS_ERRATA_6032 (1)

Definition at line 199 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_ERRATA_9595

#define FSL_FEATURE_FLEXCAN_HAS_ERRATA_9595 (1)

Definition at line 201 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_EXTENDED_FLAG_REGISTER

#define FSL_FEATURE_FLEXCAN_HAS_EXTENDED_FLAG_REGISTER (1)

Definition at line 174 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_EXTRA_MB_INT

#define FSL_FEATURE_FLEXCAN_HAS_EXTRA_MB_INT (1)

Definition at line 210 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_FLEXIBLE_DATA_RATE

#define FSL_FEATURE_FLEXCAN_HAS_FLEXIBLE_DATA_RATE (1)

Definition at line 203 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_GLITCH_FILTER

#define FSL_FEATURE_FLEXCAN_HAS_GLITCH_FILTER (1)

Definition at line 172 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_MESSAGE_BUFFER_MAX_NUMBERn

#define FSL_FEATURE_FLEXCAN_HAS_MESSAGE_BUFFER_MAX_NUMBERn | ( |  | x | ) | (64)

Definition at line 163 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_HAS_RX_FIFO_DMA

#define FSL_FEATURE_FLEXCAN_HAS_RX_FIFO_DMA (1)

Definition at line 181 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_INSTANCE_HAS_DOZE_MODE_SUPPORTn

#define FSL_FEATURE_FLEXCAN_INSTANCE_HAS_DOZE_MODE_SUPPORTn | ( |  | x | ) |

Value:
(((x) == CAN1) ? (0) : \
(((x) == CAN2) ? (0) : \
(((x) == CAN3) ? (1) : (-1))))

Definition at line 167 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_INSTANCE_HAS_EXTENDED_TIMING_REGISTERn

#define FSL_FEATURE_FLEXCAN_INSTANCE_HAS_EXTENDED_TIMING_REGISTERn | ( |  | x | ) |

Value:
(((x) == CAN1) ? (0) : \
(((x) == CAN2) ? (0) : \
(((x) == CAN3) ? (1) : (-1))))

Definition at line 176 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_INSTANCE_HAS_FLEXIBLE_DATA_RATEn

#define FSL_FEATURE_FLEXCAN_INSTANCE_HAS_FLEXIBLE_DATA_RATEn | ( |  | x | ) |

Value:
(((x) == CAN1) ? (0) : \
(((x) == CAN2) ? (0) : \
(((x) == CAN3) ? (1) : (-1))))

Definition at line 205 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_INSTANCE_HAS_RX_FIFO_DMAn

#define FSL_FEATURE_FLEXCAN_INSTANCE_HAS_RX_FIFO_DMAn | ( |  | x | ) |

Value:
(((x) == CAN1) ? (0) : \
(((x) == CAN2) ? (0) : \
(((x) == CAN3) ? (1) : (-1))))

Definition at line 183 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_INSTANCE_SUPPORT_ENGINE_CLK_SEL_REMOVEn

#define FSL_FEATURE_FLEXCAN_INSTANCE_SUPPORT_ENGINE_CLK_SEL_REMOVEn | ( |  | x | ) |

Value:
(((x) == CAN1) ? (1) : \
(((x) == CAN2) ? (1) : \
(((x) == CAN3) ? (0) : (-1))))

Definition at line 190 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXCAN_SUPPORT_ENGINE_CLK_SEL_REMOVE

#define FSL_FEATURE_FLEXCAN_SUPPORT_ENGINE_CLK_SEL_REMOVE (1)

Definition at line 188 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_DMA_REQUEST_BASE_CHANNEL

#define FSL_FEATURE_FLEXIO_DMA_REQUEST_BASE_CHANNEL (0)

Definition at line 307 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_LOGIC_MODE

#define FSL_FEATURE_FLEXIO_HAS_LOGIC_MODE (1)

Definition at line 299 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_PARALLEL_WIDTH

#define FSL_FEATURE_FLEXIO_HAS_PARALLEL_WIDTH (1)

Definition at line 301 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_PIN_STATUS

#define FSL_FEATURE_FLEXIO_HAS_PIN_STATUS (1)

Definition at line 289 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_HALF_WORD_SWAP

#define FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_HALF_WORD_SWAP (1)

Definition at line 293 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_NIBBLE_BYTE_SWAP

#define FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_NIBBLE_BYTE_SWAP (1)

Definition at line 291 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_NIBBLE_SWAP

#define FSL_FEATURE_FLEXIO_HAS_SHFT_BUFFER_NIBBLE_SWAP (1)

Definition at line 295 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_SHIFTER_STATUS

#define FSL_FEATURE_FLEXIO_HAS_SHIFTER_STATUS (1)

Definition at line 287 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_HAS_STATE_MODE

#define FSL_FEATURE_FLEXIO_HAS_STATE_MODE (1)

Definition at line 297 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_PARAM_RESET_VALUE

#define FSL_FEATURE_FLEXIO_PARAM_RESET_VALUE (0x2200404)

Definition at line 305 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXIO_VERID_RESET_VALUE

#define FSL_FEATURE_FLEXIO_VERID_RESET_VALUE (0x1010001)

Definition at line 303 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXRAM_HAS_MAGIC_ADDR

#define FSL_FEATURE_FLEXRAM_HAS_MAGIC_ADDR (0)

Definition at line 316 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXRAM_INTERNAL_RAM_BANK_SIZE

#define FSL_FEATURE_FLEXRAM_INTERNAL_RAM_BANK_SIZE (32768)

Definition at line 312 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXRAM_INTERNAL_RAM_TOTAL_BANK_NUMBERS

#define FSL_FEATURE_FLEXRAM_INTERNAL_RAM_TOTAL_BANK_NUMBERS (16)

Definition at line 314 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXSPI_AHB_BUFFER_COUNTn

#define FSL_FEATURE_FLEXSPI_AHB_BUFFER_COUNTn | ( |  | x | ) | (4)

Definition at line 321 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXSPI_HAS_INTEN_AHBBUSERROREN

#define FSL_FEATURE_FLEXSPI_HAS_INTEN_AHBBUSERROREN (0)

Definition at line 325 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_FLEXSPI_HAS_NO_DATA_LEARN

#define FSL_FEATURE_FLEXSPI_HAS_NO_DATA_LEARN (1)

Definition at line 323 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_CNTR_DISPLAY

#define FSL_FEATURE_GPC_HAS_CNTR_DISPLAY (0)

Definition at line 340 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_CNTR_DVFS0CR

#define FSL_FEATURE_GPC_HAS_CNTR_DVFS0CR (0)

Definition at line 330 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_CNTR_GPCIRQM

#define FSL_FEATURE_GPC_HAS_CNTR_GPCIRQM (0)

Definition at line 332 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_CNTR_L2PGE

#define FSL_FEATURE_GPC_HAS_CNTR_L2PGE (0)

Definition at line 334 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_CNTR_PDRAM0PGE

#define FSL_FEATURE_GPC_HAS_CNTR_PDRAM0PGE (1)

Definition at line 336 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_CNTR_VADC

#define FSL_FEATURE_GPC_HAS_CNTR_VADC (0)

Definition at line 338 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_GPC_HAS_IRQ_0_31

#define FSL_FEATURE_GPC_HAS_IRQ_0_31 (1)

Definition at line 342 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_IGPIO_HAS_DR_CLEAR

#define FSL_FEATURE_IGPIO_HAS_DR_CLEAR (1)

Definition at line 349 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_IGPIO_HAS_DR_SET

#define FSL_FEATURE_IGPIO_HAS_DR_SET (1)

Definition at line 347 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_IGPIO_HAS_DR_TOGGLE

#define FSL_FEATURE_IGPIO_HAS_DR_TOGGLE (1)

Definition at line 351 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_INTERRUPT_IRQ_MAX

#define FSL_FEATURE_INTERRUPT_IRQ_MAX (157)

Definition at line 452 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_INTERRUPT_IRQ_MIN

#define FSL_FEATURE_INTERRUPT_IRQ_MIN (-14)

Definition at line 450 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_L1DCACHE_LINESIZE_BYTE

#define FSL_FEATURE_L1DCACHE_LINESIZE_BYTE (32)

Definition at line 629 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_L1ICACHE_LINESIZE_BYTE

#define FSL_FEATURE_L1ICACHE_LINESIZE_BYTE (32)

Definition at line 627 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LCDIF_HAS_LUT

#define FSL_FEATURE_LCDIF_HAS_LUT (1)

Definition at line 360 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LCDIF_HAS_NO_AS

#define FSL_FEATURE_LCDIF_HAS_NO_AS (1)

Definition at line 356 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LCDIF_HAS_NO_RESET_PIN

#define FSL_FEATURE_LCDIF_HAS_NO_RESET_PIN (1)

Definition at line 358 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPI2C_FIFO_SIZEn

#define FSL_FEATURE_LPI2C_FIFO_SIZEn | ( |  | x | ) | (4)

Definition at line 367 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPI2C_HAS_SEPARATE_DMA_RX_TX_REQn

#define FSL_FEATURE_LPI2C_HAS_SEPARATE_DMA_RX_TX_REQn | ( |  | x | ) | (0)

Definition at line 365 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPSPI_FIFO_SIZEn

#define FSL_FEATURE_LPSPI_FIFO_SIZEn | ( |  | x | ) | (16)

Definition at line 372 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPSPI_HAS_SEPARATE_DMA_RX_TX_REQn

#define FSL_FEATURE_LPSPI_HAS_SEPARATE_DMA_RX_TX_REQn | ( |  | x | ) | (1)

Definition at line 374 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_FIFO_SIZEn

#define FSL_FEATURE_LPUART_FIFO_SIZEn | ( |  | x | ) | (4)

Definition at line 409 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_10BIT_DATA_SUPPORT

#define FSL_FEATURE_LPUART_HAS_10BIT_DATA_SUPPORT (1)

Definition at line 395 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_32BIT_REGISTERS

#define FSL_FEATURE_LPUART_HAS_32BIT_REGISTERS (1)

Definition at line 429 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_7BIT_DATA_SUPPORT

#define FSL_FEATURE_LPUART_HAS_7BIT_DATA_SUPPORT (1)

Definition at line 397 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_ADDRESS_MATCHING

#define FSL_FEATURE_LPUART_HAS_ADDRESS_MATCHING (1)

Definition at line 415 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_BAUD_RATE_FINE_ADJUST_SUPPORT

#define FSL_FEATURE_LPUART_HAS_BAUD_RATE_FINE_ADJUST_SUPPORT (0)

Definition at line 399 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_BAUD_RATE_OVER_SAMPLING_SUPPORT

#define FSL_FEATURE_LPUART_HAS_BAUD_RATE_OVER_SAMPLING_SUPPORT (1)

Definition at line 401 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_BIT_ORDER_SELECT

#define FSL_FEATURE_LPUART_HAS_BIT_ORDER_SELECT (1)

Definition at line 421 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_BOTH_EDGE_SAMPLING_SUPPORT

#define FSL_FEATURE_LPUART_HAS_BOTH_EDGE_SAMPLING_SUPPORT (1)

Definition at line 405 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_DMA_ENABLE

#define FSL_FEATURE_LPUART_HAS_DMA_ENABLE (1)

Definition at line 417 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_DMA_SELECT

#define FSL_FEATURE_LPUART_HAS_DMA_SELECT (0)

Definition at line 419 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_EXTENDED_DATA_REGISTER_FLAGS

#define FSL_FEATURE_LPUART_HAS_EXTENDED_DATA_REGISTER_FLAGS (1)

Definition at line 383 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_FIFO

#define FSL_FEATURE_LPUART_HAS_FIFO (1)

Definition at line 385 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_GLOBAL

#define FSL_FEATURE_LPUART_HAS_GLOBAL (1)

Definition at line 443 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_IMPROVED_SMART_CARD_SUPPORT

#define FSL_FEATURE_LPUART_HAS_IMPROVED_SMART_CARD_SUPPORT (0)

Definition at line 425 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_IR_SUPPORT

#define FSL_FEATURE_LPUART_HAS_IR_SUPPORT (1)

Definition at line 391 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_IRQ_EXTENDED_FUNCTIONS

#define FSL_FEATURE_LPUART_HAS_IRQ_EXTENDED_FUNCTIONS (0)

Definition at line 379 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_LIN_BREAK_DETECT

#define FSL_FEATURE_LPUART_HAS_LIN_BREAK_DETECT (1)

Definition at line 431 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_LOCAL_OPERATION_NETWORK_SUPPORT

#define FSL_FEATURE_LPUART_HAS_LOCAL_OPERATION_NETWORK_SUPPORT (0)

Definition at line 427 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_LOW_POWER_UART_SUPPORT

#define FSL_FEATURE_LPUART_HAS_LOW_POWER_UART_SUPPORT (1)

Definition at line 381 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_MODEM_SUPPORT

#define FSL_FEATURE_LPUART_HAS_MODEM_SUPPORT (1)

Definition at line 389 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_MODIR

#define FSL_FEATURE_LPUART_HAS_MODIR (1)

Definition at line 387 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_PARAM

#define FSL_FEATURE_LPUART_HAS_PARAM (1)

Definition at line 439 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_PINCFG

#define FSL_FEATURE_LPUART_HAS_PINCFG (1)

Definition at line 445 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_RX_RESYNC_SUPPORT

#define FSL_FEATURE_LPUART_HAS_RX_RESYNC_SUPPORT (1)

Definition at line 403 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_SEPARATE_DMA_RX_TX_REQn

#define FSL_FEATURE_LPUART_HAS_SEPARATE_DMA_RX_TX_REQn | ( |  | x | ) | (1)

Definition at line 435 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_SEPARATE_RX_TX_IRQ

#define FSL_FEATURE_LPUART_HAS_SEPARATE_RX_TX_IRQ (0)

Definition at line 437 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_SMART_CARD_SUPPORT

#define FSL_FEATURE_LPUART_HAS_SMART_CARD_SUPPORT (0)

Definition at line 423 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_STOP_BIT_CONFIG_SUPPORT

#define FSL_FEATURE_LPUART_HAS_STOP_BIT_CONFIG_SUPPORT (1)

Definition at line 393 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_VERID

#define FSL_FEATURE_LPUART_HAS_VERID (1)

Definition at line 441 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_HAS_WAIT_MODE_OPERATION

#define FSL_FEATURE_LPUART_HAS_WAIT_MODE_OPERATION (0)

Definition at line 433 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_IS_SCI

#define FSL_FEATURE_LPUART_IS_SCI (1)

Definition at line 407 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_MAX_DATA_WIDTH_WITH_NO_PARITY

#define FSL_FEATURE_LPUART_MAX_DATA_WIDTH_WITH_NO_PARITY (10)

Definition at line 411 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_LPUART_MAX_DATA_WIDTH_WITH_PARITY

#define FSL_FEATURE_LPUART_MAX_DATA_WIDTH_WITH_PARITY (9)

Definition at line 413 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PIT_HAS_CHAIN_MODE

#define FSL_FEATURE_PIT_HAS_CHAIN_MODE (1)

Definition at line 465 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PIT_HAS_LIFETIME_TIMER

#define FSL_FEATURE_PIT_HAS_LIFETIME_TIMER (1)

Definition at line 463 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PIT_HAS_MDIS

#define FSL_FEATURE_PIT_HAS_MDIS (1)

Definition at line 469 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PIT_HAS_SHARED_IRQ_HANDLER

#define FSL_FEATURE_PIT_HAS_SHARED_IRQ_HANDLER (1)

Definition at line 467 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PIT_TIMER_COUNT

#define FSL_FEATURE_PIT_TIMER_COUNT (4)

Definition at line 461 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PMU_HAS_LOWPWR_CTRL

#define FSL_FEATURE_PMU_HAS_LOWPWR_CTRL (0)

Definition at line 474 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_CAP_INT_HANDLER_COUNT

#define FSL_FEATURE_PWM_CAP_INT_HANDLER_COUNT (1U)

Definition at line 491 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_CHANNEL_COUNT

#define FSL_FEATURE_PWM_CHANNEL_COUNT (12U)

Definition at line 479 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_CHANNELA_COUNT

#define FSL_FEATURE_PWM_CHANNELA_COUNT (4U)

Definition at line 481 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_CHANNELB_COUNT

#define FSL_FEATURE_PWM_CHANNELB_COUNT (4U)

Definition at line 483 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_CHANNELX_COUNT

#define FSL_FEATURE_PWM_CHANNELX_COUNT (4U)

Definition at line 485 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_CMP_INT_HANDLER_COUNT

#define FSL_FEATURE_PWM_CMP_INT_HANDLER_COUNT (4U)

Definition at line 487 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_FAULT_INT_HANDLER_COUNT

#define FSL_FEATURE_PWM_FAULT_INT_HANDLER_COUNT (1U)

Definition at line 495 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_RELOAD_INT_HANDLER_COUNT

#define FSL_FEATURE_PWM_RELOAD_INT_HANDLER_COUNT (4U)

Definition at line 489 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_RERR_INT_HANDLER_COUNT

#define FSL_FEATURE_PWM_RERR_INT_HANDLER_COUNT (1U)

Definition at line 493 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PWM_SUBMODULE_COUNT

#define FSL_FEATURE_PWM_SUBMODULE_COUNT (4U)

Definition at line 497 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PXP_HAS_DITHER

#define FSL_FEATURE_PXP_HAS_DITHER (0)

Definition at line 502 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PXP_HAS_EN_REPEAT

#define FSL_FEATURE_PXP_HAS_EN_REPEAT (1)

Definition at line 504 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PXP_HAS_NO_CSC2

#define FSL_FEATURE_PXP_HAS_NO_CSC2 (1)

Definition at line 506 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_PXP_HAS_NO_LUT

#define FSL_FEATURE_PXP_HAS_NO_LUT (1)

Definition at line 508 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_RTWDOG_HAS_32BIT_ACCESS

#define FSL_FEATURE_RTWDOG_HAS_32BIT_ACCESS (1)

Definition at line 515 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_RTWDOG_HAS_WATCHDOG

#define FSL_FEATURE_RTWDOG_HAS_WATCHDOG (1)

Definition at line 513 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_CHANNEL_COUNTn

#define FSL_FEATURE_SAI_CHANNEL_COUNTn | ( |  | x | ) |

Value:
(((x) == SAI1) ? (4) : \
(((x) == SAI2) ? (1) : \
(((x) == SAI3) ? (1) : (-1))))

Definition at line 522 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_FIFO_COUNT

#define FSL_FEATURE_SAI_FIFO_COUNT (32)

Definition at line 520 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_BCLK_BYPASS

#define FSL_FEATURE_SAI_HAS_BCLK_BYPASS (0)

Definition at line 549 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_CHANNEL_MODE

#define FSL_FEATURE_SAI_HAS_CHANNEL_MODE (1)

Definition at line 553 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_CLOCKING_MODE

#define FSL_FEATURE_SAI_HAS_CLOCKING_MODE (0)

Definition at line 537 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_FIFO_COMBINE_MODE

#define FSL_FEATURE_SAI_HAS_FIFO_COMBINE_MODE (1)

Definition at line 529 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_FIFO_FUNCTION_AFTER_ERROR

#define FSL_FEATURE_SAI_HAS_FIFO_FUNCTION_AFTER_ERROR (1)

Definition at line 533 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_FIFO_PACKING

#define FSL_FEATURE_SAI_HAS_FIFO_PACKING (1)

Definition at line 531 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_MCLKDIV_REGISTER

#define FSL_FEATURE_SAI_HAS_MCLKDIV_REGISTER (0)

Definition at line 539 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_MCR

#define FSL_FEATURE_SAI_HAS_MCR (0)

Definition at line 543 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_MCR_MCLK_POST_DIV

#define FSL_FEATURE_SAI_HAS_MCR_MCLK_POST_DIV (0)

Definition at line 551 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_MDR

#define FSL_FEATURE_SAI_HAS_MDR (0)

Definition at line 547 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_NO_MCR_MICS

#define FSL_FEATURE_SAI_HAS_NO_MCR_MICS (1)

Definition at line 545 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_HAS_ON_DEMAND_MODE

#define FSL_FEATURE_SAI_HAS_ON_DEMAND_MODE (1)

Definition at line 535 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_INT_SOURCE_NUM

#define FSL_FEATURE_SAI_INT_SOURCE_NUM (2)

Definition at line 541 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SAI_MAX_WORDS_PER_FRAME

#define FSL_FEATURE_SAI_MAX_WORDS_PER_FRAME (32)

Definition at line 527 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SEMC_HAS_NOR_WDH_TIME

#define FSL_FEATURE_SEMC_HAS_NOR_WDH_TIME (0)

Definition at line 558 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SEMC_HAS_NOR_WDS_TIME

#define FSL_FEATURE_SEMC_HAS_NOR_WDS_TIME (0)

Definition at line 560 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SNVS_HAS_SRTC

#define FSL_FEATURE_SNVS_HAS_SRTC (1)

Definition at line 565 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_ADC_COUNT

#define FSL_FEATURE_SOC_ADC_COUNT (2)

Definition at line 33 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_AIPSTZ_COUNT

#define FSL_FEATURE_SOC_AIPSTZ_COUNT (4)

Definition at line 35 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_AOI_COUNT

#define FSL_FEATURE_SOC_AOI_COUNT (2)

Definition at line 37 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_CCM_ANALOG_COUNT

#define FSL_FEATURE_SOC_CCM_ANALOG_COUNT (1)

Definition at line 41 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_CCM_COUNT

#define FSL_FEATURE_SOC_CCM_COUNT (1)

Definition at line 39 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_CMP_COUNT

#define FSL_FEATURE_SOC_CMP_COUNT (4)

Definition at line 43 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_CSI_COUNT

#define FSL_FEATURE_SOC_CSI_COUNT (1)

Definition at line 45 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_DCDC_COUNT

#define FSL_FEATURE_SOC_DCDC_COUNT (1)

Definition at line 47 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_DCP_COUNT

#define FSL_FEATURE_SOC_DCP_COUNT (1)

Definition at line 49 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_DMAMUX_COUNT

#define FSL_FEATURE_SOC_DMAMUX_COUNT (1)

Definition at line 51 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_EDMA_COUNT

#define FSL_FEATURE_SOC_EDMA_COUNT (1)

Definition at line 53 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_ENC_COUNT

#define FSL_FEATURE_SOC_ENC_COUNT (4)

Definition at line 55 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_ENET_COUNT

#define FSL_FEATURE_SOC_ENET_COUNT (2)

Definition at line 57 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_EWM_COUNT

#define FSL_FEATURE_SOC_EWM_COUNT (1)

Definition at line 59 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_FLEXCAN_COUNT

#define FSL_FEATURE_SOC_FLEXCAN_COUNT (3)

Definition at line 61 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_FLEXIO_COUNT

#define FSL_FEATURE_SOC_FLEXIO_COUNT (3)

Definition at line 63 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_FLEXRAM_COUNT

#define FSL_FEATURE_SOC_FLEXRAM_COUNT (1)

Definition at line 65 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_FLEXSPI_COUNT

#define FSL_FEATURE_SOC_FLEXSPI_COUNT (2)

Definition at line 67 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_GPC_COUNT

#define FSL_FEATURE_SOC_GPC_COUNT (1)

Definition at line 69 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_GPT_COUNT

#define FSL_FEATURE_SOC_GPT_COUNT (2)

Definition at line 71 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_I2S_COUNT

#define FSL_FEATURE_SOC_I2S_COUNT (3)

Definition at line 73 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_IGPIO_COUNT

#define FSL_FEATURE_SOC_IGPIO_COUNT (9)

Definition at line 75 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_IOMUXC_COUNT

#define FSL_FEATURE_SOC_IOMUXC_COUNT (1)

Definition at line 77 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_IOMUXC_GPR_COUNT

#define FSL_FEATURE_SOC_IOMUXC_GPR_COUNT (1)

Definition at line 79 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_IOMUXC_SNVS_COUNT

#define FSL_FEATURE_SOC_IOMUXC_SNVS_COUNT (1)

Definition at line 81 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_KPP_COUNT

#define FSL_FEATURE_SOC_KPP_COUNT (1)

Definition at line 83 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_LCDIF_COUNT

#define FSL_FEATURE_SOC_LCDIF_COUNT (1)

Definition at line 85 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_LPI2C_COUNT

#define FSL_FEATURE_SOC_LPI2C_COUNT (4)

Definition at line 87 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_LPSPI_COUNT

#define FSL_FEATURE_SOC_LPSPI_COUNT (4)

Definition at line 89 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_LPUART_COUNT

#define FSL_FEATURE_SOC_LPUART_COUNT (8)

Definition at line 91 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_OCOTP_COUNT

#define FSL_FEATURE_SOC_OCOTP_COUNT (1)

Definition at line 93 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_PIT_COUNT

#define FSL_FEATURE_SOC_PIT_COUNT (1)

Definition at line 95 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_PMU_COUNT

#define FSL_FEATURE_SOC_PMU_COUNT (1)

Definition at line 97 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_PWM_COUNT

#define FSL_FEATURE_SOC_PWM_COUNT (4)

Definition at line 99 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_PXP_COUNT

#define FSL_FEATURE_SOC_PXP_COUNT (1)

Definition at line 101 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_ROMC_COUNT

#define FSL_FEATURE_SOC_ROMC_COUNT (1)

Definition at line 103 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_SEMC_COUNT

#define FSL_FEATURE_SOC_SEMC_COUNT (1)

Definition at line 105 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_SNVS_COUNT

#define FSL_FEATURE_SOC_SNVS_COUNT (1)

Definition at line 107 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_SPDIF_COUNT

#define FSL_FEATURE_SOC_SPDIF_COUNT (1)

Definition at line 109 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_SRC_COUNT

#define FSL_FEATURE_SOC_SRC_COUNT (1)

Definition at line 111 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_TEMPMON_COUNT

#define FSL_FEATURE_SOC_TEMPMON_COUNT (1)

Definition at line 113 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_TMR_COUNT

#define FSL_FEATURE_SOC_TMR_COUNT (4)

Definition at line 115 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_TRNG_COUNT

#define FSL_FEATURE_SOC_TRNG_COUNT (1)

Definition at line 117 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_TSC_COUNT

#define FSL_FEATURE_SOC_TSC_COUNT (1)

Definition at line 119 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_USB_ANALOG_COUNT

#define FSL_FEATURE_SOC_USB_ANALOG_COUNT (1)

Definition at line 127 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_USBHS_COUNT

#define FSL_FEATURE_SOC_USBHS_COUNT (2)

Definition at line 121 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_USBNC_COUNT

#define FSL_FEATURE_SOC_USBNC_COUNT (2)

Definition at line 123 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_USBPHY_COUNT

#define FSL_FEATURE_SOC_USBPHY_COUNT (2)

Definition at line 125 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_USDHC_COUNT

#define FSL_FEATURE_SOC_USDHC_COUNT (2)

Definition at line 129 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_WDOG_COUNT

#define FSL_FEATURE_SOC_WDOG_COUNT (2)

Definition at line 131 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_XBARA_COUNT

#define FSL_FEATURE_SOC_XBARA_COUNT (1)

Definition at line 133 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_XBARB_COUNT

#define FSL_FEATURE_SOC_XBARB_COUNT (2)

Definition at line 135 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SOC_XTALOSC24M_COUNT

#define FSL_FEATURE_SOC_XTALOSC24M_COUNT (1)

Definition at line 137 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_NO_SCR_WRBC

#define FSL_FEATURE_SRC_HAS_NO_SCR_WRBC (1)

Definition at line 594 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_NO_SCR_WRE

#define FSL_FEATURE_SRC_HAS_NO_SCR_WRE (1)

Definition at line 596 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_NO_SRSR_WBI

#define FSL_FEATURE_SRC_HAS_NO_SRSR_WBI (1)

Definition at line 622 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_CORE0_DBG_RST

#define FSL_FEATURE_SRC_HAS_SCR_CORE0_DBG_RST (1)

Definition at line 582 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_CORE0_RST

#define FSL_FEATURE_SRC_HAS_SCR_CORE0_RST (1)

Definition at line 584 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_CORES_DBG_RST

#define FSL_FEATURE_SRC_HAS_SCR_CORES_DBG_RST (0)

Definition at line 578 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_DBG_RST_MSK_PG

#define FSL_FEATURE_SRC_HAS_SCR_DBG_RST_MSK_PG (1)

Definition at line 574 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_EIM_RST

#define FSL_FEATURE_SRC_HAS_SCR_EIM_RST (0)

Definition at line 590 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_LOCKUP_RST

#define FSL_FEATURE_SRC_HAS_SCR_LOCKUP_RST (0)

Definition at line 586 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_LUEN

#define FSL_FEATURE_SRC_HAS_SCR_LUEN (0)

Definition at line 592 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_MASK_WDOG3_RST

#define FSL_FEATURE_SRC_HAS_SCR_MASK_WDOG3_RST (1)

Definition at line 570 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_MIX_RST_STRCH

#define FSL_FEATURE_SRC_HAS_SCR_MIX_RST_STRCH (0)

Definition at line 572 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_MTSR

#define FSL_FEATURE_SRC_HAS_SCR_MTSR (0)

Definition at line 580 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_SWRC

#define FSL_FEATURE_SRC_HAS_SCR_SWRC (0)

Definition at line 588 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SCR_WDOG3_RST_OPTN

#define FSL_FEATURE_SRC_HAS_SCR_WDOG3_RST_OPTN (0)

Definition at line 576 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SISR

#define FSL_FEATURE_SRC_HAS_SISR (0)

Definition at line 598 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_CSU_RESET_B

#define FSL_FEATURE_SRC_HAS_SRSR_CSU_RESET_B (1)

Definition at line 612 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_IPP_RESET_B

#define FSL_FEATURE_SRC_HAS_SRSR_IPP_RESET_B (1)

Definition at line 620 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_IPP_USER_RESET_B

#define FSL_FEATURE_SRC_HAS_SRSR_IPP_USER_RESET_B (1)

Definition at line 608 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_JTAG_SW_RST

#define FSL_FEATURE_SRC_HAS_SRSR_JTAG_SW_RST (1)

Definition at line 604 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_LOCKUP

#define FSL_FEATURE_SRC_HAS_SRSR_LOCKUP (0)

Definition at line 614 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_LOCKUP_SYSRESETREQ

#define FSL_FEATURE_SRC_HAS_SRSR_LOCKUP_SYSRESETREQ (1)

Definition at line 616 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_POR

#define FSL_FEATURE_SRC_HAS_SRSR_POR (0)

Definition at line 618 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_RESET_OUT

#define FSL_FEATURE_SRC_HAS_SRSR_RESET_OUT (0)

Definition at line 600 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_SNVS

#define FSL_FEATURE_SRC_HAS_SRSR_SNVS (0)

Definition at line 610 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_SW

#define FSL_FEATURE_SRC_HAS_SRSR_SW (0)

Definition at line 606 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_SRC_HAS_SRSR_WDOG3_RST_B

#define FSL_FEATURE_SRC_HAS_SRSR_WDOG3_RST_B (1)

Definition at line 602 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_TRNG_HAS_NO_TRNG_ACC

#define FSL_FEATURE_TRNG_HAS_NO_TRNG_ACC (1)

Definition at line 634 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USBHS_EHCI_COUNT

#define FSL_FEATURE_USBHS_EHCI_COUNT (2)

Definition at line 639 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USBHS_ENDPT_COUNT

#define FSL_FEATURE_USBHS_ENDPT_COUNT (8)

Definition at line 641 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USDHC_HAS_EXT_DMA

#define FSL_FEATURE_USDHC_HAS_EXT_DMA (0)

Definition at line 646 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USDHC_HAS_HS400_MODE

#define FSL_FEATURE_USDHC_HAS_HS400_MODE (0)

Definition at line 648 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USDHC_HAS_NO_RW_BURST_LEN

#define FSL_FEATURE_USDHC_HAS_NO_RW_BURST_LEN (0)

Definition at line 656 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USDHC_HAS_RESET

#define FSL_FEATURE_USDHC_HAS_RESET (0)

Definition at line 654 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USDHC_HAS_SDR104_MODE

#define FSL_FEATURE_USDHC_HAS_SDR104_MODE (1)

Definition at line 652 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_USDHC_HAS_SDR50_MODE

#define FSL_FEATURE_USDHC_HAS_SDR50_MODE (1)

Definition at line 650 of file MIMXRT1062_features.h.

## ◆ FSL_FEATURE_XBARA_INTERRUPT_COUNT

#define FSL_FEATURE_XBARA_INTERRUPT_COUNT (4)

Definition at line 661 of file MIMXRT1062_features.h.

CAN3
#define CAN3
Definition: MIMXRT1062.h:5251
CAN1
#define CAN1
Definition: MIMXRT1062.h:5243
SAI3
#define SAI3
Definition: MIMXRT1062.h:21894
SAI2
#define SAI2
Definition: MIMXRT1062.h:21890
SAI1
#define SAI1
Definition: MIMXRT1062.h:21886
CAN2
#define CAN2
Definition: MIMXRT1062.h:5247