Callisto4Bootloader: CSI Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
CSI Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| CSI Register Masks

## Data Structures

struct | CSI_Type

## Macros

#define | CSI_BASE (0x402BC000u)
#define | CSI ((CSI_Type *)CSI_BASE)
#define | CSI_BASE_ADDRS { CSI_BASE }
#define | CSI_BASE_PTRS { CSI }
#define | CSI_IRQS { CSI_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ CSI

#define CSI ((CSI_Type *)CSI_BASE)

Peripheral CSI base pointer

Definition at line 10630 of file MIMXRT1062.h.

## ◆ CSI_BASE

#define CSI_BASE (0x402BC000u)

Peripheral CSI base address

Definition at line 10628 of file MIMXRT1062.h.

## ◆ CSI_BASE_ADDRS

#define CSI_BASE_ADDRS { CSI_BASE }

Array initializer of CSI peripheral base addresses

Definition at line 10632 of file MIMXRT1062.h.

## ◆ CSI_BASE_PTRS

#define CSI_BASE_PTRS { CSI }

Array initializer of CSI peripheral base pointers

Definition at line 10634 of file MIMXRT1062.h.

## ◆ CSI_IRQS

#define CSI_IRQS { CSI_IRQn }

Interrupt vectors for the CSI peripheral type

Definition at line 10636 of file MIMXRT1062.h.