Callisto4Bootloader: SEMC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
SEMC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| SEMC Register Masks

## Data Structures

struct | SEMC_Type

## Macros

#define | SEMC_BASE (0x402F0000u)
#define | SEMC ((SEMC_Type *)SEMC_BASE)
#define | SEMC_BASE_ADDRS { SEMC_BASE }
#define | SEMC_BASE_PTRS { SEMC }
#define | SEMC_IRQS { SEMC_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ SEMC

#define SEMC ((SEMC_Type *)SEMC_BASE)

Peripheral SEMC base pointer

Definition at line 37678 of file MIMXRT1062.h.

## ◆ SEMC_BASE

#define SEMC_BASE (0x402F0000u)

Peripheral SEMC base address

Definition at line 37676 of file MIMXRT1062.h.

## ◆ SEMC_BASE_ADDRS

#define SEMC_BASE_ADDRS { SEMC_BASE }

Array initializer of SEMC peripheral base addresses

Definition at line 37680 of file MIMXRT1062.h.

## ◆ SEMC_BASE_PTRS

#define SEMC_BASE_PTRS { SEMC }

Array initializer of SEMC peripheral base pointers

Definition at line 37682 of file MIMXRT1062.h.

## ◆ SEMC_IRQS

#define SEMC_IRQS { SEMC_IRQn }

Interrupt vectors for the SEMC peripheral type

Definition at line 37684 of file MIMXRT1062.h.