Callisto4Bootloader: KPP Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
KPP Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| KPP Register Masks

## Data Structures

struct | KPP_Type

## Macros

#define | KPP_BASE (0x401FC000u)
#define | KPP ((KPP_Type *)KPP_BASE)
#define | KPP_BASE_ADDRS { KPP_BASE }
#define | KPP_BASE_PTRS { KPP }
#define | KPP_IRQS { KPP_IRQn }

## Detailed Description

## Macro Definition Documentation

## ◆ KPP

#define KPP ((KPP_Type *)KPP_BASE)

Peripheral KPP base pointer

Definition at line 25093 of file MIMXRT1062.h.

## ◆ KPP_BASE

#define KPP_BASE (0x401FC000u)

Peripheral KPP base address

Definition at line 25091 of file MIMXRT1062.h.

## ◆ KPP_BASE_ADDRS

#define KPP_BASE_ADDRS { KPP_BASE }

Array initializer of KPP peripheral base addresses

Definition at line 25095 of file MIMXRT1062.h.

## ◆ KPP_BASE_PTRS

#define KPP_BASE_PTRS { KPP }

Array initializer of KPP peripheral base pointers

Definition at line 25097 of file MIMXRT1062.h.

## ◆ KPP_IRQS

#define KPP_IRQS { KPP_IRQn }

Interrupt vectors for the KPP peripheral type

Definition at line 25099 of file MIMXRT1062.h.