MCUX CLNS MCUX Crypto Library Normal Secure |

Data Fields
mcuxClCss_InterruptOptionSet_t Union Reference
mcuxClCss » mcuxClCss_Common » mcuxClCss_Common_Types

Type to control which CSS interrupts should be set when calling mcuxClCss_SetIntFlags. More...

`#include <mcuxClCss_Common.h>`

## Data Fields

struct {
uint32_t value
| Accesses the bit field as a full word. More...
} | word
| Access mcuxClCss_InterruptOptionSet_t word-wise. More...
struct {
uint32_t cssint:1
| Whether CSS interrupt should be set. (For possible values of this field, see mcuxClCss_InterruptOptionSet_t) More...
uint32_t __pad0__:2
| RFU. More...
uint32_t __pad1__:29
| RFU. More...
} | bits
| Access mcuxClCss_InterruptOptionSet_t bit-wise. More...

## Detailed Description

Type to control which CSS interrupts should be set when calling mcuxClCss_SetIntFlags.

## Field Documentation

## ◆ value

uint32_t mcuxClCss_InterruptOptionSet_t::value

Accesses the bit field as a full word.

## ◆ word

struct { ... } mcuxClCss_InterruptOptionSet_t::word

Access mcuxClCss_InterruptOptionSet_t word-wise.

## ◆ cssint

uint32_t mcuxClCss_InterruptOptionSet_t::cssint

Whether CSS interrupt should be set. (For possible values of this field, see mcuxClCss_InterruptOptionSet_t)

## ◆ __pad0__

uint32_t mcuxClCss_InterruptOptionSet_t::__pad0__

RFU.

## ◆ __pad1__

uint32_t mcuxClCss_InterruptOptionSet_t::__pad1__

RFU.

## ◆ bits

struct { ... } mcuxClCss_InterruptOptionSet_t::bits

Access mcuxClCss_InterruptOptionSet_t bit-wise.