MCUX CLNS MCUX Crypto Library Normal Secure |

mcuxClCss_Common.h
Go to the documentation of this file.
1 /*--------------------------------------------------------------------------*/
2 /* Copyright 2020-2021 NXP */
3 /* */
4 /* NXP Confidential. This software is owned or controlled by NXP and may */
5 /* only be used strictly in accordance with the applicable license terms. */
6 /* By expressly accepting such terms or by downloading, installing, */
7 /* activating and/or otherwise using the software, you are agreeing that */
8 /* you have read, and that you agree to comply with and are bound by, such */
9 /* license terms. If you do not agree to be bound by the applicable license */
10 /* terms, then you may not retain, install, activate or otherwise use the */
11 /* software. */
12 /*--------------------------------------------------------------------------*/
13
27 #ifndef MCUXCLCSS_COMMON_H_
28 #define MCUXCLCSS_COMMON_H_
29
30 #include <mcuxClCss_Types.h> // Common types
31 #include <mcuxCsslFlowProtection.h>
32
40 #define MCUXCLCSS_API
41
42 /**********************************************
43 * CONSTANTS
44 **********************************************/
45
57 #define MCUXCLCSS_HW_VERSION ((mcuxClCss_HwVersion_t) { \
58 .bits = { \
59 .level = (uint32_t) 0, \
60 .major = (uint32_t) 2, \
61 .minor = (uint32_t) 19, \
62 .revision = (uint32_t) 0 \
63 } \
64 })
65
72 #define MCUXCLCSS_CSS_INTERRUPT_ENABLE ((uint32_t) 1U)
73 #define MCUXCLCSS_CSS_INTERRUPT_DISABLE ((uint32_t) 0U)
74
82 #define MCUXCLCSS_CSS_RESET_CLEAR ((uint32_t) 1U)
83 #define MCUXCLCSS_CSS_RESET_KEEP ((uint32_t) 0U)
84
92 #define MCUXCLCSS_CSS_INTERRUPT_SET ((uint32_t) 1U)
93 #define MCUXCLCSS_CSS_INTERRUPT_KEEP ((uint32_t) 0U)
94
102 #define MCUXCLCSS_ERROR_FLAGS_KEEP ((mcuxClCss_ErrorHandling_t) 0x0u)
103 #define MCUXCLCSS_ERROR_FLAGS_CLEAR ((mcuxClCss_ErrorHandling_t) 0x1u)
104
112 #define MCUXCLCSS_RESET_DO_NOT_CANCEL ((mcuxClCss_ResetOption_t) 0x0u)
113 #define MCUXCLCSS_RESET_CANCEL ((mcuxClCss_ResetOption_t) 0x1u)
114
127 #define MCUXCLCSS_STATUS_PPROT_UNPRIVILEGED_SECURE ((uint32_t) 0x0u)
128 #define MCUXCLCSS_STATUS_PPROT_PRIVILEGED_SECURE ((uint32_t) 0x1u)
129 #define MCUXCLCSS_STATUS_PPROT_UNPRIVILEGED_NONSECURE ((uint32_t) 0x2u)
130 #define MCUXCLCSS_STATUS_PPROT_PRIVILEGED_NONSECURE ((uint32_t) 0x3u)
131
139 #define MCUXCLCSS_STATUS_ECDSAVFY_NORUN ((uint32_t) 0x0u)
140 #define MCUXCLCSS_STATUS_ECDSAVFY_FAIL ((uint32_t) 0x1u)
141 #define MCUXCLCSS_STATUS_ECDSAVFY_OK ((uint32_t) 0x2u)
142 #define MCUXCLCSS_STATUS_ECDSAVFY_ERROR ((uint32_t) 0x3u)
143
150 #define MCUXCLCSS_STATUS_DRBGENTLVL_NONE ((uint32_t) 0x0u)
151 #define MCUXCLCSS_STATUS_DRBGENTLVL_LOW ((uint32_t) 0x1u)
152 #define MCUXCLCSS_STATUS_DRBGENTLVL_HIGH ((uint32_t) 0x2u)
153
163 /**********************************************
164 * TYPEDEFS
165 **********************************************/
166
179 typedef union
180 {
181 struct
182 {
183 uint32_t value;
184 } word;
185 struct
186 {
187 uint32_t revision :4;
188 uint32_t minor :8;
189 uint32_t major :4;
190 uint32_t level :4;
191 uint32_t :12;
192 } bits;
193 } mcuxClCss_HwVersion_t;
194
200 typedef union
201 {
202 struct
203 {
204 uint32_t value;
205 } word;
206 struct
207 {
208 uint32_t busy :1;
209 uint32_t irq :1;
210 uint32_t err :1;
211 uint32_t prngready :1;
212 uint32_t ecdsavfy :2;
213 uint32_t pprot :2;
214 uint32_t drbgentlvl :2;
215 uint32_t dtrng_busy: 1;
216 uint32_t :2;
217 uint32_t :3;
218 uint32_t :1;
219 uint32_t :15;
220 } bits;
221 } mcuxClCss_HwState_t;
222
228 typedef uint32_t mcuxClCss_ErrorHandling_t;
229
235 typedef uint32_t mcuxClCss_ResetOption_t;
236
242 typedef union
243 {
244 struct
245 {
246 uint32_t value;
247 } word;
248 struct
249 {
250 uint32_t cssint :1;
251 uint32_t :1;
252 uint32_t :30;
253 } bits;
254 } mcuxClCss_InterruptOptionEn_t;
255
259 typedef union
260 {
261 struct
262 {
263 uint32_t value;
264 } word;
265 struct
266 {
267 uint32_t cssint :1;
268 uint32_t :1;
269 uint32_t :30;
270 } bits;
271 } mcuxClCss_InterruptOptionRst_t;
272
276 typedef union
277 {
278 struct
279 {
280 uint32_t value;
281 } word;
282 struct
283 {
284 uint32_t cssint :1;
285 uint32_t :2;
286 uint32_t :29;
287 } bits;
288 } mcuxClCss_InterruptOptionSet_t;
289
295 typedef union
296 {
297 struct
298 {
299 uint32_t value;
300 } word;
301 struct
302 {
303 uint32_t ciphersup :1;
304 uint32_t authciphersup :1;
305 uint32_t ecsignsup :1;
306 uint32_t ecvfysup :1;
307 uint32_t eckxchsup :1;
308 uint32_t keygensup :1;
309 uint32_t keyinsup :1;
310 uint32_t keyoutsup :1;
311 uint32_t kdeletesup :1;
312 uint32_t keyprovsup :1;
313 uint32_t ckdfsup :1;
314 uint32_t hkdfsup :1;
315 uint32_t tlsinitsup :1;
316 uint32_t hashsup :1;
317 uint32_t hmacsup :1;
318 uint32_t cmacsup :1;
319 uint32_t drbgreqsup :1;
320 uint32_t drbgtestsup :1;
321 uint32_t dtrgncfgloadsup :1;
322 uint32_t dtrngevalsup :1;
323 uint32_t gdetcfgloadsup :1;
324 uint32_t gdettrimsup :1;
325 uint32_t :10;
326 } bits;
327 } mcuxClCss_HwConfig_t;
328
329 #define drbgreqsub drbgreqsup
330
331
332
337 /**********************************************
338 * FUNCTIONS
339 **********************************************/
359 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetHwVersion)
360 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetHwVersion(
361 mcuxClCss_HwVersion_t * result
362 );
363
375 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetHwConfig)
376 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetHwConfig(
377 mcuxClCss_HwConfig_t * result
378 );
379
391 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetHwState)
392 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetHwState(
393 mcuxClCss_HwState_t * result
394 );
395
407 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_Enable_Async)
408 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_Enable_Async(
409 void
410 );
411
436 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_Reset_Async)
437 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_Reset_Async(
438 mcuxClCss_ResetOption_t options
439 );
440
452 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_Disable)
453 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_Disable(
454 void
455 );
456
468 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_SetIntEnableFlags)
469 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_SetIntEnableFlags(
470 mcuxClCss_InterruptOptionEn_t options
471 );
472
484 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetIntEnableFlags)
485 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetIntEnableFlags(
486 mcuxClCss_InterruptOptionEn_t * result
487 );
488
500 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_ResetIntFlags)
501 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_ResetIntFlags(
502 mcuxClCss_InterruptOptionRst_t options
503 );
504
516 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_SetIntFlags)
517 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_SetIntFlags(
518 mcuxClCss_InterruptOptionSet_t options
519 );
520
538 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_WaitForOperation)
539 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_WaitForOperation(
540 mcuxClCss_ErrorHandling_t errorHandling
541 );
542
564 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_LimitedWaitForOperation)
565 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_LimitedWaitForOperation(
566 uint32_t counterLimit,
567 mcuxClCss_ErrorHandling_t errorHandling
568 );
569
579 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_ResetErrorFlags)
580 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_ResetErrorFlags(
581 void);
582
596 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetErrorCode)
597 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetErrorCode(
598 mcuxClCss_ErrorHandling_t errorHandling
599 );
600
616 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetErrorLevel)
617 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetErrorLevel(
618 mcuxClCss_ErrorHandling_t errorHandling,
619 uint32_t *errorLevel
620 );
621
635 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_SetRandomStartDelay)
636 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_SetRandomStartDelay(
637 uint32_t delay
638 );
639
653 MCUX_CSSL_FP_FUNCTION_DECL(mcuxClCss_GetRandomStartDelay)
654 MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetRandomStartDelay(
655 uint32_t * delay
656 );
657
658
659
660
661
662
663
664
665
666 #endif /* MCUXCLCSS_COMMON_H_ */
667
mcuxClCss_GetHwVersion
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetHwVersion(mcuxClCss_HwVersion_t *result)
Determines the version of the underlying CSS hardware IP.
mcuxClCss_GetIntEnableFlags
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetIntEnableFlags(mcuxClCss_InterruptOptionEn_t *result)
Get interrupt enable flags.
mcuxClCss_HwState_t::prngready
uint32_t prngready
CSS PRNG is seeded and ready to use.
Definition: mcuxClCss_Common.h:211
MCUXCLCSS_API
#define MCUXCLCSS_API
Marks a function as a public API function of the mcuxClCss component.
Definition: mcuxClCss_Common.h:40
mcuxClCss_HwState_t::dtrng_busy
uint32_t dtrng_busy
Indicates the DTRNG is gathering entropy.
Definition: mcuxClCss_Common.h:215
mcuxClCss_InterruptOptionRst_t
Type to control which CSS interrupts should be reset when calling mcuxClCss_ResetIntFlags.
Definition: mcuxClCss_Common.h:259
mcuxClCss_HwVersion_t::value
uint32_t value
Accesses the bit field as a full word.
Definition: mcuxClCss_Common.h:183
mcuxClCss_HwConfig_t::keyprovsup
uint32_t keyprovsup
Indicates whether the keyprov command is supported.
Definition: mcuxClCss_Common.h:312
mcuxClCss_HwConfig_t::authciphersup
uint32_t authciphersup
Indicates whether the auth_cipher command is supported.
Definition: mcuxClCss_Common.h:304
mcuxClCss_HwConfig_t::gdettrimsup
uint32_t gdettrimsup
Indicates whether the gdet_trim command is supported.
Definition: mcuxClCss_Common.h:324
mcuxClCss_HwConfig_t::ciphersup
uint32_t ciphersup
Indicates whether the cipher command is supported.
Definition: mcuxClCss_Common.h:303
mcuxClCss_HwState_t::pprot
uint32_t pprot
The privilege/security level of the most recently started CSS command (For possible values of this fi...
Definition: mcuxClCss_Common.h:213
mcuxClCss_HwState_t::value
uint32_t value
Accesses the bit field as a full word.
Definition: mcuxClCss_Common.h:204
mcuxClCss_HwConfig_t::keyoutsup
uint32_t keyoutsup
Indicates whether the keyout command is supported.
Definition: mcuxClCss_Common.h:310
mcuxClCss_HwConfig_t::dtrngevalsup
uint32_t dtrngevalsup
Indicates whether the dtrng_eval command is supported.
Definition: mcuxClCss_Common.h:322
mcuxClCss_HwState_t
Result type of mcuxClCss_GetHwState.
Definition: mcuxClCss_Common.h:200
mcuxClCss_SetRandomStartDelay
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_SetRandomStartDelay(uint32_t delay)
Set the random start delay for AES based operations.
mcuxClCss_HwVersion_t::major
uint32_t major
Major version.
Definition: mcuxClCss_Common.h:189
mcuxClCss_Disable
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_Disable(void)
Disable the CSSv2.
mcuxClCss_GetHwConfig
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetHwConfig(mcuxClCss_HwConfig_t *result)
Determines the hardware configuration of the underlying CSS hardware IP.
mcuxClCss_LimitedWaitForOperation
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_LimitedWaitForOperation(uint32_t counterLimit, mcuxClCss_ErrorHandling_t errorHandling)
Await the completion of a CSS operation for a limited amount of time and optionally clear the error s...
mcuxClCss_HwConfig_t::drbgtestsup
uint32_t drbgtestsup
Indicates whether the drbg_test command is supported.
Definition: mcuxClCss_Common.h:320
mcuxClCss_InterruptOptionRst_t::cssint
uint32_t cssint
Whether CSS interrupt should be reset. (For possible values of this field, see mcuxClCss_InterruptOpt...
Definition: mcuxClCss_Common.h:267
mcuxClCss_HwConfig_t::eckxchsup
uint32_t eckxchsup
Indicates whether the dhkey_xch command is supported.
Definition: mcuxClCss_Common.h:307
mcuxClCss_ResetErrorFlags
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_ResetErrorFlags(void)
Resets all error flags that have been set by a previous operation.
mcuxClCss_HwConfig_t::hkdfsup
uint32_t hkdfsup
Indicates whether the hkdf command is supported.
Definition: mcuxClCss_Common.h:314
mcuxClCss_HwVersion_t::revision
uint32_t revision
Revision number.
Definition: mcuxClCss_Common.h:187
mcuxClCss_Types.h
CSSv2 type header.
mcuxClCss_ErrorHandling_t
uint32_t mcuxClCss_ErrorHandling_t
Type to handle CSS error clearing options.
Definition: mcuxClCss_Common.h:228
mcuxClCss_HwConfig_t::drbgreqsup
uint32_t drbgreqsup
Indicates whether the drbg_req command is supported.
Definition: mcuxClCss_Common.h:319
mcuxClCss_GetRandomStartDelay
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetRandomStartDelay(uint32_t *delay)
Get the random start delay for AES based operations.
mcuxClCss_HwConfig_t::value
uint32_t value
Accesses the bit field as a full word.
Definition: mcuxClCss_Common.h:299
mcuxClCss_HwConfig_t::ecsignsup
uint32_t ecsignsup
Indicates whether the ecsign command is supported.
Definition: mcuxClCss_Common.h:305
mcuxClCss_HwState_t::drbgentlvl
uint32_t drbgentlvl
Entropy quality of the current DRBG instance (For possible values of this field, see MCUXCLCSS_STATUS...
Definition: mcuxClCss_Common.h:214
mcuxClCss_GetErrorCode
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetErrorCode(mcuxClCss_ErrorHandling_t errorHandling)
Get the last CSS error code and optionally clear the error status.
mcuxClCss_InterruptOptionSet_t
Type to control which CSS interrupts should be set when calling mcuxClCss_SetIntFlags.
Definition: mcuxClCss_Common.h:276
mcuxClCss_HwConfig_t::kdeletesup
uint32_t kdeletesup
Indicates whether the kdelete command is supported.
Definition: mcuxClCss_Common.h:311
mcuxClCss_HwConfig_t::hmacsup
uint32_t hmacsup
Indicates whether the hmac command is supported.
Definition: mcuxClCss_Common.h:317
mcuxClCss_HwConfig_t::keyinsup
uint32_t keyinsup
Indicates whether the keyin command is supported.
Definition: mcuxClCss_Common.h:309
mcuxClCss_HwState_t::irq
uint32_t irq
CSS interrupt activated.
Definition: mcuxClCss_Common.h:209
mcuxClCss_HwVersion_t::minor
uint32_t minor
Minor version.
Definition: mcuxClCss_Common.h:188
mcuxClCss_HwConfig_t::tlsinitsup
uint32_t tlsinitsup
Indicates whether the tls_init command is supported.
Definition: mcuxClCss_Common.h:315
mcuxClCss_HwConfig_t::ecvfysup
uint32_t ecvfysup
Indicates whether the ecvfy command is supported.
Definition: mcuxClCss_Common.h:306
mcuxClCss_HwConfig_t::hashsup
uint32_t hashsup
Indicates whether the hash command is supported.
Definition: mcuxClCss_Common.h:316
mcuxClCss_HwConfig_t::keygensup
uint32_t keygensup
Indicates whether the keygen command is supported.
Definition: mcuxClCss_Common.h:308
mcuxClCss_HwVersion_t::level
uint32_t level
Release level version.
Definition: mcuxClCss_Common.h:190
mcuxClCss_HwConfig_t::dtrgncfgloadsup
uint32_t dtrgncfgloadsup
Indicates whether the dtrng_cfg_load command is is supported.
Definition: mcuxClCss_Common.h:321
mcuxClCss_HwState_t::busy
uint32_t busy
CSS is busy.
Definition: mcuxClCss_Common.h:208
mcuxClCss_HwConfig_t::ckdfsup
uint32_t ckdfsup
Indicates whether the ckdf command is supported.
Definition: mcuxClCss_Common.h:313
mcuxClCss_HwConfig_t
Result type of mcuxClCss_GetHwConfig.
Definition: mcuxClCss_Common.h:295
mcuxClCss_HwConfig_t::gdetcfgloadsup
uint32_t gdetcfgloadsup
Indicates whether the gdet_cfg_load command is supported.
Definition: mcuxClCss_Common.h:323
mcuxClCss_GetErrorLevel
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetErrorLevel(mcuxClCss_ErrorHandling_t errorHandling, uint32_t *errorLevel)
Get the last CSS error code and level and optionally clear the error status.
mcuxClCss_InterruptOptionEn_t::value
uint32_t value
Accesses the bit field as a full word.
Definition: mcuxClCss_Common.h:246
mcuxClCss_HwVersion_t
Result type of mcuxClCss_GetHwVersion.
Definition: mcuxClCss_Common.h:179
mcuxClCss_SetIntFlags
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_SetIntFlags(mcuxClCss_InterruptOptionSet_t options)
Set the interrupt status register, for debug and testing purposes.
mcuxClCss_GetHwState
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_GetHwState(mcuxClCss_HwState_t *result)
Determines the current state of the CSS.
mcuxClCss_InterruptOptionEn_t
Command option type for mcuxClCss_SetIntEnableFlags and mcuxClCss_GetIntEnableFlags.
Definition: mcuxClCss_Common.h:242
mcuxClCss_WaitForOperation
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_WaitForOperation(mcuxClCss_ErrorHandling_t errorHandling)
Wait for a CSS operation and optionally clear the error status.
mcuxClCss_ResetIntFlags
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_ResetIntFlags(mcuxClCss_InterruptOptionRst_t options)
Clear the interrupt status register.
mcuxCsslFlowProtection.h
Provides the API for the CSSL flow protection mechanism.
mcuxClCss_InterruptOptionSet_t::value
uint32_t value
Accesses the bit field as a full word.
Definition: mcuxClCss_Common.h:280
mcuxClCss_SetIntEnableFlags
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_SetIntEnableFlags(mcuxClCss_InterruptOptionEn_t options)
Set interrupt enable flags.
mcuxClCss_HwState_t::ecdsavfy
uint32_t ecdsavfy
ECDSA verify operation state (For possible values of this field, see MCUXCLCSS_STATUS_ECDSAVFY_)
Definition: mcuxClCss_Common.h:212
mcuxClCss_InterruptOptionSet_t::cssint
uint32_t cssint
Whether CSS interrupt should be set. (For possible values of this field, see mcuxClCss_InterruptOptio...
Definition: mcuxClCss_Common.h:284
mcuxClCss_ResetOption_t
uint32_t mcuxClCss_ResetOption_t
Type to handle CSS reset options.
Definition: mcuxClCss_Common.h:235
mcuxClCss_Enable_Async
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_Enable_Async(void)
Enables the CSS.
mcuxClCss_InterruptOptionEn_t::cssint
uint32_t cssint
Whether CSS interrupt should be used. (For possible values of this field, see mcuxClCss_InterruptOpti...
Definition: mcuxClCss_Common.h:250
mcuxClCss_HwConfig_t::cmacsup
uint32_t cmacsup
Indicates whether the cmac command is supported.
Definition: mcuxClCss_Common.h:318
MCUX_CSSL_FP_FUNCTION_DECL
#define MCUX_CSSL_FP_FUNCTION_DECL(id)
Declaration of a flow protected function.
Definition: mcuxCsslFlowProtection.h:119
mcuxClCss_Reset_Async
MCUXCLCSS_API mcuxClCss_Status_Protected_t mcuxClCss_Reset_Async(mcuxClCss_ResetOption_t options)
Perform a synchronous reset of the CSS.
mcuxClCss_Status_Protected_t
uint64_t mcuxClCss_Status_Protected_t
Type for CSS driver protected status codes.
Definition: mcuxClCss_Types.h:183
mcuxClCss_InterruptOptionRst_t::value
uint32_t value
Accesses the bit field as a full word.
Definition: mcuxClCss_Common.h:263
mcuxClCss_HwState_t::err
uint32_t err
CSS is in error state.
Definition: mcuxClCss_Common.h:210