<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Adc</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Adc</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Adc</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-POST-BUILD</IMPLEMENTATION-CONFIG-VARIANT>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>AdcConfigSet_0</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>AdcDigitalFilterLength</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcDigitalFilterLength</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcDigitalFilterLength/AdcDigitalFilterLength0</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcDigitalFilterLength/AdcDigitalFilterLength1</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>AdcHwUnit_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcCalibration</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcClockSource</DEFINITION-REF>
                      <VALUE>CLK_SRC_0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcExternalMultiplexing</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcHwUnitId</DEFINITION-REF>
                      <VALUE>ADC0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcLogicalUnitId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcPrescale</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcResolution</DEFINITION-REF>
                      <VALUE>BITS_12</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcTransferType</DEFINITION-REF>
                      <VALUE>ADC_INTERRUPT</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>AdcChannel_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcChannel</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcChannel/AdcChannelCalibration</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcChannel/AdcChannelId</DEFINITION-REF>
                          <VALUE>AN_0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcChannel/AdcChannelResolution</DEFINITION-REF>
                          <VALUE>12</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcChannel/AdcChannelSampTime</DEFINITION-REF>
                          <VALUE>3</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcChannel/AdcLogicalChannelId</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>AdcGroup_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcEnableDoubleBuffering</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcEnableHalfInterrupt</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupAccessMode</DEFINITION-REF>
                          <VALUE>ADC_ACCESS_MODE_SINGLE</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupConversionMode</DEFINITION-REF>
                          <VALUE>ADC_CONV_MODE_ONESHOT</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupConversionType</DEFINITION-REF>
                          <VALUE>ADC_CONV_TYPE_NORMAL</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupFifo</DEFINITION-REF>
                          <VALUE>ADC_FIFO_0</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupId</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupPriority</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupTriggSrc</DEFINITION-REF>
                          <VALUE>ADC_TRIGG_SRC_SW</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcHwTrigSrc</DEFINITION-REF>
                          <VALUE>FIFO0_RTI</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-FUNCTION-NAME-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcNotification</DEFINITION-REF>
                          <VALUE>NULL_PTR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-TEXTUAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcStreamingBufferMode</DEFINITION-REF>
                          <VALUE>ADC_STREAM_BUFFER_LINEAR</VALUE>
                        </ECUC-TEXTUAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcStreamingNumSamples</DEFINITION-REF>
                          <VALUE>1</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcWithoutInterrupts</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Adc/AdcConfigSet/AdcHwUnit/AdcGroup/AdcGroupDefinition</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Adc/Adc/AdcConfigSet_0/AdcHwUnit_0/AdcChannel_0</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>AdcDemEventParameterRefs</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcDemEventParameterRefs</DEFINITION-REF>
              <REFERENCE-VALUES>
                <ECUC-REFERENCE-VALUE>
                  <DEFINITION-REF DEST="ECUC-SYMBOLIC-NAME-REFERENCE-DEF">/TS_T2D41M10I0R0/Adc/AdcDemEventParameterRefs/ADC_E_TIMEOUT</DEFINITION-REF>
                  <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dem/Dem/DemConfigSet_0/ADC_E_TIMEOUT</VALUE-REF>
                </ECUC-REFERENCE-VALUE>
              </REFERENCE-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>AdcGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcConvTimeout</DEFINITION-REF>
                  <VALUE>65535</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcDeInitApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcEnableLimitCheck</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcEnableQueuing</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcEnableStartStopGroupApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcGrpNotifCapability</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcHwTriggerApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcPriorityImplementation</DEFINITION-REF>
                  <VALUE>ADC_PRIORITY_NONE</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcPriorityQueueMaxDepth</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcReadGroupApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcResultAlignment</DEFINITION-REF>
                  <VALUE>ADC_ALIGN_RIGHT</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcTimeout</DEFINITION-REF>
                  <VALUE>65535</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcGeneral/AdcVersionInfoApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>AdcPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AdcPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcPublishedInformation/AdcChannelValueSigned</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcPublishedInformation/AdcGroupFirstChannelFixed</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AdcPublishedInformation/AdcMaxChannelResolution</DEFINITION-REF>
                  <VALUE>12</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>AutosarExt</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcDisableDemReportErrorStatus</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcEnableCalibration</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcEnableDoubleBufferingOptimization</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcEnableDualClockMode</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcEnableGroupDependentChannelNames</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Adc/AutosarExt/AdcOptimizeOneShotHwTriggerConversions</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>3</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>123</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Adc/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
