<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:b29f2c08-0514-4b78-8757-9cd197ea3150">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:032b6h33-3415-4410-a59b-a903c0egfa2d">
          <SHORT-NAME>Mcl_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Mcl</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:b750487e-a7d6-48f5-a05a-d25be733d971">
          <SHORT-NAME>Mcl</SHORT-NAME>
          <DESC>
            <L-2 L="EN">Vendor specific: Configuration of the Mcl (MicroController Library ) module.</L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.6.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2014-10-31</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:967c3e2b-7845-4bc8-848f-e0a6291bf4d0">
              <SHORT-NAME>MclGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">Vendor specific: Configuration of general Mcl parameters.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9936de9b-1261-4720-9e80-145e3870a2cb">
                  <SHORT-NAME>MclDisableDemReportErrorStatus</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enable/Disable Dem error reporting.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:d8897d9d-1ae0-4020-85fc-70dfeb9f28fe">
                  <SHORT-NAME>MclDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Switches the Development Error Detection and Notification on or off.
                                            
                                                true: Enabled.
                                                false: Disabled.
                                            
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:3d5a31fa-1f07-473c-a834-28de454e98d5">
                  <SHORT-NAME>MclDmaNotificationSupported</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> This parameter is obsolete. The newly added MclIsrAvailable configures the interrupts available.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:5bc9853b-1050-4c44-8d22-909a3f601ec4">
                  <SHORT-NAME>MclErrorChecking</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific:
                                
                                    Vendor specific: Switch to indicate if the error user notification is supported.
                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:42da3770-7248-47fd-b1a8-8986ca635060">
                  <SHORT-NAME>Mcl_VersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Enables/Disables the get version info API function</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:42da3770-7248-47fd-b1a8-8986ca635033">
                  <SHORT-NAME>Mcl_DmaGetChannelErrorStatusApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Enables/Disables the get channel error status API Mcl_DmaGetChannelErrorStatus</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:42da4570-7248-47fd-b1a8-8986ca635033">
                  <SHORT-NAME>Mcl_DmaGetGlobalErrorStatusApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Enables/Disables the get global error status API Mcl_DmaGetGlobalErrorStatus</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c2a44725-ca66-4165-9aa8-dc51d263ef72">
                  <SHORT-NAME>Mcl_DeInitApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Enables/Disables the Mcl_DeInit API</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d28c1d-9311-41a5-ba35-40021a249a75">
                  <SHORT-NAME>EnableDMA</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific: Activates/Deactivates DMA configuration. DMA configuration must be enabled here.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:85d28c1d-9311-41a5-ba35-40021a249a75">
                  <SHORT-NAME>MclEnableCrossbarSwitch</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific: Activates/Deactivates Crossbar Switch configuration</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:fdf29f83-dbae-4cd2-abf2-c0941851a05e">
                  <SHORT-NAME>MclEnableUserModeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                When this parameter is enabled, the MCL module will adapt to run from User Mode, with the following measures:
                                                b) using 'call trusted function' stubs for all internal function calls that access registers requiring supervisor mode.
                                                for more information, please see chapter 5.7 User Mode Support in IM 
                                                Note: Implementation Specific Parameter.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:fdf23f83-dbae-4cd2-abf2-c0941851a05e">
                  <SHORT-NAME>EnableSemaphoreSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            When this parameter is enabled, the Semaphore APIs are enabled to the user.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:69223E7A-8051-4241-A982-2C56D70C96DF">
                  <SHORT-NAME>CoreUsed</SHORT-NAME>
                  <DESC>
                    <L-2 L="FOR-ALL">
                                                Core that's used in the driver for semaphore and cache operations.
                                                NOTE: It must be selected by the user to match the core that the code runs on.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:89eea1f4-7523-11e8-adc0-fa7ae01bbebc">
                  <SHORT-NAME>MclEnableLogicalAddress</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                When this parameter is enabled, the MCL module will adapt to run with logical address:
                                                Note: Implementation Specific Parameter.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:c5326d00-5f70-500e-90c4-36a4df202b6f">
                  <SHORT-NAME>MclErrorNotification</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                    User callback function for an error which does not belong to any Dma channel.
                                    Ex: Synchronize cache failed when calling &quot;DMA start channel&quot; function.
                                    NOTE: please use NULL or NULL_PTR w/o any quotes. If the used string is different from NULL
                                    or NULL_PTR it will be used as the configured function name.
                                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
              </PARAMETERS>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:04ac838a-72f5-480b-b9ec-cc43a5100e5b">
                  <SHORT-NAME>MclIsrAvailable</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                             Vendor specific:
                                            Mcl ISRs Available.Please check the ISRs which are needed for the application.
                                            Warning: This is a precompile configuration.If you uncheck a ISR, you will not be able to enable the 
                                            respective channel or error functionality at post build time.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>128</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>128</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:00a8505c-39fd-499a-9b7f-acf75976173b">
                      <SHORT-NAME>MclIsrName</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                Mcl Interrupt Name.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>eDMA_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_8</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_9</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_10</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_11</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_12</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_13</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_14</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_15</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_24</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_25</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_26</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_27</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_28</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_29</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_30</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_31</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_32</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_33</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_34</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_35</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_36</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_37</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_38</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_39</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_40</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_41</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_42</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_43</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_44</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_45</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_46</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_47</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_48</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_49</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_50</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_51</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_52</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_53</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_54</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_55</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_56</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_57</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_58</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_59</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_60</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_61</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_62</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_63</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_64</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_65</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_66</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_67</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_68</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_69</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_70</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_71</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_72</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_73</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_74</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_75</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_76</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_77</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_78</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_79</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_80</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_81</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_82</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_83</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_84</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_85</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_86</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_87</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_88</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_89</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_90</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_91</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_92</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_93</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_94</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_95</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_96</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_97</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_98</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_99</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_100</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_101</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_102</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_103</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_104</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_105</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_106</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_107</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_108</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_109</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_110</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_111</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_112</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_113</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_114</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_115</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_116</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_117</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_118</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_119</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_120</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_121</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_122</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_123</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_124</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_125</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_126</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_127</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:e1524282-63e7-4426-bfb8-590fd3d096d6">
                      <SHORT-NAME>MclIsrEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific: Switch to indicate if the interrupt is enabled 
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:b181c056-c89a-4dfb-b4e4-82717666b9f1">
              <SHORT-NAME>MclDemEventParameterRefs</SHORT-NAME>
              <DESC>
                <L-2 L="EN"> Vendor specific:
                                                Container for the references to DemEventParameter elements which shall be 
                                                invoked using the API Dem_SetEventStatus in case the corresponding error occurs. 
                                                The EventId is taken from the referenced DemEventParameter/DemEventId value.
                                                </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <REFERENCES>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:70c4dc1d-3618-4412-b231-9c7d0d9ad78d">
                  <SHORT-NAME>MCL_E_DMA_DESCRIPTOR</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when a descriptor error occurs</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:48d44ebc-e362-48b6-869a-df2b1bd4abdc">
                  <SHORT-NAME>MCL_E_DMA_ECC</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when an unrecoverable ECC error occured</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:b367f8f7-ad1d-458e-8e87-6f57ab58b165">
                  <SHORT-NAME>MCL_E_DMA_BUS</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when a bus error occured.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:67c39b2d-4477-466e-b96b-cd1a6d7492c6">
                  <SHORT-NAME>MCL_E_DMA_PRIORITY</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when a descriptor error occurs</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:67c39b2d-4588-466e-b96b-cd1a6d7492c6">
                  <SHORT-NAME>MCL_E_DMA_INCONSISTENCY</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when a descriptor error occurs</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:67c39b2d-4477-466e-b96b-cd1a6d8882c6">
                  <SHORT-NAME>MCL_E_DMA_UNRECOGNIZED</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when a descriptor error occurs</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:b824a41e-5f5e-48b6-9c71-0e63b429c3da">
              <SHORT-NAME>MclConfigSet</SHORT-NAME>
              <DESC>
                <L-2 L="EN"> Vendor specific: This container is the base for a multiple configuration set
                                        </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5d10957b-c38a-45ed-b06b-4b7e365f1cc3">
                  <SHORT-NAME>DmaInstance</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Configuration of a DMA Instance.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>3</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:f7cbd8ea-f1bc-41a1-ad0a-e9f4015cf1e5">
                      <SHORT-NAME>DmaHwInstance</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                Select the physical eDMA Instance.
                                                NOTE: This is an Implementation Specific Parameter.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>eDMA_Instance0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_Instance0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_Instance1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:f2ced8ea-f1bc-41a1-ad0a-e9f4015cf1e5">
                      <SHORT-NAME>DmaHwInstanceVersion</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                Select the version type of eDMA Instance.
                                                NOTE: This is an Implementation Specific Parameter.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>eDMA_v2</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_v2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:244bee90-b361-4d1b-9092-37ac333b32c7">
                      <SHORT-NAME>MclEDMA_CX</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[CX].
                                                        Cancel Transfer.
                                                        0 - Normal operation.
                                                        1 - Cancel the remaining data transfer. 
                                                               Stop the executing channel and force the minor loop to be finished. 
                                                               The cancel takes effect after the last write of the current read/write sequence. 
                                                               The CXFR bit clears itself after the cancel has been honored. 
                                                               This cancel retires the channel normally as if the minor loop was completed.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c1adfc64-6ce4-4378-ad5b-f6b5e1778a6c">
                      <SHORT-NAME>MclEDMA_ECX</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[ECX].
                                                        Error Cancel Transfer.
                                                        0 - Normal operation.
                                                        1 - Cancel the remaining data transfer in the same fashion as the CX cancel transfer. 
                                                               Stop the executing channel and force the minor loop to be finished. 
                                                               The cancel takes effect after the last write of the current read/write sequence. 
                                                               The ECX bit clears itself after the cancel cancel has been honored. 
                                                               In addition to cancelling the transfer, the ECX treats the cancel as an error condition; 
                                                               thus updating the DMAES register and generating an optional error interrupt.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c1adfc64-6df4-4378-ad5b-f6b5e1778a6c">
                      <SHORT-NAME>MclEDMA_EBW</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[ECX].
                                                        Enable buffer writes. The parameter is vailable only for eDMA3 modules. 
                                                        0 - Buffered writes on the system bus are disabled.
                                                        1 - The bufferable write signal is asserted on all system bus writes except during the last write sequence.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c1adfc64-6df4-4378-ad5b-f6b5aa778a6c">
                      <SHORT-NAME>MclEDMA_GMRC</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CSR[GMRC].Available only for eDMA3 instances.
                                                        Global master ID replication control
                                                        0 - Master ID replication is disabled for all channels
                                                        1 - Master ID replication is available and it is controlled by each channel's CHn_SBR[EMI] setting.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:57e011aa-0227-46d2-95b9-1ad432d12b66">
                      <SHORT-NAME>MclEDMAChGroup0Priority</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[GRP0PRI] field configuration.
                                                        Group 0 priority level when fixed priority group arbitration is enabled.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>3</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:07a7cb8f-4feb-4067-bbf7-e18e4a75406f">
                      <SHORT-NAME>MclEDMAChGroup1Priority</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[GRP1PRI] field configuration.
                                                        Group 1 priority level when fixed priority group arbitration is enabled.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>3</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:895b9b77-9484-4bd6-9493-831e8aa6f58d">
                      <SHORT-NAME>MclEDMAChGroup2Priority</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[GRP2PRI] field configuration.
                                                        Group 2 priority level when fixed priority group arbitration is enabled.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>2</DEFAULT-VALUE>
                      <MAX>3</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:52c458c1-577c-42e2-b4b4-d77cc79662e7">
                      <SHORT-NAME>MclEDMAChGroup3Priority</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[GRP3PRI] field configuration.
                                                        Group 3 priority level when fixed priority group arbitration is enabled.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>3</DEFAULT-VALUE>
                      <MAX>3</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:b595ac4b-65a7-431c-a948-37bea8c36302">
                      <SHORT-NAME>MclEDMA_CLM</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[CLM].
                                                        Continuous Link Mode.
                                                        0 - A minor loop channel link made to itself will go through channel arbitration before being activated again.
                                                        1 - A minor loop channel link made to itself will not go through channel arbitration before being activated again. 
                                                               Upon minor loop completion the channel will active again if that channel has has a minor loop channel link enabled and the link channel is itself.
                                                               This effectively applies the minor loop offsets and restarts the next minor loop.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:dd63275d-22f0-4ba3-b64b-f29b8ea667f5">
                      <SHORT-NAME>MclEDMA_GCLC</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[GCLC].
                                                        Global Channel Linking Control.
                                                        0 - Channel linking is disabled for all channels.
                                                        1 - Channel linking is available and controlled by each channel's link settings.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ba1a826e-eaa0-4975-a20e-b754d1f7261f">
                      <SHORT-NAME>MclEDMA_HALT</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[HALT].
                                                        Halt eDMA Operations.
                                                        0 - Normal operation.
                                                        1 - Stall the start of any new channels. 
                                                               Executing channels are allowed to complete. 
                                                               Channel execution will resume when the HALT bit is cleared.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:cce36948-aa6d-419c-ae97-a483c133fe6c">
                      <SHORT-NAME>MclEDMA_HOE</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[HOE] for eDMA2 instances or DMA_CSR[HAE] for eDMA3 instances.
                                                        Halt On/After Error.
                                                        0 - Normal operation.
                                                        1 - Any error will cause the HALT bit to be set.
                                                               Subsequently, all service requests will be ignored until the HALT bit is cleared.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:eccbc35d-355b-477e-9c71-f2b7a440de8d">
                      <SHORT-NAME>MclEDMA_ERGA</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[ERGA].
                                                        Enable Round Robin Group Arbitration.
                                                        0 - Fixed priority arbitration is used for selection among the groups.
                                                        1 - Round robin arbitration is used for selection among the groups.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:b7ee1249-087c-42f7-be8b-3233fb220cfc">
                      <SHORT-NAME>MclEDMA_ERCA</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[ERCA].
                                                        Enable Round Robin Channel Arbitration.
                                                        0 - Fixed-priority arbitration is used for channel selection within each group.
                                                        1 - Round-Robin arbitration is used for channel selection within each group.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:feb20843-4496-4542-8956-ab9a45086f8a">
                      <SHORT-NAME>MclEDMA_EDBG</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        DMA_CR[EDBG].
                                                        Enable Debug.
                                                        0 - The assertion of the system debug control input is ignored.
                                                        1 - The assertion of the system debug control input causes the eDMA to stall the start of a new channel. 
                                                               Executing channels are allowed to complete. 
                                                               Channel execution will resume when either the system debug control input is negated or the EDBG bit is cleared.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:04ac837b-72f5-480b-b9ec-cc43a5100e5b">
                  <SHORT-NAME>DMAChannel</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                             Vendor specific:
                                            All data needed to configure one DMA channel.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>128</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e621be28-bb23-41dc-803b-5a40d1ba1318">
                      <SHORT-NAME>MclDMAChannelId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                        Id for the current DMA logical Channel.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>127</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:0aff248e-f32e-42b6-94be-372ca32a5726">
                      <SHORT-NAME>DmaHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                Select the physical eDMA Channel.
                                                NOTE: This is an Implementation Specific Parameter.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>eDMA_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_8</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_9</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_10</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_11</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_12</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_13</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_14</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_15</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_24</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_25</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_26</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_27</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_28</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_29</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_30</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_31</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_32</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_33</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_34</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_35</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_36</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_37</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_38</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_39</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_40</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_41</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_42</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_43</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_44</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_45</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_46</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_47</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_48</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_49</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_50</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_51</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_52</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_53</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_54</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_55</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_56</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_57</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_58</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_59</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_60</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_61</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_62</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_63</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_64</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_65</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_66</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_67</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_68</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_69</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_70</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_71</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_72</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_73</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_74</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_75</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_76</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_77</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_78</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_79</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_80</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_81</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_82</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_83</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_84</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_85</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_86</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_87</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_88</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_89</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_90</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_91</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_92</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_93</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_94</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_95</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_96</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_97</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_98</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_99</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_100</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_101</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_102</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_103</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_104</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_105</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_106</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_107</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_108</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_109</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_110</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_111</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_112</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_113</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_114</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_115</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_116</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_117</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_118</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_119</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_120</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_121</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_122</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_123</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_124</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_125</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_126</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eDMA_127</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:c6cdae0c-ae94-4618-b593-06fcc5cc6367">
                      <SHORT-NAME>DMAChannelPriority</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                         Vendor specific: Priority level for DMA channel. Priorities assigned to channels from the same Group must be unique.
                                                         Please read section Enhanced Direct Memory Access (eDMA) from the manual for more information
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <!-- @Calculated /TS_T2D41M10I0R0/Mcl/MclConfigSet/DMAChannel/DMAChannelPriority: INVALID(XPath: (num:i(substring-after(node:value(../DmaHwChannel),&apos;eDMA_&apos;)) &lt; num:i((text:split(&apos;0&apos;,&apos; &apos;)[1]))) and (node:value(.)&lt;0 or node:value(.)&gt;7), (num:i(substring-after(node:value(../DmaHwChannel),&apos;eDMA_&apos;)) &gt;= num:i((text:split(&apos;0&apos;,&apos; &apos;)[1]))) and (node:value(.)&lt;0 or node:value(.)&gt;15))-->
                      <MAX>9223372036854775807</MAX>
                      <MIN>-9223372036854775808</MIN>
                      <!-- @CalculatedEnd -->
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:c6cdae0c-ae94-4623-b593-06fcc5cc6367">
                      <SHORT-NAME>DMAChannelGroupPriority</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                         Vendor specific: Priority group for DMA channel(CHn_GRPRI). The parameter is used only by channels starting from eDMA_0 up to eDMA_63.
                                                         Please read section Enhanced Direct Memory Access (eDMA3) from the hardware manual for more information
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>31</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6226a5b4-0c7c-4da2-a5df-65859769c65b">
                      <SHORT-NAME>ECP</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                         Vendor specific:
                                                        Enable channel preemption.
                                                         0 (unchecked) - Channel n cannot be suspended by a higher priority channel's service request
                                                         1 (checked)   - Channel n can be temporarily suspended by a higher priority channel's service request
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:0fd1b5ae-3281-4fea-b886-933369f355df">
                      <SHORT-NAME>DPA</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                         Vendor specific:
                                                        Disable preemptive ability.
                                                         0 (unchecked) - Channel n can suspen a lower priority channel
                                                         1 (checked)   - Channel n cannot suspend any channel, regardless of the channel's priority.
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7f875a72-0f89-4257-82d2-8c7140d49fc2">
                      <SHORT-NAME>EMI</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                         Vendor specific:
                                                        Enable Master ID replication.
                                                         0 (unchecked) - Master ID replication is disabled
                                                         1 (checked)   - Master ID replication is enabled
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-FUNCTION-NAME-DEF UUID="ECUC:c5326d00-5f70-49fe-90c4-36a4df202b63">
                      <SHORT-NAME>MclDmaTransferCompletionNotif</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                User callback function to report that the trasnfer is half or complete depending on configuration.
                                                NOTE: please use NULL or NULL_PTR w/o any quotes. If the used string is different from NULL
                                                or NULL_PTR it will be used as the configured function name.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                        <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                          <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                        </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    </ECUC-FUNCTION-NAME-DEF>
                    <ECUC-FUNCTION-NAME-DEF UUID="ECUC:c5326d00-5f70-500e-90c4-36a4df402b6f">
                      <SHORT-NAME>MclDmaTransferErrorNotif</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                               User callback function
                                               NOTE: please use NULL or NULL_PTR w/o any quotes. If the used string is different from NULL
                                               or NULL_PTR it will be used as the configured function name.
                                               </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                        <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                          <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                        </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    </ECUC-FUNCTION-NAME-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:04ac777b-72f5-480b-b9ec-cc43a5100e5b">
                  <SHORT-NAME>MclCrossbarLogicalSlavePorts</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                     Vendor specific:
                                    Data to configure the crossbar logical slave ports.
                                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>12</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e62115g8-bb23-41dc-983b-5a40d1ba1318">
                      <SHORT-NAME>MclCrossbarLogicalSlavePortId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                    Id for the current crossbar logical slave port
                                                    Note: Implementation Specific Parameter.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>15</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:2bb4117d-a963-550e-9fbb-e9f8740cbafe">
                      <SHORT-NAME>MclCrossbarHwSlavePortRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                            
                                            Select the hardware slave port reference.
                                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Mcl/MclConfigSet/MclCrossbarInstance/MclCrossbarHwSlavePort</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:04acfffb-73f5-480b-b9ec-cc43a5100e5b">
                  <SHORT-NAME>MclCrossbarLogicalMasterPorts</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                     Vendor specific:
                                    Data to configure the crossbar logical Master ports.
                                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>16</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e621be28-bb23-41dc-983b-5a40d1ba1318">
                      <SHORT-NAME>MclCrossbarLogicalMasterPortId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                                    Id for the current crossbar logical slave port
                                                    Note: Implementation Specific Parameter.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>15</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:2bb4117d-a963-572f-9fbb-e9f8740cbafe">
                      <SHORT-NAME>MclCrossbarHwMasterPortRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                            
                                            Select the hardware slave port reference.
                                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Mcl/MclConfigSet/MclCrossbarInstance/MclCrossbarHwMasterPort</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5d10957b-c38a-66ed-b06b-4b7e365f1cc3">
                  <SHORT-NAME>MclCrossbarInstance</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Configuration of a crossbar instance.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>2</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:0aaa248e-f32e-45b6-94be-372ca32a5726">
                      <SHORT-NAME>MclCrossbarHwInstance</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific:
                                            Select the physical crossbar instance.
                                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>AXBS_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>AXBS_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                  </PARAMETERS>
                  <SUB-CONTAINERS>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:762d3422-214a-550f-9f1a-61a2630520cf">
                      <SHORT-NAME>MclCrossbarHwSlavePort</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                            Hardware slave port configuration.
                                                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>8</UPPER-MULTIPLICITY>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b90b7537-4320-4954-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclSlavePortNumber</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Slave port number in hardware.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-4954-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster0</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master 0 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-4954-81a0-11c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster1</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master1 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-5054-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster2</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master2 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-5154-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster3</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master3 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-5254-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster4</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master4 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-5354-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster5</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master5 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-5454-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster6</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master6 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b89b7537-4320-5554-81a0-d0c4167fe36e">
                          <SHORT-NAME>MclCrossbarPrioMaster7</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                        Priority of the master7 on the cross bar.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>7</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c1d-9311-41a5-ba35-40021a249a75">
                          <SHORT-NAME>MclCrossbarEnableLock</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific: Locks the configuration registers for the respective slave port.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a5-ba35-40021a249a75">
                          <SHORT-NAME>MclCrossbarHaltLowPrio</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific: Sets the initial arbitration priority for low power mode requests. Setting this bit will not affect the request
                                            for low power mode from attaining highest priority once it has control of the slave ports. Disabled = The low power mode request has the highest priority for arbitration on this slave port;
                                            Enabled = The low power mode request has the lowest initial priority for arbitration on this slave port</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a75">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM0</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 0. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a76">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM1</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 1. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a77">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM2</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 2. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a78">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM3</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 3. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a79">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM4</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 4. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a7a">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM5</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 5. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a7b">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM6</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 6. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30c3d-9311-41a6-ba35-40021a249a7c">
                          <SHORT-NAME>MclCrossbarEnablePrioElevM7</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, enable priority elevation for master 7. If enabled, the master is able to elevate its priority
                                            to the highest.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72d30d3d-9311-41a6-ba35-40021a249a75">
                          <SHORT-NAME>MclCrossbarEnableFixedPrio</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Vendor specific:  On this slave port, select the arbitraion mode: if enabled the arbitration mode will be FIXED PRIORITY, if disabled it will be ROUND ROBIN.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:2e702c03-9a34-407f-9476-e14c2d713c75">
                          <SHORT-NAME>MclCrossbarParkingControl</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                                    
                                                    Determines the slave port?s parking control. The low-power park feature results in an overall power
                                                    savings if the slave port is not saturated; however, this forces an extra latency clock when any master tries
                                                    to access the slave port while not in use because it is not parked on any master.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ParkField</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ParkField</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>LastMaster</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>LowPowerPark</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:0aaa248e-f32e-45b6-97be-442ca32a5726">
                          <SHORT-NAME>MclCrossbarParkField</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                    Determines which master port the current slave port parks on when no masters are actively making requests and the MclCrossbarParkingControl=ParkField.
                                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>Master0</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master4</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master5</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master6</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>Master7</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                      </PARAMETERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:762d3422-214a-550f-9f1a-61a263052ccc">
                      <SHORT-NAME>MclCrossbarHwMasterPort</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                Hardware Master port configuration.
                                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>8</UPPER-MULTIPLICITY>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b90b7537-4320-4954-81a0-d0c4167fe333">
                          <SHORT-NAME>MclMasterPortNumber</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Vendor specific:
                                                    Master port number in hardware.
                                                </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>Freescale</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>8</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:2e702c03-9a34-407f-9476-e14c2d713c88">
                          <SHORT-NAME>MclCrossbarArbitrates</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                                
                                                Determines whether, and when, the crossbar switch arbitrates away the slave port the master owns when
                                                the master is performing undefined length burst accesses.
                                                    0 - No arbitration is allowed during an undefined length burst.
                                                    1 - Arbitration is allowed at any time during an undefined length burst.
                                                    2 - Arbitration is allowed after four beats of an undefined length burst.
                                                    3 - Arbitration is allowed after eight beats of an undefined length burst.
                                                    4 - Arbitration is allowed after 16 beats of an undefined length burst.
                                                </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>4</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                      </PARAMETERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                  </SUB-CONTAINERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:b37b96c6-7528-11e8-adc0-fa7ae01bbebc">
                  <SHORT-NAME>MclLogicalMemorySectionConfig</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                         Vendor specific:
                                        Data to configure Logical address and physical address.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b37b9964-7528-11e8-adc0-fa7ae01bbebc">
                      <SHORT-NAME>LogicalAddressStart</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                        This parameter represents the Logical Address Start.
                                                        The address must be aligned to 4 bytes.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b37b9aa4-7528-11e8-adc0-fa7ae01bbebc">
                      <SHORT-NAME>LogicalAddressEnd</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                        This parameter represents the Logical Address Start.
                                                        The address must be aligned to 4 bytes.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:145207b4-784e-11e8-adc0-fa7ae01bbebc">
                      <SHORT-NAME>PhysicalAddressStart</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                        This parameter represents the Physical Address Start.
                                                        The address must be aligned to 4 bytes.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:14520a3e-784e-11e8-adc0-fa7ae01bbebc">
                      <SHORT-NAME>PhysicalAddressEnd</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                        This parameter represents the Physical Address Start.
                                                        The address must be aligned to 4 bytes.
                                                        Note: Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:44919a79-b892-492e-a9ca-564bb60af38c">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN"> Vendor specific:
                                    Common container, aggregated by all modules. It contains published information about vendor and versions.
                                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:2a4dc367-722b-4ab8-8fa9-5abf36baef63">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:247a09d1-9463-492b-9be9-f1a925db120a">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:626a79b2-3f52-46ad-b609-6a985d61698b">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:efb0dbc4-d1ca-4374-b5c2-c2bf4bf93a05">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific:
                                        Module ID of this module from Module List.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>255</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>255</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:ccd5e5a9-6082-4267-ba3d-003be289c116">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d018972e-992d-4e6d-8c7c-cd4126e14d5e">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e3fb879e-f034-473e-9b52-837934896c40">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:9f393227-196a-42b8-a12e-337c0279f451">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        In driver modules which can be instantiated several times on a single ECU, BSW00347 requires 
                                        that the name of APIs is extended by the VendorId and a vendor specific name. 
                                        This parameter is used to specify the vendor specific name. In total, the 
                                        implementation specific name is generated as follows: &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt;.
                                        E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 
                                        This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:2e77dfe4-b371-4d6b-aaec-2e70169abc6d">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Vendor specific:
                                        Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>