<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:4af873de-a8cf-41ad-a857-11cca7dcd97a">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:86c29246-beb5-4384-b5dd-4cc6baac161a">
          <SHORT-NAME>Mcem_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Mcem</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:a8a495cc-11e9-459b-807f-0179efa09e77">
          <SHORT-NAME>Mcem</SHORT-NAME>
          <DESC>
            <L-2 L="EN">
                                 Mcem
                                 Configuration of the Mcem (Microcontroller error manager) module
                                 </L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.6.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2014-10-31</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:17517e42-6da8-437e-b057-35cc7f943c0e">
              <SHORT-NAME>McemGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                    McemGeneral
                                    All general parameters of the MCEM driver are collected here.
                                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9e744655-7df7-4a93-b826-65e7bf3760ad">
                  <SHORT-NAME>McemDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Mcem Development Error Detect
                                            Compile switch to enable / disable development error detection for this module.
                                            
                                            Unchecked: Development error detection disabled
                                            Checked  : Development error detection enabled 
                                            
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:22b5db0e-c172-4efb-a08b-8ffe218aa92a">
                  <SHORT-NAME>McemVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            MCEM VersionInfo Api
                                            Compile switch to enable / disable the version information API.
                                            
                                            Checked  : API enabled 
                                            Unchecked:API disabled 
                                            
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:0e089a82-6516-4e09-a6b5-859781abc8d8">
                  <SHORT-NAME>McemAlarmNotificationApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            MCEM Alarm Notification
                                            Compile switch to enable / disable the alarm notification .
                                            
                                            Checked  : Notification  enabled 
                                            Unchecked: Notification disabled 
                                            
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ae744656-7df7-4a93-b826-65e7bf3760ad">
                  <SHORT-NAME>McemDemExtendedData</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Mcem DEM Extended Data
                                            Compile switch to enable / disable reporting DEM extended data.
                                            
                                            Unchecked: Reporting DEM extended data disabled
                                            Checked  : Reporting DEM extended data enabled 
                                            
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:faa4800a-3714-4ef4-9a8b-457befc658cd">
                  <SHORT-NAME>McemEnableUserModeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        
                                            When this parameter is enabled, the MCEM module will adapt to run from User Mode, with the following measures:
                                            (if applicable) a) configuring REG_PROT for the MCEM registers so that the registers under protection can be accessed from user mode by setting UAA bit in REG_PROT_GCR to 1
                                            (if applicable) b) using 'call trusted function' stubs for all internal function calls that access registers requiring supervisor mode.
                                            (if applicable) c) other module specific measures for more information, please see chapter 5.7 User Mode Support in IM
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:a97ef180-0e66-4eeb-974d-8166ce6750b1">
              <SHORT-NAME>McemDemEventParameterRefs</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                         Container for the references to DemEventParameter elements which shall be 
                                         invoked using the API Serr_NotifyErrorEvent in case the corresponding error occurs. 
                                         The EventId is taken from the referenced DemEventParameter/DemEventId value.
                                         </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <REFERENCES>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:27d9fd11-b247-43a6-bfff-b36b67fb4fdd">
                  <SHORT-NAME>MCEM_E_INIT_FAILED</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the initialization function has failed.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:3fda88af-5143-4276-b8b8-a58cf5b7d256">
              <SHORT-NAME>McemConfigSet</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                    This container is the base for a multiple configuration set.
                                        </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:378b0655-d873-48a7-b3e7-9dd13005552e">
                  <SHORT-NAME>FccuGlitchFilterBypass</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            FCCU Glitch Filter Bypass.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:9889877e-7535-411c-875d-f66f6df20e29">
                  <SHORT-NAME>FccuGlitchFilterWidth</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            FCCU Glitch Filter Width
                                            
                                             Filters glitches of up to 50 us 
                                             Filters glitches of up to 75 us 
                                             Filters glitches of up to 100 us 
                                            
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>Up_To_50_us</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>Up_To_50_us</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>Up_To_75_us</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>Up_To_100_us</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1f40c244-6e74-494e-877e-9a7288eaecdc">
                  <SHORT-NAME>FaultTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                          Non-critical fault timeout. If the fault with enabled recovery timeout is not recovered 
                                          within the timeout period the FCCU moves from the ALARM state to the FAULT state.
                                          NCF timeout can be computed using the following equations:
                                          Timeout&amp;nbsp;=&amp;nbsp;TRC16MHz&amp;nbsp;&amp;times;&amp;nbsp;FaultTimeout
                                          Timeout&amp;nbsp;=&amp;nbsp;0.0625&amp;nbsp;&amp;times;&amp;nbsp;FaultTimeout&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;[&amp;mu;s]
                                          </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>65535</DEFAULT-VALUE>
                  <MAX>4294967295</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:16b5d888-ff9f-4df7-82a1-9858fc540475">
                  <SHORT-NAME>DeltaT</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                          In case of a failure event, the pin(s) are set to faulty state for a minimum time T_min, even if SW
                                            tries to release it before (for the case of error pin configured in Bistable mode only).
                                          T_min&amp;nbsp;=&amp;nbsp;250&amp;nbsp;&amp;mu;s&amp;nbsp;+&amp;nbsp;delta_T
                                          with delta_T parameter being configurable by SW up to 16,383&amp;nbsp;&amp;mu;s (10&amp;nbsp;ms).
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>16383</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:858cdd75-7dd4-4b6b-b6e2-5bde89cc0744">
                  <SHORT-NAME>ConfigTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> 
                                          If the configuration is not completed within the time-out, 
                                            the FCCU moves automatically from the CONFIG state to the NORMAL state and 
                                            the default values for the configuration register is restored.
                                          Configuration timeout can be computed using the following equation:
                                          Timeout&amp;nbsp;=&amp;nbsp;TRC16MHz&amp;nbsp;&amp;times;&amp;nbsp;2(ConfigTimeout&amp;nbsp;+&amp;nbsp;10)
                                          
                                            
                                              Value
                                              Timeout[&amp;mu;s]
                                              Value
                                              Timeout[&amp;mu;s]
                                            
                                            
                                              0
                                              64
                                              1
                                              128
                                            
                                            
                                              2
                                              256
                                              3
                                              512
                                            
                                            
                                              4
                                              1024
                                              5
                                              2048
                                            
                                            
                                              6
                                              4096
                                              7
                                              8192
                                            
                                          
                                          </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>6</DEFAULT-VALUE>
                  <MAX>7</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:9779877e-7535-411c-875d-f66f6df20e29">
                  <SHORT-NAME>EOUT_FaultOutputMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Fault Output Mode Selection
                                        
                                         Dual-Rail (default state) [fccu_eout[1:0]= outputs] 
                                         Time Switching [fccu_eout[1:0]= output to be used] 
                                         Bi-Stable 
                                        
                                         Note: In the Test mode, a simple double-stage resynchronization stage is used to resynchronize the EOUT input/outputs on the system/safe clock. 
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>EOUT_DualRail</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EOUT_DualRail</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EOUT_TimeSwitching</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EOUT_BiStable</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:9779877e-7355-411c-875d-f66f6df20e29">
                  <SHORT-NAME>EOUT_Prescaler</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Fault Output Prescaler configuration (applicable for Dual-Rail or Time-Switching mode only). When in Dual-Rail or Time-Switching mode, the togglling frequency of EOUT signal is calculated by the following equation: 
                                        EOUTfreq&amp;nbsp;=&amp;nbsp;CLK_SAFEfreq&amp;nbsp;&amp;divide;&amp;nbsp;((EOUT_Prescaler&amp;nbsp;+&amp;nbsp;1)&amp;times;&amp;nbsp;2&amp;nbsp;&amp;times;&amp;nbsp;2048&amp;nbsp;)
                                         Note: This value will not impact functional in BiStable mode. 
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>127</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:377b0655-c873-48a7-b3e7-9dd13005552e">
                  <SHORT-NAME>CfgToIrqEnabled</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Configuration Timeout Interrupt Enable.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:bbe1e60f-0e7c-402d-8068-e89799970f43">
                  <SHORT-NAME>McemHardlockedConfiguration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Hard-lock this configuration set: 
                                        
                                            Unchecked: After Mcem_Init, the configuration is not locked. 
                                            Checked: After Mcem_Init, the configuration is hardlocked. 
                                        
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:f8c348ee-b9ff-41c6-87ee-c182e9b87e25">
                  <SHORT-NAME>EOUT_SwitchingMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        EOUT Switching mode
                                        
                                        Unchecked: EOUT protocol (dual-rail, time-switching) slow switching mode. 
                                        Checked  : EOUT protocol (dual-rail, time-switching) fast switching mode. 
                                        
                                        Switching Mode has no effect on the bi-stable protocol.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:50970b86-6dfc-44d2-a0d8-3b533828790c">
                  <SHORT-NAME>EOUT_PolaritySelection</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        EOUT Polarity Selection
                                        
                                        Unchecked: fcc_eout[1] active high, fcc_eout[0] active low. 
                                        Checked: fcc_eout[1] active low, fcc_eout[0] active high. 
                                        
                                        This bit can be read and written by the software. Active state means a state indicating FAULT and 
                                        is applicable for non-toggling protocols only.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:f1167cd6-5eda-4d34-ac2d-a7250e7f52d9">
                  <SHORT-NAME>EOUT_AfterReset</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        This bit controls the enable of the error output pins after reset lifts:
                                        
                                        Unchecked: error pins move to HI-Z state.
                                        Checked  : start EOUT pins functioning.
                                        
                                        Unless is this bit written to 1, the error outout pins stay in High-Z state after reset lifts and 
                                        the FCCU EOUT reporting is not functioning.
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:58b5e6c6-4207-499b-9b26-f473d37fdff6">
                  <SHORT-NAME>AlarmNotificationApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                          In case of a failure event, if alarm interrupt is enabled, the fault shall be notified to 
                                            application using this callback. The prototype of the notification function is
                                          void Mcem_NotificationCallbackFunction( Mcem_FaultType FaultID );
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:58b5e6c6-4207-466b-9b26-f473d37fdff6">
                  <SHORT-NAME>McemConfigTimeOutNotificationAPI</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                          In case of a timeout during mode configuration, if Configuration TimeOut Interrupt is enabled, the timeout shall be notified to 
                                            application using this callback. The prototype of the notification function is
                                          void &lt;Mcem_NotificationCallbackFunction(void)&gt;;
                                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
              </PARAMETERS>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:ac16f412-b19d-48a6-ab7b-6c7a806afd6a">
                  <SHORT-NAME>DefaultFaultConfig</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            This subcontainer specifies default configuration of all non-critical fault sources.
                                               All sources are enabled by default.
                                            Possible deviations must to be explicitly specified at  the Fault tab.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:51dce42e-4ecc-4baa-9f55-6b8bf350eff5">
                      <SHORT-NAME>RecoveryType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    Non-critical fault configuration
                                                    
                                                    HW recoverable fault
                                                    SW recoverable fault
                                                    
                                                    The non-critical fault configuration defines the fault recovery mode.
                                                    HW recoverable faults are self recovered (status flag clearing and related) if the root cause (input fault)has been removed.
                                                    SW recoverable faults are recovered (status flag clearing) by SW clearing of the related status flag.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>SwRecoverableFault</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SwRecoverableFault</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>HwRecoverableFault</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:d1fec224-4ecc-481d-8fc1-ac559f77edc6">
                      <SHORT-NAME>ReactionType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    Non-critical fault state configuration
                                                    
                                                     Short functional reset request pulse (FAULT state reaction)
                                                     Long functional reset request pulse (FAULT state reaction)
                                                     No reset reaction 
                                                    
                                                    
                                                    Note:
                                                    Due to hardware limitations then:
                                                    
                                                    Reset Reaction of all Faults default is No Reset Reaction. 
                                                    User can change this configuration for each Fault in Fault tab. 
                                                    With Fault MCEM_FCCU_FLASH_INIT allways configured is No Reset Reaction.
                                                    
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>NoResetReaction</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ShortResetReaction</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>LongResetReaction</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>NoResetReaction</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:789e1d41-4ecc-458f-b9cc-2f433d73c11e">
                      <SHORT-NAME>RecoveryTimeOutEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    Fault time-out enable
                                                    
                                                    Unchecked: FCCU moves into the FAULT state if the respective fault is enabled
                                                    Checked: FCCU moves into the ALARM state if the respective fault is enabled
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:61000e3f-4ecc-4bb1-9a1d-4549f0c93299">
                      <SHORT-NAME>AlarmIrqEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    IRQ alarm enable
                                                    
                                                    Unchecked: Alarm is disabled for the configured error source.
                                                    Checked: Alarm is enabled for the configured error source. 
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9a901a2f-4ecc-4366-9720-ed4596ca730a">
                      <SHORT-NAME>FaultNmiEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    NMI enable
                                                    
                                                    Unchecked: NMI is disabled for error (NCF/) source x.
                                                    Checked: NMI is enabled for error (NCF/) source x. 
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:573d22a8-4ecc-455c-bff4-b6cca35ac3d9">
                      <SHORT-NAME>ActivateOutputPins</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    EOUT signaling enable
                                                    
                                                    Unchecked:EOUT signaling is disabled for error (NCF/) source x. Error pins are as if in non-faulty state.
                                                    Checked: EOUT signaling is enabled for error (NCF/) source x. 
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:e2d99ec4-d1ad-4aab-8bbf-b262974338d8">
                  <SHORT-NAME>Fault</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Reference to faults with non-default handlings.
                                            By default, all non-reserved faults are enabled and handled according to the default configurations. The explicitly created fault is enabled, and the default values for recovery and reaction
type are selected. It can be disabled or configured differently.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:0f02227e-6eae-4546-b144-245da2ecfcf5">
                      <SHORT-NAME>SignalDesc</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                Non-critical fault enable
                                                
                                                 No actions following the respective non-critical fault assertion 
                                                 FCCU moves to ALARM or FAULT state 
                                                
                                                If fault is selected, it is automatically enabled, and the default values for recovery and reaction type are selected.
                                                Also Alarm and Fault interrupts (IRQ and NMI), Timeout and EOUT signaling are selected.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>MCEM_FCCU_TEMP_ERROR</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_TEMP_ERROR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_LVD_ERROR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_HVD_ERROR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_DPMC_SELF_TEST</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_MEMORY_DCF_SAFETY_ERR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SSCM_XFER_ERR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_STCU_UF</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_STCU_RF</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_STCU_LMBIST_USR_ERR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SPURIOUS_DEBUG_SSCM_ACTIVATION</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_RCCU_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_RCCU_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_WDRS_DBRC0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_WDRS_DBRC1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SWTRS0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SWTRS1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SWTINT0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_FLASH_INIT</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SSCM_INIT</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_PER_CE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_PER_UCE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_FLS_CE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_FLS_UCE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_PLL_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_PLL_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_CMU_0_OSC</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_CMU_0_PLL</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_CMU_COMP</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_CMU_OTHER</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_EDC_ECC_FLASH</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_EDC_ECC_FLASH_C</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_ENC_ERR_FLASH</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_ADDR_FDBK_ERR_FLASH_C</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_XBAR_TRANSACTION_MONITOR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_ADDR_FDBK_ERR_PRAM_RAM_LWB_ERR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SSCM_PASS_ECC_ERR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_EDC_ERR_PRAM</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_DFT1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_DFT2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_DFT3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_DFT4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_SAFETY_CORE_MACHINE_CHECK_EXCEPTION</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_LOCKSTEP_MODE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_ERROR_IN_ERR</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_RESERVED_44</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_ERM_CE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>MCEM_FCCU_ERM_UCE</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:1e7fb351-a25a-4169-a1f1-c30a391777f8">
                      <SHORT-NAME>FaultDisabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                Fault source disabled
                                                
                                                Unchecked: Specified non-critical fault source is enabled (default).
                                                Checked: Specified non-critical fault source is disabled.
                                                
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:51dce42e-156c-4baa-9f55-6b8bf350eff5">
                      <SHORT-NAME>RecoveryType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    Non-critical fault configuration
                                                    
                                                    HW recoverable fault
                                                    SW recoverable fault
                                                    
                                                    The non-critical fault configuration defines the fault recovery mode.
                                                    HW recoverable faults are self recovered (status flag clearing and related) if the root cause (input fault)has been removed.
                                                    SW recoverable faults are recovered (status flag clearing) by SW clearing of the related status flag.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>SwRecoverableFault</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SwRecoverableFault</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>HwRecoverableFault</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:d1fec224-156c-481d-8fc1-ac559f77edc6">
                      <SHORT-NAME>ReactionType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    Non-critical fault state configuration
                                                    
                                                     Short functional reset request pulse (FAULT state reaction)
                                                     Long functional reset request pulse (FAULT state reaction)
                                                     No reset reaction 
                                                    
													
													Note:
													Due to hardware limitations then:
													
													Reset Reaction of all Faults default is No Reset Reaction. 
													User can change this configuration for each Fault in Fault tab. 
													With Fault MCEM_FCCU_FLASH_INIT allways configured is No Reset Reaction.
													
													
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>NoResetReaction</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ShortResetReaction</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>LongResetReaction</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>NoResetReaction</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:789e1d41-156c-458f-b9cc-2f433d73c11e">
                      <SHORT-NAME>RecoveryTimeOutEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    Fault time-out enable
                                                    
                                                    Unchecked: FCCU moves into the FAULT state if the respective fault is enabled
                                                    Checked: FCCU moves into the ALARM state if the respective fault is enabled
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:61000e3f-156c-4bb1-9a1d-4549f0c93299">
                      <SHORT-NAME>AlarmIrqEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    IRQ alarm enable
                                                    
                                                    Unchecked: Alarm is disabled for the configured error source.
                                                    Checked: Alarm is enabled for the configured error source. 
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9a901a2f-156c-4366-9720-ed4596ca730a">
                      <SHORT-NAME>FaultNmiEnabled</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    NMI enable
                                                    
                                                    Unchecked: NMI is disabled for error (NCF/) source x.
                                                    Checked: NMI is enabled for error (NCF/) source x. 
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:573d22a8-156c-455c-bff4-b6cca35ac3d9">
                      <SHORT-NAME>ActivateOutputPins</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    EOUT signaling enable
                                                    
                                                    Unchecked:EOUT signaling is disabled for error (NCF/) source x. Error pins are as if in non-faulty state.
                                                    Checked: EOUT signaling is enabled for error (NCF/) source x. 
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:524f6901-17f0-4d12-a8c6-521b65ab2a85">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                        CommonPublishedInformation
                                        Common container, aggregated by all modules. It contains published information about vendor and versions.
                                        </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:0eb7f210-dc10-42c4-882d-108232f4190e">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            AUTOSAR Release Major Version
                                            Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1b0559ac-f026-40a5-be94-d47aba94caf7">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            AUTOSAR Release Minor Version
                                            Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:f244de86-186b-4c28-aef3-8990a2302432">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            AUTOSAR Patch Version
                                            Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:bd007180-4e46-4f30-8e4e-f76a83e2b700">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Module ID
                                            Module ID of this module from Module List.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:5d32253a-accb-4c10-b20c-315433021383">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Software Major Version
                                            Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:9a91dd84-07ab-4047-af02-2966dc1dc344">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Software Minor Version
                                            Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e987bc51-a6e3-47e6-8387-c463f5dead01">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Software Patch Version
                                            Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:9a99c43a-5c29-4ee3-803a-3a1e8b5a852e">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Vendor Api Infix
                                            In driver modules which can be instantiated several times on a single ECU, BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name. 
                                            This parameter is used to specify the vendor specific name. In total, the implementation specific name is generated as follows:
                                            &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt;.

                                            E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 

                                            This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:0e3963bf-453b-43a2-865b-204cc3b387f1">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            Vendor ID
                                            Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>