<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>IoDal</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>IoDal</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/IoDal</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-POST-BUILD</IMPLEMENTATION-CONFIG-VARIANT>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>2</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>2</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>100</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>IoDalBswConfig</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Adc_Pot</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>250</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Input</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Analog</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Adc/Adc/AdcConfigSet_0/AdcHwUnit_0/AdcChannel_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Adc/Adc/AdcConfigSet_0/AdcHwUnit_0/AdcGroup_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/IoDal/IoDal/IoDalBswConfig/TimeTriggerTable_0/SchedulePoints_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Dio_Key1</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Input</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Digital</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dio/Dio/DioConfig_0/Dio_PH/Dio_DigKey1</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Dio_Out1</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Output</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Digital</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dio/Dio/DioConfig_0/Dio_PH/Dio_out1</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Ocu_Trigger</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Trigger</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Ocu</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/IoDal/IoDal/IoDalBswConfig/TimeTriggerTable_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Pwm_Key2</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Input</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Digital</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Dio/Dio/DioConfig_0/Dio_PH/Dio_PwmKey2</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Pwm_Out1</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Output</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Pwm</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Pwm/Pwm/PwmChannelConfigSet_0/PwmChannel_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>IoDal_Pwm_Out2</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ConvTime</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DigitalSignalLevel</DEFINITION-REF>
                      <VALUE>STD_LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmMask</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmType</DEFINITION-REF>
                      <VALUE>NORMAL</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceDirection</DEFINITION-REF>
                      <VALUE>Output</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ReferenceType</DEFINITION-REF>
                      <VALUE>Pwm</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TriggerType</DEFINITION-REF>
                      <VALUE>SW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogChRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/AnalogRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/DioRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/ExtDevSensingRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/IcuRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/PwmRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Pwm/Pwm/PwmChannelConfigSet_0/PwmChannel_1</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/SwTriggerScheduling</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/IoDescriptors/TimeTriggerTableRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>TimeTriggerTable_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/TimeTriggerTable</DEFINITION-REF>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/TimeTriggerTable/OcuRef</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Ocu/Ocu/OcuConfigSet_0/OcuChannel_0</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>SchedulePoints_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/TimeTriggerTable/SchedulePoints</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalBswConfig/TimeTriggerTable/SchedulePoints/ValueInTicks</DEFINITION-REF>
                          <VALUE>100</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>IoDalGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/IoDal/IoDalGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/IoDal/IoDalGeneral/EnableDevErrorDetect</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
