<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:781016ba-cac9-4286-95f6-6c2e5f2d5180">
          <SHORT-NAME>IntegrationApp_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D47M10I0R0/IntegrationApp</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:aa293437-42fc-3434-b6a4-f8c4da165866">
          <SHORT-NAME>IoDal</SHORT-NAME>
          <DESC>
            <L-2 L="EN">
                                        Configuration of the Generic integration applicaton components.
                                    </L-2>
          </DESC>
          <ADMIN-DATA>
            <LANGUAGE>EN</LANGUAGE>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>1.0.0</REVISION-LABEL>
                <ISSUED-BY>NXP</ISSUED-BY>
                <DATE>2010-12-03</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD-SELECTABLE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:100d668b-c1c3-4833-9bd8-2ebcdc32b277">
              <SHORT-NAME>IoDalGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">This container holds the general, pre-compile configuration parameters for the EcuMFlex.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:2810d48b-c07e-46f0-b111-100148be101d">
                  <SHORT-NAME>EnableDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                       
                                       This flag indicates whether Det error report is enabled or not.
                                       </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:8d95680f-9d41-4ab0-80fb-341e78968c4b">
              <SHORT-NAME>IoDalBswConfig</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                    
                                    Configuration of the Basic software for Iodal component.
                                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de1adbaf-34dd-5f7e-89de-65775795e1b9">
                  <SHORT-NAME>IoDescriptors</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Configuration of the Io Driver Abstraction layer.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:42ccb255-341e-9d91-acdf-977c9fc0cb23">
                      <SHORT-NAME>ReferenceDirection</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                            
                                            IO signal direction (Input, Output or Trigger)
                                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Input</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Output</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Trigger</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:42c341e5-1f6b-9d91-341e-977c9fc0cb23">
                      <SHORT-NAME>ReferenceType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Signal type: Analog, Input capture, PWM etc
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Analog</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Icu</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Digital</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Pwm</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Ocu</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ExtDev</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ExtSensDev</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:28a89e8b-341e-46f0-341e-dbf248bedc09">
                      <SHORT-NAME>DigitalSignalLevel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Parameter defines the default Signal Level: Low or High.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>STD_LOW</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STD_LOW</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STD_HIGH</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:6fc4decb-1d18-4bfe-decb-12f1decbaf28">
                      <SHORT-NAME>ConvTime</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Analog Conversion time (estimated in ticks)
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>5</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:decbb255-1f6b-9d91-acdf-977c9fc0cb23">
                      <SHORT-NAME>TriggerType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Analog trigger type: SW trigger or HW trigger.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>SW</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SW</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>HW</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:41fece55-1f6b-9d91-acdf-977c9fc0cb23">
                      <SHORT-NAME>PwmType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Parameter describe if the PWM channel runs in a special mode (SYNC) or Normal mode.
                                                In Sync mode, several PWM channel can be syncronized to have their ouptut waveform updates happening at the same time. 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>NORMAL</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SYNC</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>NORMAL</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:41fece55-1f6b-9d91-ce55-977c9fc0ce55">
                      <SHORT-NAME>PwmMask</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Selects PWM channels that are syncronized.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6f341eda-1d18-341e-84fb-12f19390af28">
                      <SHORT-NAME>AnalogRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                               Reference to the Analog group (Adc)
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Adc/AdcConfigSet/AdcHwUnit/AdcGroup</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc4decb-1d18-4bfe-decb-12f19390af28">
                      <SHORT-NAME>AnalogChRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                               Reference to the Analog Channel (Adc)
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Adc/AdcConfigSet/AdcHwUnit/AdcChannel</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc1feca-1d18-1fec-84fb-12f19390af28">
                      <SHORT-NAME>SwTriggerScheduling</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Scheduling point for SW triggered Analog inputs.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/IoDal/IoDalBswConfig/TimeTriggerTable/SchedulePoints</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc493da-1fec-4bfe-84fb-12f19391fec8">
                      <SHORT-NAME>DioRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to DIO channel (for digital input/output channels). 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dio/DioConfig/DioPort/DioChannel</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:61fec3da-1d18-4bfe-1fec-12f19390af28">
                      <SHORT-NAME>PwmRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                 Reference to PWM channel. 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Pwm/PwmChannelConfigSet/PwmChannel</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc4ce55-1d18-4bfe-ce55-12f19390af28">
                      <SHORT-NAME>TimeTriggerTableRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to OCU channel. 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/IoDal/IoDalBswConfig/TimeTriggerTable</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc493da-1d18-4bfe-84fb-12f11d18af28">
                      <SHORT-NAME>IcuRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to ICU channel. 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Icu/IcuConfigSet/IcuChannel</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc493da-1d18-4bfe-1d18-121d1890af28">
                      <SHORT-NAME>ExtDevRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to External device channel. 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/IoDal/IoDalBswConfig/IoExtDevices/MotorBridges</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc493da-1d18-4bfe-1d18-121d1890af28">
                      <SHORT-NAME>ExtDevSensingRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to External device channel. 
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/IoDal/IoDalBswConfig/IoExtDevices/ExternalSensors</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de1a4567-34dd-5f7e-89de-657456795e1b9">
                  <SHORT-NAME>IoExtDevices</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                             Configuration for external devices (SPI, I2C)
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <SUB-CONTAINERS>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de4567af-34dd-4567-89de-65775795e1b9">
                      <SHORT-NAME>MotorBridges</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Holds configuration for Motor Bridge type device 
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:42ccb255-1f6b-9d91-1234-977c9fc0cb23">
                          <SHORT-NAME>MotorBridgeDeviceType</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                                        
                                                        Motor bridge device Type: MC33932EK (used for brushed motors), MC34GD3000 (used for brushless motors).
                                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DEFAULT-VALUE>COMDAL_TXCHANNEL</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>MC33932EK</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>MC34GD3000</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                      </PARAMETERS>
                      <REFERENCES>
                        <ECUC-REFERENCE-DEF UUID="ECUC:6fc41939-1d18-4bfe-1939-12f19390af28">
                          <SHORT-NAME>MotorCtrlPwmOutput1</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Motor Control primary output </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Pwm/PwmChannelConfigSet/PwmChannel</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                        <ECUC-REFERENCE-DEF UUID="ECUC:6fc41939-1d18-4bfe-1939-12f19190af28">
                          <SHORT-NAME>MotorCtrlPwmOutput2</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Motor Control primary output </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Pwm/PwmChannelConfigSet/PwmChannel</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                        <ECUC-REFERENCE-DEF UUID="ECUC:6fc41939-1d18-4bfe-1939-12f19190af28">
                          <SHORT-NAME>MotorCtrlPwmOutput3</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN"> Motor Control primary output </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Pwm/PwmChannelConfigSet/PwmChannel</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                      </REFERENCES>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de4567af-34dd-4567-89de-62342579e1b9">
                      <SHORT-NAME>ExternalSensors</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Holds configuration for External Sensors devices.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <REFERENCES>
                        <ECUC-REFERENCE-DEF UUID="ECUC:6fc41939-1d18-4bfe-1939-12f19191af28">
                          <SHORT-NAME>MotorCtrlCWIncrement</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">  Dio Channel used for clockwise speed increment </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dio/DioConfig/DioPort/DioChannel</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                        <ECUC-REFERENCE-DEF UUID="ECUC:6fc41939-1d18-4bfe-1939-12f1a191af28">
                          <SHORT-NAME>MotorCtrlCCWIncrement</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">  Dio Channel used for clockwise speed increment </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dio/DioConfig/DioPort/DioChannel</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                      </REFERENCES>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de4567af-34dd-4567-89de-65775795e1b9">
                      <SHORT-NAME>LedDrivers</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Holds configuration for Led driver devices 
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                  </SUB-CONTAINERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de1adbaf-4567-5f7e-4567-65775795e1b9">
                  <SHORT-NAME>TimeTriggerTable</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Time Trigger table configuration
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:6fc493da-1d18-4567-84fb-12f45670af28">
                      <SHORT-NAME>OcuRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to OCU channel used for time triggering.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Ocu/OcuConfigSet/OcuChannel</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                  <SUB-CONTAINERS>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de1adbaf-4567-5f7e-89de-65745675e1b9">
                      <SHORT-NAME>SchedulePoints</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Scheduling points definition. (Time trigger entry list)
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-INTEGER-PARAM-DEF>
                          <SHORT-NAME>ValueInTicks</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                                        
                                                        Time value in tick used for setting up the next compare match event.
                                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>4294967295</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                      </PARAMETERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                  </SUB-CONTAINERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:f7a92bc0-df21-48a8-8bcc-eb9df292f1b2">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                      Common container, aggregated by all modules. It contains published information about vendor and versions.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:55930215-d177-41b2-8660-bc960723a9cb">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                         Major version number of AUTOSAR specification on which the appropriate implementation is based on.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d2dc342f-2834-4cc0-bd45-9aebf96876ce">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Minor version number of AUTOSAR specification on which the appropriate implementation is based on.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>2</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:7dd3874a-e6e9-4035-bd38-14299176aa46">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Revision version number of AUTOSAR specification on which the appropriate implementation is based on.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>2</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:bd6d918d-03f9-4da3-9131-75c1d6b4cad1">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Module ID of this module from Module List.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>100</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e02435a3-0cbf-4209-9908-d147ed439d34">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Major version number of the vendor specific implementation of the module. The numbering is vendor specific.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:5eefadd2-c509-423a-9ed8-6e587eb683f2">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:41425ebf-876a-47e0-9569-fad6d5db22c1">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                        Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:79eb6936-7081-44cd-bf5f-7adb993f72ba">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                In driver modules which can be instantiated several times on a single ECU, BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name. 
                                This parameter is used to specify the vendor specific name. In total, the implementation specific name is generated as follows:
                                &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt;.
                                E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 
                                This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:839d446a-ffad-4105-a647-2816e258f21e">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                          Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>