<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Dem</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Dem</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Dem</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-POST-BUILD</IMPLEMENTATION-CONFIG-VARIANT>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>3</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>54</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>DemConfigSet_0</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>ADC_E_TIMEOUT</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DEM_E_GENERAL_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>19</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>ETH_E_ACCESS</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_COMPARE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>6</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_ERASE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>4</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_READ_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>5</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_UNEXPECTED_FLASH_ID</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FLS_E_WRITE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>3</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>FR_E_ACCESS</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>8</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>LIN_E_TIMEOUT</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>9</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_CLOCK_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>10</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_LOCK_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>11</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_QUARTZ_FAILURE</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>12</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>MCU_E_TIMEOUT_TRANSITION</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>13</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>PWM_E_UNEXPECTED_IRQ</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>14</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SPI_E_HARDWARE_ERROR</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>15</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_DISABLE_REJECTED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>17</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_MISS_TRIGGER</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>18</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>WDG_E_MODE_FAILED</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventAvailable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventFailureCycleCounterThreshold</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventId</DEFINITION-REF>
                      <VALUE>16</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemEventKind</DEFINITION-REF>
                      <VALUE>DEM_EVENT_KIND_BSW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemFFPrestorageSupported</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemOperationCycleRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-CHOICE-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass</DEFINITION-REF>
                      <SUB-CONTAINERS>
                        <ECUC-CONTAINER-VALUE>
                          <SHORT-NAME>DemDebounceAlgorithmClass</SHORT-NAME>
                          <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased</DEFINITION-REF>
                          <REFERENCE-VALUES>
                            <ECUC-REFERENCE-VALUE>
                              <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemConfigSet/DemEventParameter/DemDebounceAlgorithmClass/DemDebounceCounterBased/DemDebounceCounterBasedClassRef</DEFINITION-REF>
                            </ECUC-REFERENCE-VALUE>
                          </REFERENCE-VALUES>
                        </ECUC-CONTAINER-VALUE>
                      </SUB-CONTAINERS>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>DemGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemAgingCycleCounterProcessing</DEFINITION-REF>
                  <VALUE>DEM_PROCESS_AGINGCTR_EXTERN</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemAgingRequieresTestedCycle</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemAvailabilitySupport</DEFINITION-REF>
                  <VALUE>DEM_NO_AVAILABILITY</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemBswErrorBufferSize</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemClearDTCBehavior</DEFINITION-REF>
                  <VALUE>DEM_CLRRESP_NONVOLATILE_FINISH</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemClearDTCLimitation</DEFINITION-REF>
                  <VALUE>DEM_ALL_SUPPORTED_DTCS</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemDataElementDefaultEndianness</DEFINITION-REF>
                  <VALUE>BIG_ENDIAN</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemDebounceCounterBasedSupport</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemDebounceTimeBasedSupport</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemDtcStatusAvailabilityMask</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemEventCombinationSupport</DEFINITION-REF>
                  <VALUE>DEM_EVCOMB_DISABLED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemEventDisplacementStrategy</DEFINITION-REF>
                  <VALUE>DEM_DISPLACEMENT_FULL</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemEventMemoryEntryStorageTrigger</DEFINITION-REF>
                  <VALUE>DEM_TRIGGER_ON_TEST_FAILED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemGeneralInterfaceSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemMaxNumberEventEntryPermanent</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemMaxNumberPrestoredFF</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOBDSupport</DEFINITION-REF>
                  <VALUE>DEM_OBD_NO_OBD_SUPPORT</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOccurrenceCounterProcessing</DEFINITION-REF>
                  <VALUE>DEM_PROCESS_OCCCTR_CDTC</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOperationCycleStatusStorage</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemPTOSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemResetConfirmedBitOnOverflow</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemStatusBitHandlingTestFailedSinceLastClear</DEFINITION-REF>
                  <VALUE>DEM_STATUS_BIT_AGING_AND_DISPLACEMENT</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemStatusBitStorageTestFailed</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemSuppressionSupport</DEFINITION-REF>
                  <VALUE>DEM_DTC_SUPPRESSION</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTaskTime</DEFINITION-REF>
                  <VALUE>0.1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTriggerDcmReports</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTriggerDltReports</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTriggerFiMReports</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTriggerMonitorInitBeforeClearOk</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTypeOfDTCSupported</DEFINITION-REF>
                  <VALUE>DEM_DTC_TRANSLATION_ISO11992_4</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemTypeOfFreezeFrameRecordNumeration</DEFINITION-REF>
                  <VALUE>DEM_FF_RECNUM_CALCULATED</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemVersionInfoApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DemFreezeFrameRecNumClass_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemFreezeFrameRecNumClass</DEFINITION-REF>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <INDEX>0</INDEX>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemFreezeFrameRecNumClass/DemFreezeFrameRecordClassRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DemOperationCycle_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOperationCycle</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOperationCycle/DemOperationCycleAutomaticEnd</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOperationCycle/DemOperationCycleAutostart</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemOperationCycle/DemOperationCycleType</DEFINITION-REF>
                      <VALUE>DEM_OPCYC_IGNITION</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>DemPrimaryMemory</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemPrimaryMemory</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T2D41M10I0R0/Dem/DemGeneral/DemPrimaryMemory/DemMaxNumberEventEntryPrimary</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
