<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:8d4fdbd4-309e-4615-8f34-a64d5adbf2cc">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:67590c1f-f952-4b87-b78c-94f327edc863">
          <SHORT-NAME>Adc_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Adc</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:88c438bf-b6be-49f2-993b-3e287fdb21fc">
          <SHORT-NAME>Adc</SHORT-NAME>
          <DESC>
            <L-2 L="EN">Configuration of the Adc (Analog Digital Conversion) module.</L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.3.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2011-11-24T17:00:00+01:00</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <REFINED-MODULE-DEF-REF DEST="ECUC-MODULE-DEF">/AUTOSAR/EcucDefs/Adc</REFINED-MODULE-DEF-REF>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5c49ee28-8607-4878-ada6-4023d50d3efd">
              <SHORT-NAME>AdcConfigSet</SHORT-NAME>
              <DESC>
                <L-2 L="EN">This is the base container that contains the post-build selectable configuration parameters</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:3d5fdf44-841b-443b-9cf1-bccd75b6198a">
                  <SHORT-NAME>AdcHwUnit</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">This container contains the Driver configuration (parameters) depending on grouping of channels.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:cf47d824-8ae8-475f-9aca-b4e66095bbd5">
                      <SHORT-NAME>AdcTransferType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Select the Interrupt or Dma transfer Type. If DMA is used, user must not run SW and HW groups at the same time on the same HW unit because the same DMA channel will be used for both. If DMA is required for AdcTransferType, it is recommended to keep AdcWithoutInterrupts as false, otherwise, DMA will not be configured and it will be user responsibilty to read the results from registers directly by calling Adc_ReadGroup</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>ADC_INTERRUPT</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ADC_DMA</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ADC_INTERRUPT</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:d9d2de7c-e7da-4d5a-a3c1-b241cb8342bd">
                      <SHORT-NAME>AdcClockSource</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">This parameter is used to select the system clock signal of
                                                       the prescaler output clock signal.
                                                       CLK_SRC_0 = Prescaler output clock is selected.
                                                       CLK_SRC_1 = System clock is selected - maximum frequency.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>CLK_SRC_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>CLK_SRC_0</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>CLK_SRC_1</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:0c231b0e-e445-4ffc-be38-5b9e4425a277">
                      <SHORT-NAME>AdcHwUnitId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Specifies the used ADC Hardware Unit.
                            ADC0 and ADC1 are corresponding ADC number 0 and ADC number 1 of EQADCA 
                            ADC2 and ADC3 are corresponding ADC number 0 and ADC number 1 of EQADCB</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>ADC0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ADC0</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ADC1</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ADC2</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ADC3</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:f8f69c4d-d49e-4c7f-8651-5f7cfc5e3533">
                      <SHORT-NAME>AdcLogicalUnitId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Specifies the Logical id of the Hardware Unit.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>3</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:2b4de5da-3319-4745-bf24-fc936c3f68b7">
                      <SHORT-NAME>AdcResolution</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Used to set the ADC resolution mode.
                                  
                                  BITS_8           - 8-bit conversion.
                                  BITS_10          - 10-bit conversion.
                                  BITS_12          - 12-bit conversion.
                                  .</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>BITS_12</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>BITS_8</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>BITS_10</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>BITS_12</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:43c026fc-c64d-4dd4-b273-8d45334a6f92">
                      <SHORT-NAME>AdcPrescale</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">ADCn Clock Prescaler (ADCn_CLK_PS bits in ADCn_CR register).
                                    The ADCn_CLK_PS field controls the system clock divide factor for the ADCn clock as in the following table:
                                    ADCn_CLK_PS           System Clock Divide Factor
                                    0             -----   2
                                    1             -----   4
                                    2             -----   6
                                    ...                    
                                    30            -----  62
                                    31            -----  64
                                    Note: This parameter value is applicable only when the Prescaler output clock is selected in AdcClockSource parameter.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>31</DEFAULT-VALUE>
                      <MAX>31</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:43c026fc-c64d-4dd4-b273-8d85334a6f92">
                      <SHORT-NAME>AdcAltPrescale</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">ADCn Clock Prescaler (ADCn_CLK_PS bits in ADCn_CR register).
                                    The ADCn_CLK_PS field controls the system clock divide factor for the ADCn clock as in the following table:
                                    ADCn_CLK_PS           System Clock Divide Factor
                                    0             -----   2
                                    1             -----   4
                                    2             -----   6
                                    ...                    
                                    30            -----  62
                                    31            -----  64
                                    Note: This parameter value is applicable only when the Prescaler output clock is selected in AdcClockSource parameter.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>31</DEFAULT-VALUE>
                      <MAX>31</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:d1dd89fe-fdb8-43e4-a51d-927bd64e8e88">
                      <SHORT-NAME>AdcExternalMultiplexing</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables external multiplexing (ADCn_EMUX bit in ADCn_CR register). The ADC units of one EQADC (0-1, 2-3) cannot have external multiplexing enabled at the same time. Note: This is an Implementation Specific Parameter.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c24b64bc-f39d-4f6b-af73-386e6c09ac55">
                      <SHORT-NAME>AdcCalibration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                   Enables/disables the calibration on this hw unit.
                                   Besides this configuration parameter it is also needed to enable &amp;quotAdcCalibrationApi&amp;quot parameter
                                   and &quot;AdcChannelCalibration&quot; for the channel which should be calibrated.
                                   Note: This is an Implementation Specific Parameter.
                                   </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                  <SUB-CONTAINERS>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:1bda8cf5-cdd6-4b14-8b9f-8a6f6f567ed8">
                      <SHORT-NAME>AdcChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">This container contains the channel configuration (parameters) depending on the hardware capability.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:25414223-a7a9-4f46-bb8f-7f86fa8b5500">
                          <SHORT-NAME>AdcChannelConvTime</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Configuration of conversion time, i.e. the time during which the analogue value is converted into digital representation, (in clock cycles) for each channel, if supported by hardware.
                                                          This parameter is not used by the current implementation.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>18446744073709551615</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:ca1022a6-a5bb-44e1-b817-ece122e5951b">
                          <SHORT-NAME>AdcChannelHighLimit</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">High limit - used for limit checking.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>18446744073709551615</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e2e71142-5b64-4236-b15f-9b880ca8325c">
                          <SHORT-NAME>AdcLogicalChannelId</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">This is the logical Id of the ADC channel.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>1024</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:029500a6-3405-401f-a1c2-a159e534c0be">
                          <SHORT-NAME>AdcChannelId</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">This parameter defines the assignment of the channel to the physical ADC hardware channel. Note: Range of the ADC Channels depends on the selected package.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>AN_0</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_0</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_1</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_2</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_3</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_4</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_5</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_6</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_7</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_8</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_9</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_10</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_11</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_12</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_13</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_14</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_15</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_16</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_17</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_18</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_19</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_20</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_21</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_22</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_23</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_24</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_25</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_26</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_27</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_28</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_29</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_30</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_31</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_32</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_33</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_34</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_35</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_36</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_37</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_38</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_39</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_40</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_41</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_42</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_43</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_44</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_45</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_64</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_65</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_66</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_67</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_68</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_69</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_70</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_71</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_72</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_73</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_74</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_75</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_76</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_77</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_78</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_79</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_80</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_81</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_82</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_83</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_84</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_85</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_86</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_87</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_88</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_89</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_90</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_91</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_92</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_93</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_94</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_95</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_96</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_97</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_98</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_99</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_128</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_129</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_145</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_224</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_225</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_226</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_227</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_228</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_229</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_230</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_231</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_232</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_233</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_234</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_235</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_236</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_237</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_238</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_239</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_240</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_241</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_242</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_243</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_244</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_245</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_246</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_247</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_248</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_249</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_250</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_251</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_252</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_253</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_254</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>AN_255</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:3c8fd425-d4b7-4550-aea0-9c4ce253f9e4">
                          <SHORT-NAME>AdcChannelLimitCheck</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Enables or disables limit checking for an ADC channel.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:ed93d1f8-7c4d-459e-b781-d7b28fe97cb7">
                          <SHORT-NAME>AdcChannelLowLimit</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Low limit - used for limit checking.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>18446744073709551615</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:4f3db645-2a27-4289-bef1-a3c669f2d86c">
                          <SHORT-NAME>AdcChannelRangeSelect</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">In case of active limit checking: defines which conversion values are taken into account related to the boarders defined with AdcChannelLowLimit and AdcChannelHighLimit.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_RANGE_ALWAYS</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_ALWAYS</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_BETWEEN</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_NOT_BETWEEN</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_NOT_OVER_HIGH</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_NOT_UNDER_LOW</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_OVER_HIGH</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_RANGE_UNDER_LOW</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:e141efcc-a3d5-4127-bf67-52e7ca378d89">
                          <SHORT-NAME>AdcChannelRefVoltsrcHigh</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Upper reference voltage source for each channel.This parameter is not used by the current implementation.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>UPPER_REF_VOLT_0</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>UPPER_REF_VOLT_0</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:f71ff945-81dc-4e80-a7bd-587776a932b7">
                          <SHORT-NAME>AdcChannelRefVoltsrcLow</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Lower reference voltage source for each channel.This parameter is not used by the current implementation.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>LOWER_REF_VOLT_0</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>LOWER_REF_VOLT_0</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:115f2554-ffe3-4171-8abd-d2caa3a498c7">
                          <SHORT-NAME>AdcChannelResolution</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Resolution of converted value. Valid resolution values are: 12-bit, 10-bit and 8-bit.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>12</DEFAULT-VALUE>
                          <MAX>63</MAX>
                          <MIN>1</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:54bf9db3-2c2c-45ba-81d0-4df31213e7ab">
                          <SHORT-NAME>AdcChannelCalibration</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Indicates if the returning channel conversion result is calibrated (CAL bit in conversion command message). Note that besides this configuration item it is also needed to globally enable calibration by &quot;AdcCalibrationApi&quot; and to enable calibration on hw unit by &quot;AdcCalibration&quot; parameter. Note: This is an Implementation Specific Parameter.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:5fab3df1-dd6e-4a42-8a60-21d1ee5a530a">
                          <SHORT-NAME>AdcChannelSampTime</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Sampling time, i.e. the time during whuch the value is sampled, (in clock cycles) for each channel.
                            
                                0    ---------      ADC_2_CLOCK_CYCLES
                                1    ---------      ADC_8_CLOCK_CYCLES
                                2    ---------      ADC_64_CLOCK_CYCLES
                                3    ---------      ADC_128_CLOCK_CYCLES
                                
                                When AdcExternalMultiplexing parameter is enabled in this case EQADC_ADC_64_CLOCK_CYCLES_U32 or EQADC_ADC_128_CLOCK_CYCLES_U32 sampling cycles is recommended.
                                </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>3</DEFAULT-VALUE>
                          <MAX>3</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                      </PARAMETERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:1a9750b2-e985-4bfe-afeb-69760dbfdddd">
                      <SHORT-NAME>AdcGroup</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">This container contains the Group configuration (parameters).</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:e0b07dba-d097-4aa4-9b2b-c87b5e68fbff">
                          <SHORT-NAME>AdcGroupAccessMode</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Type of access mode to group conversion results.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_ACCESS_MODE_SINGLE</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_ACCESS_MODE_SINGLE</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_ACCESS_MODE_STREAMING</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:cecb9b6c-d664-43fa-80b7-5122d3a178cc">
                          <SHORT-NAME>AdcGroupConversionMode</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Type of Conversion mode of the channel group.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_CONV_MODE_ONESHOT</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_CONV_MODE_CONTINUOUS</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_CONV_MODE_ONESHOT</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:9c7e30ee-cca4-4874-90b2-0492458cb413">
                          <SHORT-NAME>AdcGroupConversionType</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Normal or Injected conversion type.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_CONV_TYPE_NORMAL</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_CONV_TYPE_NORMAL</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_CONV_TYPE_INJECTED</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:84e98da0-f4af-4c03-a4a4-a9b7efd5b563">
                          <SHORT-NAME>AdcGroupId</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Numeric ID of the group. This parameter is the symbolic name to be used on the API. This symbolic name allows accessing Channel Group data. This value will be assigned to the symbolic name derived of the AdcGroup container shortName.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>1023</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1f39cff8-368c-4814-bbce-34a529f2e9f8">
                          <SHORT-NAME>AdcGroupPriority</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Priority level of the AdcGroup. This item is ignored if Adc/AdcGeneral/AdcPriorityImplementation is defined to ADC_PRIORITY_NONE.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>255</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:040e7ff3-d837-4037-9a61-c284bbad9a32">
                          <SHORT-NAME>AdcGroupReplacement</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Replacement mechanism used on ADC group level, if a group conversion is interrupted by a group which has a higher priority. It's fixed to Abort/Restart</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_GROUP_REPL_ABORT_RESTART</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_GROUP_REPL_ABORT_RESTART</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_GROUP_REPL_SUSPEND_RESUME</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:d6ca518c-2748-42bb-b382-6b052094b115">
                          <SHORT-NAME>AdcGroupTriggSrc</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Type of source event that starts a group conversion. It' s possible select Hw or Sw trigger.
                              In case of HW trigger source the actual HW trigger source will be selected by the &quot;AdcHwTrigSrc&quot; parameter and it can be any of the supported HW trigger sources available for this controller.
                              </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_TRIGG_SRC_SW</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_TRIGG_SRC_HW</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_TRIGG_SRC_SW</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:52c43528-a85b-4dcc-b5b5-7ab3e18e67ac">
                          <SHORT-NAME>AdcHwTrigSignal</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Configures on which edge of the hardware trigger signal the driver should reach, i.e. start the conversion.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_HW_TRIG_RISING_EDGE</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_HW_TRIG_FALLING_EDGE</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_HW_TRIG_RISING_EDGE</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_HW_TRIG_BOTH_EDGES</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:5fe66517-3dfa-49cf-b1cd-a111b7baaefe">
                          <SHORT-NAME>AdcHwTrigTimer</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reload value of the ADC module embedded timer. This parameter is not used by the current implementation.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>0</DEFAULT-VALUE>
                          <MAX>18446744073709551615</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-FUNCTION-NAME-DEF UUID="ECUC:aa328ce2-6361-49fa-8ba2-ca8904101cfd">
                          <SHORT-NAME>AdcNotification</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Callback function for each group. This function pointer is called everytime when the conversion of this group is completed.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                            <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                              <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                            </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                          </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                        </ECUC-FUNCTION-NAME-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:572a24d6-27ac-4f8c-85b9-1cefae44cb8c">
                          <SHORT-NAME>AdcStreamingBufferMode</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Select the streaming buffer as linear buffer (i.e. the ADC Driver stops the conversion as soon as the stream buffer is full) or as ring buffer (wraps around if the end of the stream buffer is reached).</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_STREAM_BUFFER_LINEAR</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_STREAM_BUFFER_CIRCULAR</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_STREAM_BUFFER_LINEAR</SHORT-NAME>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:3ca7b97c-36e2-4d2a-a199-37c07804cb65">
                          <SHORT-NAME>AdcEnableDoubleBuffering</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                            Enable/ Disable the Double Buffering feature for Adc group conversions. this Parameter can be configured only for groups configured with ADC_ACCESS_MODE_STREAMING Access Mode, and only if ADC_DMA is configured as the transfer method for the Adc Unit.
                                            When this parameter is Disabled, normal functionlaity shall be executed.
                                            Note: This is an Implementation Specific Parameter. This feature supported only for Groups which is configured as hardware trigger</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c08c3abb-86b5-4f8f-be15-672bb9fdf90c">
                          <SHORT-NAME>AdcEnableHalfInterrupt</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                          Enable/ Disable the interrupt when half sample complete for double bufferring feature. Double buffering must be enable for configure this feature. </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1862f873-395e-407f-82e6-1cb911c5faa4">
                          <SHORT-NAME>AdcStreamingNumSamples</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Number of ADC values to be acquired per channel in streaming access mode.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>1</DEFAULT-VALUE>
                          <MAX>255</MAX>
                          <MIN>1</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:c904ad1f-ea97-46c8-9263-13c638e22165">
                          <SHORT-NAME>AdcHwTrigSrc</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                    Selects the source for the eQADC trigger inputs (bits TSEL4_7 in SIU_ISEL register).
                                    SIU_ISEL select registers [4:5] are used to select a trigger source for command FIFOs in eQADC_A 
                                    SIU_ISEL select registers [6:7] are used to select a trigger source for command FIFOs in eQADC_B 
                                    Note: This is an Implementation Specific Parameter.
                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>FIFO0_RTI</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_RTI</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_PIT0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_PIT1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_PIT2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_PIT3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_ETRIG1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUA28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUA29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUA30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUA31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUB28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUB29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUB30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUB31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUC28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUC29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUC30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eTPUC31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_16</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_17</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_18</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_19</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_20</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_21</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS0_23</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_eMIOS1_2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO0_ETRIG0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_RTI</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_PIT0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_PIT1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_PIT2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_PIT3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUA7</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_ETRIG0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUA28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUA29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUA30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUA31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUB28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUB29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUB30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUB31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUC28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUC29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUC30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eTPUC31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_16</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_17</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_18</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_19</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_20</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_21</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS0_23</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_eMIOS1_3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO1_ETRIG1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_RTI</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_PIT0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_PIT1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_PIT2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_PIT3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUA14</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_ETRIG1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUA28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUA29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUA30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUA31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUB28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUB29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUB30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUB31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUC28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUC29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUC30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eTPUC31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_16</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_17</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_18</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_19</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_20</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_21</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS0_23</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_eMIOS1_7</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO2_ETRIG0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_RTI</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_PIT0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_PIT1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_PIT2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_PIT3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUA22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_ETRIG0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUA28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUA29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUA30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUA31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUB28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUB29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUB30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUB31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUC28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUC29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUC30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eTPUC31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_16</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_17</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_18</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_19</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_20</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_21</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS0_23</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_eMIOS1_6</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO3_ETRIG1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_RTI</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_PIT0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_PIT1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_PIT2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_PIT3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUA30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_ETRIG1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUA28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUA29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUA31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUB28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUB29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUB30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUB31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUC28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUC29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUC30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUC31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_16</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_17</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_18</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_19</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_20</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_21</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS0_23</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eTPUA27</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_eMIOS1_5</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO4_ETRIG0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_RTI</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_PIT0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_PIT1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_PIT2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_PIT3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_ETRIG0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUA28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUA29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUA30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUA31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUB28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUB29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUB30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUB31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUC28</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUC29</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUC30</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUC31</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_16</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_17</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_18</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_19</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_20</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_21</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_22</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS0_23</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eTPUA26</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_eMIOS1_4</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>FIFO5_ETRIG1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:d3d368be-d30b-4bd6-adcd-26c34727816a">
                          <SHORT-NAME>AdcGroupFifo</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Selects the FIFO on which the channels belongs to the group converted.
                              ADC_FIFO_0 to ADC_FIFO_2 is used for unit0 and unit2 while ADC_FIFO_3 to ADC_FIFO_5 is used for unit1 and unit3
                              by eQADC_A and eQADC_B
                              Note:- This is an Implementation Specific Parameter.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>ADC_FIFO_0</DEFAULT-VALUE>
                          <LITERALS>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_FIFO_0</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_FIFO_1</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_FIFO_2</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_FIFO_3</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_FIFO_4</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                            <ECUC-ENUMERATION-LITERAL-DEF>
                              <SHORT-NAME>ADC_FIFO_5</SHORT-NAME>
                              <ORIGIN>NXP</ORIGIN>
                            </ECUC-ENUMERATION-LITERAL-DEF>
                          </LITERALS>
                        </ECUC-ENUMERATION-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:2dbb0804-e88c-4f64-8bf9-b70ce22e5b71">
                          <SHORT-NAME>AdcWithoutInterrupts</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                            Enable/ Disable the occuring of ADC Interrupts and Reading of the group conversion results periodically without interrupts.
                                            A) When this parameter is enabled, interrupts are disabled .
                                            The conversion will run without software intervention (no interrupt generated anymore) and application can read the results
                                            by calling Adc_ReadGroup().
                                            B) When this parameter is enabled, the result buffer is no longer to be used to read the results as the results will be directly read from HW registers.
                                            When this parameter is Disabled, normal functionlaity shall be executed.
                                            On Cobra55, this feature only support for group with only one channel.
                                            Note: This is an Implementation Specific Parameter.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                      </PARAMETERS>
                      <REFERENCES>
                        <ECUC-REFERENCE-DEF UUID="ECUC:26fd14c8-d5af-4316-acc3-ddf94411ff8c">
                          <SHORT-NAME>AdcGroupDefinition</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Assignment of channels to a AdcGroups. For each AdcChannel that should belong to the group, a reference needs to be defined.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Adc/AdcConfigSet/AdcHwUnit/AdcChannel</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                      </REFERENCES>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                  </SUB-CONTAINERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5d3d9066-300f-4ba4-9d89-42717f28d942">
                  <SHORT-NAME>AdcDigitalFilterLength</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                Digital Filter Length (DFL bits in EQADC_ETDFR register).
                                Specifies the minimum number of system clocks that must the digital filter counter count
                                to recognize a logic state change on EQADC trigger input.
                                DFL  --------- Minimum number of system clocks
                                0    ---------      2
                                1    ---------      3
                                2    ---------      5
                                3    ---------      9
                                4    ---------     17
                                5    ---------     33
                                6    ---------     65
                                7    ---------    129
                                8    ---------    257
                                9    ---------    513
                                10   ---------   1025
                                11   ---------   2049
                                12   ---------   4097
                                13   ---------   8193
                                14   ---------  16385
                                15   ---------  32769
                                Note: This is an Implementation Specific Parameter.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:31fef1c1-2760-43e8-847f-6c3428e4a102">
                      <SHORT-NAME>AdcDigitalFilterLength0</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                Digital Filter Length (DFL bits in EQADC_ETDFR register) for EQADCA.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>5</DEFAULT-VALUE>
                      <MAX>15</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:31fef1c1-2420-43e8-847f-6c3538e4a102">
                      <SHORT-NAME>AdcDigitalFilterLength1</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                Digital Filter Length (DFL bits in EQADC_ETDFR register) for EQADCB.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>5</DEFAULT-VALUE>
                      <MAX>15</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5d3d9066-300f-4ba4-9d89-02717f28d967">
              <SHORT-NAME>AdcGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">General configuration (parameters) of the ADC Driver software module.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c2a39725-ca66-4165-9aa8-dc51d263ef72">
                  <SHORT-NAME>AdcDeInitApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Adds/removes the service Adc_DeInit() from the code.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ab29d43a-e9a4-4eed-9f4d-8559b4e39e89">
                  <SHORT-NAME>AdcDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enable/Disable Development Error Detection.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:1f75320a-0500-4767-b096-d9f9b2a372e6">
                  <SHORT-NAME>AdcEnableLimitCheck</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enable/disable limit checking feature in the ADC driver.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:30a4f3cf-e092-4deb-8353-a92a1738229d">
                  <SHORT-NAME>AdcEnableQueuing</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enable/Disable the Queue. Note that if AdcPriorityImplementation=ADC_PRIORITY_HW_SW this field is always enabled.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:e72dfb05-6a85-4661-8a6b-2aded1691995">
                  <SHORT-NAME>AdcEnableStartStopGroupApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Adds / removes the services Adc_StartGroupConversion() and Adc_StopGroupConversion from the code.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:0b3ecae2-f557-4f90-94f0-5452e9c03659">
                  <SHORT-NAME>AdcGrpNotifCapability</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Determines, if the group notification mechanism (the functions to enable and disable the notifications) is available at runtime.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:e2930cb1-2824-42e0-84fd-4e72fb180f7d">
                  <SHORT-NAME>AdcHwTriggerApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Adds / removes the services Adc_EnableHardwareTrigger() and Adc_DisableHardwareTrigger() from the code.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:b30e7432-c589-413d-bb14-fa157c615067">
                  <SHORT-NAME>AdcReadGroupApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Adds / removes the service Adc_ReadGroup() from the code.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6dde8f53-d250-4c27-bb2b-3c64b3d20df9">
                  <SHORT-NAME>AdcVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Adds / removes the service Adc_GetVersionInfo() from the code.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:58a45c6e-7392-4d34-8d22-7ff2cdb40fab">
                  <SHORT-NAME>AdcPriorityImplementation</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Select the Priority mechanism. In this version the ADC_PRIORITY_HW isn't used.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>ADC_PRIORITY_NONE</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>ADC_PRIORITY_HW</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>ADC_PRIORITY_HW_SW</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>ADC_PRIORITY_NONE</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:e842717e-7446-417d-97d4-b3bd7232b2ab">
                  <SHORT-NAME>AdcResultAlignment</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Alignment of ADC raw results in ADC result buffer (left/right alignment).</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>ADC_ALIGN_RIGHT</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>ADC_ALIGN_LEFT</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>ADC_ALIGN_RIGHT</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:3a07e4c9-908b-4a38-ab20-877acc8148a7">
                  <SHORT-NAME>AdcTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">This timeout is used to wait until the FIFO status is updated when EOQ flag is set
                        or Result fifo is cleared or fifo is disabled.
                        If the Status is not updated then after this timeout the ADC_E_TIMEOUT
                        production error will be reported and the rest of the functionality will be skipped.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>65535</DEFAULT-VALUE>
                  <MAX>4294967295</MAX>
                  <MIN>1000</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:227c9750-f44e-4373-b847-e0cec414d1a7">
                  <SHORT-NAME>AdcConvTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">This timeout is used to wait until the all the conversions pending in the CBuffer are done.
                                              If the Status is not updated within this timeout the ADC_E_TIMEOUT production error will
                                              be reported and the rest of the functionality will be skipped.
                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>65535</DEFAULT-VALUE>
                  <MAX>4294967295</MAX>
                  <MIN>1000</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66aa4b95-cf28-4be4-a243-d0dd6b0c648b">
                  <SHORT-NAME>AdcPriorityQueueMaxDepth</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Maximum depth of queue used for queuing of incoming conversion requests when hardware unit is busy.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>65535</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:e2930cb1-2824-42e0-84fd-4e72fb180e7d">
                  <SHORT-NAME>AdcLowPowerStatesSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Adds / removes all power state management related APIs (Adc_SetPowerState, Adc_GetCurrentPowerState, Adc_GetTargetPowerState, Adc_PreparePowerState, Adc_Main_PowerTransitionManager), indicating if the HW offers low power state management. This parameter is disabled, there is no power management support implemented for this platform.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c20b0644-70bf-435d-ace6-8626ec469675">
                  <SHORT-NAME>AdcPowerStateAsynchTransitionMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / disables support of the ADCDriver to the asynchronous power state transition. This feature is not implemented on this platform.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:66904f78-ff07-4ed3-878e-401a3430cd38">
                  <SHORT-NAME>AdcPowerStateConfig</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Each instance of this parameter defines a power state and the callback to be called when this power state is reached.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:41902199-e783-4afe-bef3-41c69e08b32d">
                      <SHORT-NAME>AdcPowerState</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Each instance of this parameter describes a different power state 
                             supported by the ADC HW. It should be defined by the HW supplier and 
                             used by the ADCDriver to reference specific HW configurations which set 
                             the ADC HW module in the referenced power state. At least the power mode
                             corresponding to full power state shall be always configured.
                             This parameter shall only be configured if the parameter AdcLowPowerStatesSupport is set to true.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>18446744073709551615</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-FUNCTION-NAME-DEF UUID="ECUC:b9c222fc-6b92-40e9-922e-f73addaf2320">
                      <SHORT-NAME>AdcPowerStateReadyCbkRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Each instance of this parameter contains a reference to a power mode callback defined in a CDD or IoHwAbs component.
                             This parameter shall only be configured if the parameter AdcLowPowerStatesSupport is set to true</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                        <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                          <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                        </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    </ECUC-FUNCTION-NAME-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:3e265978-346e-4de7-be8c-c406a7ef02e0">
              <SHORT-NAME>AdcPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">Additional published parameters not covered by CommonPublishedInformation container.
                    Note that these parameters do not have any configuration class setting, since they are published information.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:acb88fcc-ebdd-4232-b93f-d6c818ced64e">
                  <SHORT-NAME>AdcChannelValueSigned</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Information whether the result value of the ADC driver has sign information (true) or not (false). If the result shall be interpreted as signed value it shall apply to C-language rules.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:d70338f5-2be1-4d89-9cdf-d012ba5db883">
                  <SHORT-NAME>AdcGroupFirstChannelFixed</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Information whether the first channel of an ADC Channel group can be configured (false) or is fixed (true) to a value determined by the ADC HW Unit.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:dbe4e009-1c76-47ef-861c-9a4ea2871965">
                  <SHORT-NAME>AdcMaxChannelResolution</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Maximum Channel resolution in bits (does not specify accuracy).</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>12</DEFAULT-VALUE>
                  <MAX>63</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:8a492572-bd3e-4c18-b2b3-4923f25b9b1e">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                      Common container, aggregated by all modules. It contains published information about vendor and versions.
                  </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e7e9d572-8eef-4b6c-9433-8aad276eec7c">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:3d870209-be10-47c3-9857-538e620076c9">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:a83e5ff1-972e-4db3-8da8-0bbbc7689ec2">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:dace0d32-017d-481a-844b-ca56c5fe5d98">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Module ID of this module from Module List.
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>123</DEFAULT-VALUE>
                  <MAX>123</MAX>
                  <MIN>123</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:931ea035-fc4a-451a-a9d6-8a45883e4cf1">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:bc6133b1-3991-449e-8584-49b11eff3a7f">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:7f523334-ef23-4b15-b142-694a9d63fab9">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:36a6319a-24af-44aa-bde8-4119ca8e61fd">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      In driver modules which can be instantiated several times on a single ECU, BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name. 
                      This parameter is used to specify the vendor specific name. In total, the implementation specific name is generated as follows:
                      &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt;.
                      E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 
                      This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:4fec8752-a2fc-44db-811a-3ee2a51d5ae1">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                          Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:a840d02b-4967-4e98-8e41-b89fd1272780">
              <SHORT-NAME>AutosarExt</SHORT-NAME>
              <DESC>
                <L-2 L="EN">Autosar Extension API settings.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:cf08470c-77d7-4326-a615-90a0e35c390f">
                  <SHORT-NAME>AdcEnableGroupDependentChannelNames</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">This is used to generate ADC symbolic names, that depend also on the ADC group 
                        to which each ADC channel is mapped. The generated symbolic name will be something 
                        like:
                        #define &amp;quotADC_GroupName&amp;quot_&amp;quotADC_ChannelName&amp;quot  &amp;quotChannel index value&amp;quot,
                        where &amp;quotChannel index value&amp;quot is the channel index in the current group.
                        Channel indexes in each group are generated to allow result buffer access by symbolic names.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:00118f07-32be-429d-8b41-3f7dc39d1848">
                  <SHORT-NAME>AdcEnableCalibration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                          If this parameter has been configured to &quot;TRUE&quot;, the Autosar Extension function &quot;Adc_Calibrate()&quot;  shall be accessible, otherwise this function shall be removed from the code.
                          This functionality is not available for this platform (not supported by HW).
                          NoteThis is an Implementation Specific Parameter.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:8436de9b-c7e1-4720-9e80-145e3870a2cb">
                  <SHORT-NAME>AdcDisableDemReportErrorStatus</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enable/Disable Dem error reporting.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:00118f07-32be-429d-8b41-3f7dc79d1848">
                  <SHORT-NAME>AdcEnableDualClockMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                        The Adc driver shall provide an optional API and configuration parameters for changing the base clock of the controlled hardware. 
                        This shall comprise the conversion timing registers of the ADC as well.
                        Per default this optional functionality and configuration parameters shall be disabled..</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6d78d92b-c387-4656-ba8c-8113fdef7247">
                  <SHORT-NAME>AdcEnableDoubleBufferingOptimization</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Implementation Specific Parameter.
                         Enable/Disable The Adc driver double buffering optimization for Streaming access.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6d78d92b-c387-4656-ba8c-8113fdef7243">
                  <SHORT-NAME>AdcOptimizeOneShotHwTriggerConversions</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN"> Implementation Specific Parameter.
                         Enable/Disable The Adc driver optimization for HW Triggered groups, OneShot, Single access.
                         If Enabled, other types of groups cannot be configured in ADC driver and the code for interrupt routine / Dma notification will be optimized for speed.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:84a3553a-7f99-48a2-be06-5d97ebbc2eff">
                  <SHORT-NAME>AdcEnableUserModeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                When this parameter is enabled, the Adc module will adapt to run from User Mode, with the following measures:
                                by using 'call trusted function' stubs for all internal function calls that access registers requiring supervisor mode.
                                for more information, please see chapter 5.7 User Mode Support in IM 
                                Note: Implementation Specific Parameter.
                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:89409b54-221f-496a-9d8a-e7c524795d8f">
              <SHORT-NAME>AdcDemEventParameterRefs</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                          Container for the references to DemEventParameter elements which shall be invoked using the Dem_ReportErrorStatus API in case the corresponding error occurs. The EventId is taken from the referenced DemEventParameter's DemEventId value. The standardized errors are provided in the container and can be extended by vendor specific error references.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <REFERENCES>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:43e34850-f886-4b31-a12c-e1c8094b9390">
                  <SHORT-NAME>ADC_E_TIMEOUT</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                            Reference to configured DEM event to report &quot;Timeout failure&quot;.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>