<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:311f62c9-81d6-479d-b622-304eddbd28d1">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:b0cef610-e29c-401b-bc6c-eade35441720">
          <SHORT-NAME>Wdg_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Wdg</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:7413c125-5c5c-4881-8404-8946cbc33df4">
          <SHORT-NAME>Wdg</SHORT-NAME>
          <DESC>
            <L-2 L="EN">
                                    
                                    Wdg
                                    Configuration of the Wdg (Watchdog driver) module
                                    </L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.6.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2014-10-31</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <REFINED-MODULE-DEF-REF DEST="ECUC-MODULE-DEF">/AUTOSAR/EcucDefs/Wdg</REFINED-MODULE-DEF-REF>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-LINK-TIME</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:7d918cce-a524-4501-ad5f-9c6c8e7fc9c3">
              <SHORT-NAME>WdgDemEventParameterRefs</SHORT-NAME>
              <DESC>
                <L-2 L="EN">Container for the references to DemEventParameter elements which shall be invoked using the API Dem_SetEventStatus in case the corresponding error occurs. The EventId is taken from the referenced DemEventParameter's DemEventId value.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <REFERENCES>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:6055f74a-670e-4f85-9621-982c8aba0939">
                  <SHORT-NAME>WDG_E_DISABLE_REJECTED</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Initialization or mode switch failed because it would disable the watchdog&quot; has occurred.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:e208b5bb-0a84-4234-9e79-ac8b22dea3b5">
                  <SHORT-NAME>WDG_E_MODE_FAILED</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Setting a watchdog mode failed (during initialization or mode switch)&quot; has occurred.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:3bfa03e8-6e4f-4e87-815e-5f500e6183f9">
                  <SHORT-NAME>WDG_E_CORRUPT_CONFIG</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when Wdg detects a memory corruption.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:40d548c8-776a-4f72-b62e-cc3e89089762">
                  <SHORT-NAME>WDG_E_UNLOCKED</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when Wdg detects the call of SafetyCheck when the driver is unlocked.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:4d5753dd-9191-4ecd-8b85-c88d3f00abfb">
                  <SHORT-NAME>WDG_E_INVALID_PARAMETER</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when Wdg detects the call of a function was made with invalid parameters.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:2d5cdae7-bfa1-40dc-9954-dadda25e8047">
                  <SHORT-NAME>WDG_E_FORBIDDEN_INVOCATION</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when Wdg detects a non reentrant function shall detect if it is pre-empting itself</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:d2bcaf6e-dd65-43fe-931d-c8aa7e66e483">
                  <SHORT-NAME>WDG_E_INVALID_CALL</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Vendor specific: Reference to the DemEventParameter which shall be issued when Wdg detects calling on a locked configuration.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:87f0db1a-53bd-46bb-a6f7-3f7258353e54">
              <SHORT-NAME>WdgGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                        
                                        WdgGeneral
                                        All general parameters of the watchdog driver are collected here.
                                        </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:15153f07-87cb-44aa-9ba7-9cf6e972c586">
                  <SHORT-NAME>WdgDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Development Error Detect
                                            Compile switch to enable / disable development error detection for this module.
                                            True: Development error detection enabled
                                            False: Development error detection disabled
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:d3708048-7953-4094-b66f-dd5378416d85">
                  <SHORT-NAME>WdgDisableAllowed</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Disable Allowed
                                            Compile switch to allow / forbid disabling the watchdog driver during runtime.
                                            True: Disabling the watchdog driver at runtime is allowed
                                            False:Disabling the watchdog driver at runtime is not allowed
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:fbb4800a-1114-4ef4-9a8b-396befc654cd">
                  <SHORT-NAME>WdgEnableUserModeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                          
                                          Wdg Enable User Mode Support
                                               When this parameter is enabled, the Wdg module will adapt to run from User Mode, with
                                               the following measure : configuring REG_PROT for Wdg IPs so that the registers under
                                               protection can be accessed from user mode by setting UAA bit in REG_PROT_GCR to 1
                                               for more information and availability on this platform, please see chapter &quot;User Mode
                                               Support&quot; in IM.
                                               
                                               True: Wdg module will adapt to run from User Mode.
                                               
                                               False:Wdg module will not apdapt to run from User Mode.
                                               
                                          If this parameter is not ediatable, that means Wdg driver can run in User Mode.
                                          </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-4dbc-9683-482d6de10c37">
                  <SHORT-NAME>WdgIndex</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Instance 0 Index
                                            Represents the watchdog driver's ID for Instance 0 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-4dbc-9683-482d6de10c41">
                  <SHORT-NAME>WdgIndex1</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 1 Index
                                            Represents the watchdog driver's ID for Instance 1 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-4dbc-9683-482d6de10c67">
                  <SHORT-NAME>WdgIndex2</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 2 Index
                                            Represents the watchdog driver's ID for Instance 2 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>2</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-4dbc-9623-422d6de10c67">
                  <SHORT-NAME>WdgIndex3</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 3 Index
                                            Represents the watchdog driver's ID for Instance 3 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-4dbc-9613-412d6de10c67">
                  <SHORT-NAME>WdgIndex4</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 4 Index
                                            Represents the watchdog driver's ID for Instance 4 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-4dbc-9613-41229de10c67">
                  <SHORT-NAME>WdgIndex5</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 5 Index
                                            Represents the watchdog driver's ID for Instance 5 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>5</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-22bc-9613-412d6de10c68">
                  <SHORT-NAME>WdgIndex6</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 6 Index
                                            Represents the watchdog driver's ID for Instance 6 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>6</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-22bc-9613-412d6de10c69">
                  <SHORT-NAME>WdgIndex7</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 7 Index
                                            Represents the watchdog driver's ID for Instance 7 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>7</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-22bc-9613-412d6de10c70">
                  <SHORT-NAME>WdgIndex8</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 8 Index
                                            Represents the watchdog driver's ID for Instance 8 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>8</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-22bc-9613-412d6de10c71">
                  <SHORT-NAME>WdgIndex9</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 9 Index
                                            Represents the watchdog driver's ID for Instance 9 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>9</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:66c3dd06-42fe-22bc-9613-412d6de10c72">
                  <SHORT-NAME>WdgIndex10</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Vendor specific:
                                            Wdg Instance 10 Index
                                            Represents the watchdog driver's ID for Instance 10 so that it can be referenced by the watchdog interface.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>10</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-FLOAT-PARAM-DEF UUID="ECUC:8c6a446f-943e-4410-8efb-a29445666618">
                  <SHORT-NAME>WdgInitialTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Initial Timeout
                                            The initial timeout (sec) for the trigger condition to be initialized during Init function. It shall be not larger than WdgMaxTimeout.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0.0</DEFAULT-VALUE>
                  <MAX>65.535</MAX>
                  <MIN>0.0</MIN>
                </ECUC-FLOAT-PARAM-DEF>
                <ECUC-FLOAT-PARAM-DEF UUID="ECUC:429bdb31-4cde-4b03-beae-44b1fbf61541">
                  <SHORT-NAME>WdgMaxTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Max Timeout
                                            The maximum timeout (sec) to which the watchdog trigger condition can be initialized.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0.0</DEFAULT-VALUE>
                  <MAX>65.535</MAX>
                  <MIN>0.0</MIN>
                </ECUC-FLOAT-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:db420f37-919c-409b-b421-e035178222dc">
                  <SHORT-NAME>WdgRunArea</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Run Area
                                            Represents the watchdog driver execution area is either from ROM(Flash) or RAM as required with the particular microcontroller.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>ROM</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>RAM</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>ROM</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:9c57e64c-49c4-4ab5-beaa-bea629c8b57d">
                  <SHORT-NAME>WdgTriggerLocation</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Trigger Location
                                            Location (memory address) of the watchdog trigger routine.
                                            Note:Not supported by the current hardware.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:280c6066-e239-4fc5-97cd-5cc99cdafb8e">
                  <SHORT-NAME>WdgCallbackNotification0</SHORT-NAME>
                  <DESC>
                    <L-2 L="FOR-ALL">
                                            Vendor specific:
                                            WdgCallbackNotification0
                                            Callback notification for the ISR Wdg_Swt0_Isr function
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
                <ECUC-FUNCTION-NAME-DEF UUID="ECUC:280c6066-e239-4fc5-97cd-5cc99cdbfb9e">
                  <SHORT-NAME>WdgCallbackNotification1</SHORT-NAME>
                  <DESC>
                    <L-2 L="FOR-ALL">
                                            Vendor specific:
                                            WdgCallbackNotification1
                                            Callback notification for the ISR Wdg_Swt1_Isr function
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                    </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                  </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                </ECUC-FUNCTION-NAME-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:496c0201-1cbb-4aae-91e2-92e53ddf6ad1">
                  <SHORT-NAME>WdgVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg VersionInfo Api
                                            Compile switch to enable or disable the version information API.
                                            True: API enabled
                                            False:API disabled
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:ee17a92f-c2de-417d-9eda-4c52a5998d3d">
                  <SHORT-NAME>AutosarExt</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Autosar Extension settings.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9936de9b-c7e1-4720-9e80-145e3870a2cb">
                      <SHORT-NAME>WdgDisableDemReportErrorStatus</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enable/Disable Dem error reporting.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:8c5fa102-9c46-4246-9e89-28309ad786ec">
              <SHORT-NAME>WdgClockReferencePoint</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                                This container contains a parameter, which represents a reference to a container of the type McuClockReferencePoint (defined in module MCU). 
                                                If the cip is trimmed (internal RC oscillator clock FIRC running at 48MHz frequency), then configure in MCU a reference point of FIRC type
                                                with 48MHz frequency. If the cip is not trimmed (FIRC running at frequency different than 48MHz), then configure in MCU a reference point 
                                                of CUSTOM type with the real FIRC frequency measured on the cip.
                                            </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <REFERENCES>
                <ECUC-REFERENCE-DEF UUID="ECUC:c474f2e4-385a-48de-a90d-5745a7b836ab">
                  <SHORT-NAME>WdgClockReference</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                    
                                                        Reference to a container of the type McuClockReferencePoint, to select an input clock.
                                                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DESTINATION-REF>
                </ECUC-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:24d0c999-068c-4345-b9a9-768ff6303c06">
              <SHORT-NAME>WdgSettingsConfig</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                            
                                            WdgSettingsConfig
                                            Configuration items for the different watchdog settings, including those for external watchdog hardware.
                                            </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:6a19f763-6eec-4080-95e7-aa532a493624">
                  <SHORT-NAME>WdgInstance</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                Vendor specific:
                                                Wdg Hardware Instance
                                                Select specific hardware instance for watchdog driver initialization.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>SWT0</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>SWT0</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>SWT1</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:1a56da9d-0f04-44af-a072-42f174aebd23">
                  <SHORT-NAME>WdgDefaultMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                Wdg Default Mode
                                                Default mode for watchdog driver initialization.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>WDGIF_SLOW_MODE</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>WDGIF_FAST_MODE</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>WDGIF_OFF_MODE</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>WDGIF_SLOW_MODE</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:1a56da9d-0h04-4daf-a022-42b17naebd23">
                  <SHORT-NAME>WdgInterruptContentEnable</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                Vendor specific:
                                                Wdg Interrupt Enable
                                                This parametter is used to generate interrupt content for each SWT.
                                                True = Interrupt content is generated.
                                                False = Interrupt content is not generated.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
              <REFERENCES>
                <ECUC-CHOICE-REFERENCE-DEF UUID="ECUC:3c599e87-2138-4c57-ba30-aa4f5b34d2a7">
                  <SHORT-NAME>WdgExternalTriggerCounterRef</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                Vendor specific:
                                                Wdg External Trigger Counter
                                                Reference to the GptChannel configuration which set for the watchdog servicing routine implementation.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REFS>
                    <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Gpt/GptChannelConfigSet/GptChannelConfiguration</DESTINATION-REF>
                  </DESTINATION-REFS>
                </ECUC-CHOICE-REFERENCE-DEF>
              </REFERENCES>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:2d2f3c57-b55c-47be-bc21-43ab8da6ed9a">
                  <SHORT-NAME>WdgExternalConfiguration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                WdgExternalConfiguration
                                                Configuration items for an external watchdog hardware
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <REFERENCES>
                    <ECUC-CHOICE-REFERENCE-DEF UUID="ECUC:5028835a-baad-440d-8ce0-04641c8d69ce">
                      <SHORT-NAME>WdgExternalContainerRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    WdgExternalContainerRef
                                                    Reference to either
                                                    - a DioChannelGroup container in case the hardware watchdog is connected via DIO pins
                                                    - a SpiSequenceConfiguration container in case the watchdog hardware is accessed via SPI
                                                    Note:This parameter is not used by current implementation
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REFS>
                        <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dio/DioConfig/DioPort/DioChannelGroup</DESTINATION-REF>
                        <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Spi/SpiDriver/SpiSequence</DESTINATION-REF>
                      </DESTINATION-REFS>
                    </ECUC-CHOICE-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:f7dffb47-f373-43d8-b758-2577791bb6e6">
                  <SHORT-NAME>WdgSettingsFast</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                WdgSettingsFast
                                                Hardware dependent settings for the watchdog driver's fast mode.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:702a1683-9305-42c9-9c77-c7455452cf0d">
                      <SHORT-NAME>WdgClockValue</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Clock Value 
                                                    This is the Implementation Specific parameter.
                                                    Indicates Wdg Clock Value in KHz (internal oscilator clock value is by default 128KHz).
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>133000</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:1336fa79-9ce9-449b-8866-ae17cd0f308d">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster0</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 0. .
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:43c007ea-12cb-4fee-bf87-1159c8608328">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster1</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 1.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:5a2b9695-a274-48e5-b10a-2860e9dde840">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster2</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 2.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:eef61052-6db8-4b69-b12e-82d8409d8265">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster3</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 3.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:94702287-1899-4e6f-84d1-3d05f5d856e0">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster4</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 4.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6cde22f9-77d5-462f-affd-5a9acca1300e">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster5</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 5.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:15bfcb79-b3dd-4f63-9ba5-e4a9083c134f">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster6</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 6.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:498ca09d-a88a-4807-ab3c-53337bf1929d">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster7</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 7.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:4bccc3e2-347d-458d-8345-648f027cf6db">
                      <SHORT-NAME>WdgKeyedService</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Fixed Service Sequence or Keyed Service Mode .
                                                    False = Fixed Service Sequence, the fixed sequence 0xA602, 0xB480 is used to service the watchdog.
                                                    True = Keyed Service Mode, two pseudorandom key values are used to service the watchdog.
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:cf66d53f-b410-4a07-ae4a-2c75c0fafae4">
                      <SHORT-NAME>WdgServiceKeyValue</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Service Key
                                                    This value is the initial service key value used in keyed service mode.
                                                    If SWT_CR[KEY] is set, the next key value to be written to the SWT_SR is (17*SK+3) mod 2^16.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>65535</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:2902b8f1-5e72-4243-b204-ece315fe120c">
                      <SHORT-NAME>WdgSoftLockConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    SoftLockConfiguration
                                                    This is the Implementation Specific parameter.Soft Lock for the Software Watchdog Timer Control (SWTCR) Register
                                                    
                                                    Enabled : SWTCR can be read or written.
                                                    Disabled: SWTCR can be read only.
                                                    An unlock sequence should be written into service register before this register can again be written.
                                                    
                                                    The setting of this switch is intended to prevent accidental writes of the SWTCR from changing the defined system watchdog configuration.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:29f9a76d-09f5-4ab8-95bd-afb838cc44bf">
                      <SHORT-NAME>WdgHardLockConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Read Only
                                                    This is the Implementation Specific parameter.HardLock for the Software Watchdog Timer Control (SWTCR) Register
                                                    
                                                    Enabled :  SWTCR can be read or written.
                                                    Disabled:  SWTCR can be read only.
                                                    A system reset is required before this register can again be written.
                                                    
                                                    The setting of this switch is intended to prevent accidental writes of the SWTCR from changing the defined system watchdog configuration.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:883ced91-72b6-43af-ac42-391c67874a5e">
                      <SHORT-NAME>WdgRunsInStopMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Runs in Stop Mode
                                                    This is the Implementation Specific parameter.
                                                    
                                                    Enabled:   SWT continues to count even while the processor core is in stop mode.
                                                    Disabled:  SWT stops counting if the processor core is in stop mode.
                                                    
                                                    Note: The 'WdgRunsInStopMode' parameter specifies if the watchdog timer should run or not while the clock to the core is halted.
                                                    This is true only for the STOP0 mode of the controller. It will always run while the controller is in the HALT0 mode.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:345b2600-9e87-4e0a-8d93-4d68cbfa55ea">
                      <SHORT-NAME>WdgRunsInDebugMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Runs In Debug Mode
                                                    This is the Implementation Specific parameter.
                                                    
                                                    Enabled:   SWT continues to count even while the device enters the debug mode.
                                                    Disabled:  SWT stops counting if the processor core when the device enters the debug mode
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:380c37c4-0885-4131-848a-435ed3c204a1">
                      <SHORT-NAME>WdgOperationMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Operation Mode
                                                    This is the Implementation Specific parameter.
                                                    
                                                    ResetOnTimeOut:   Generate a reset on a time-out.
                                                    Interrupt:    Generate an interrupt on an initial time-out, reset on a second consecutive time-out.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>ResetOnTimeOut</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ResetOnTimeOut</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Interrupt</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:380c37c4-0885-4131-848a-435ed3c205a2">
                      <SHORT-NAME>WdgResetOnInvalidAccess</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Reset on Invalid Access
                                                    If window mode is enabled, the service sequence must be
                                                    performed in the last part of the window time out period. The window is open when
                                                    the down counter is less than the value in the SWT_WN register. Outside of this window,
                                                    service sequence writes are invalid access and generate:
                                                    
                                                    BusError:    Invalid access to the SWT generates a bus error.
                                                    SystemReset: Invalid access to the SWT causes a system reset if WEN=1.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>SystemReset</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>BusError</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SystemReset</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:2e702c08-9a3f-407f-9476-e14c2d713c75">
                      <SHORT-NAME>WdgClockSelection</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Clock Selection
                                                    The SWT counter clock is the FIRC - 48Mhz. 
                                                    The value of the clock need to
                                                    be set up in the Wdg/WdgGeneral/WdgClockValue. 
                                                    The value set up in the WdgClockValue will be used
                                                    by all the configurations and it is a precompile 
                                                    parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>OscillatorClock</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>OscillatorClock</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SystemClock</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-FLOAT-PARAM-DEF UUID="ECUC:058e63b2-5717-4823-a47a-2863e6c27cf6">
                      <SHORT-NAME>WdgTimeoutPeriod</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Timeout Period
                                                     Wdg Timeout Period
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0.002</DEFAULT-VALUE>
                      <MAX>65.536</MAX>
                      <MIN>0.002</MIN>
                    </ECUC-FLOAT-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:cbf1d6ba-56ed-484f-932c-1af41d4b04f9">
                      <SHORT-NAME>WdgWindowMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg WindowMode.
                                                    
                                                    Disabled:   Regular mode, service sequence can be done at any time.
                                                    Enabled :  Windowed mode, the service sequence is only valid when the down counter is less than value in the SWTWN register.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-FLOAT-PARAM-DEF UUID="ECUC:80fbabee-e664-4a94-88b3-1fb549e7d0b7">
                      <SHORT-NAME>WdgWindowPeriod</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Window Period
                                                    This is the Implementation Specific parameter.
                                                    Window start value. When window mode is enabled, the service sequence can only be written when
                                                    the internal down counter is less than this value.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0.0</DEFAULT-VALUE>
                      <MAX>89.4784853125</MAX>
                      <MIN>0.0</MIN>
                    </ECUC-FLOAT-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:f123edc2-382d-4d8e-9e96-7b23c31c31db">
                      <SHORT-NAME>WdgClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to the WdgClockReferencePoint from which the clock is derived.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Wdg/WdgClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:7081fa45-e0bb-49c6-b77d-705c26c6ea12">
                  <SHORT-NAME>WdgSettingsOff</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                WdgSettingsOff
                                                Hardware dependent settings for the watchdog driver's off mode.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:bf933db3-a35c-4bbd-9da5-74bf8165519f">
                      <SHORT-NAME>WdgSoftLockConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    SoftLockConfiguration
                                                    This is the Implementation Specific parameter.Soft Lock for the Software Watchdog Timer Control (SWTCR) Register
                                                    
                                                    Enabled : SWTCR can be read or written.
                                                    Disabled: SWTCR can be read only.
                                                    An unlock sequence should be written into service register before this register can again be written.
                                                    
                                                    The setting of this switch is intended to prevent accidental writes of the SWTCR from changing the defined system watchdog configuration.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:b5c1556a-4850-4d0d-9558-31f41dca9cbd">
                      <SHORT-NAME>WdgHardLockConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Read Only
                                                    This is the Implementation Specific parameter.HardLock for the Software Watchdog Timer Control (SWTCR) Register
                                                    
                                                    Enabled :  SWTCR can be read or written.
                                                    Disabled:  SWTCR can be read only.
                                                    A system reset is required before this register can again be written.
                                                    
                                                    The setting of this switch is intended to prevent accidental writes of the SWTCR from changing the defined system watchdog configuration.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:8d308a63-7f0b-471b-b0f4-b64fb5702aa3">
                  <SHORT-NAME>WdgSettingsSlow</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                                
                                                WdgSettingsSlow
                                                Hardware dependent settings for the watchdog driver's slow mode.
                                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:702a458a-9305-42c9-9c77-c7455452cf0d">
                      <SHORT-NAME>WdgClockValue</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Clock Value 
                                                    This is the Implementation Specific parameter.
                                                    Indicates Wdg Clock Value in KHz (internal oscilator clock value is by default 128KHz).
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>133000</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:af43474c-c584-478b-a332-e8551f3886fe">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster0</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 0. .
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:15f3a3ad-6820-4c7c-bd25-68ce0ac67815">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster1</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 1.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c92340c3-30ff-4bed-86e3-7616c29893b8">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster2</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 2.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:38a73bff-f3cd-40b4-be30-df57b19974e0">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster3</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 3.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7713df84-a70d-4803-8580-2b3474e3f0a3">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster4</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 4.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:5ee477b2-6251-442f-8c2f-8945ebfccf93">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster5</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 5.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:202c51ff-94f4-4163-b7ca-f9c404995b90">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster6</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 6.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:0e5e3633-728f-46f0-a451-f78d94039828">
                      <SHORT-NAME>WdgMasterAccessProtectionforMaster7</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Master Access Protection for Master 7.
                                                    False = Access for the master is not enabled.
                                                    True = Access for the master is enabled
                                                    NoteThis is an Implementation Specific Parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:1d9e21a8-bfe4-4d5d-9bd4-926bdbab56ce">
                      <SHORT-NAME>WdgKeyedService</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Vendor specific:
                                                Fixed Service Sequence or Keyed Service Mode .
                                                False = Fixed Service Sequence, the fixed sequence 0xA602, 0xB480 is used to service the watchdog.
                                                True = Keyed Service Mode, two pseudorandom key values are used to service the watchdog.
                                                NoteThis is an Implementation Specific Parameter.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:7383a7c2-835d-400a-b521-65453c1c5176">
                      <SHORT-NAME>WdgServiceKeyValue</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Service Key
                                                    This value is the initial service key value used in keyed service mode.
                                                    If SWT_CR[KEY] is set, the next key value to be written to the SWT_SR is (17*SK+3) mod 2^16.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>65535</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:50758c2f-a5f6-421e-a07d-70c64ac70376">
                      <SHORT-NAME>WdgSoftLockConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    SoftLockConfiguration
                                                    This is the Implementation Specific parameter.Soft Lock for the Software Watchdog Timer Control (SWTCR) Register
                                                    
                                                    Enabled : SWTCR can be read or written.
                                                    Disabled: SWTCR can be read only.
                                                    An unlock sequence should be written into service register before this register can again be written.
                                                    
                                                    The setting of this switch is intended to prevent accidental writes of the SWTCR from changing the defined system watchdog configuration.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7fc5558b-3c7c-4341-bd9e-9f5ea6f61e40">
                      <SHORT-NAME>WdgHardLockConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Read Only
                                                    This is the Implementation Specific parameter.HardLock for the Software Watchdog Timer Control (SWTCR) Register
                                                    
                                                    Enabled :  SWTCR can be read or written.
                                                    Disabled:  SWTCR can be read only.
                                                    A system reset is required before this register can again be written.
                                                    
                                                    The setting of this switch is intended to prevent accidental writes of the SWTCR from changing the defined system watchdog configuration.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:45d0cece-2aa2-4fc3-a214-c658cb3b5be2">
                      <SHORT-NAME>WdgRunsInStopMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Runs in Stop Mode
                                                    This is the Implementation Specific parameter.
                                                    
                                                    Enabled:   SWT continues to count even while the processor core is in stop mode.
                                                    Disabled:  SWT stops counting if the processor core is in stop mode.
                                                    
                                                    Note: The 'WdgRunsInStopMode' parameter specifies if the watchdog timer should run or not while the clock to the core is halted.
                                                    This is true only for the STOP0 mode of the controller. It will always run while the controller is in the HALT0 mode.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:78aa306d-c9a8-434b-be61-e69e2f47ce8b">
                      <SHORT-NAME>WdgRunsInDebugMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Runs In Debug Mode
                                                    This is the Implementation Specific parameter.
                                                    
                                                    Enabled:   SWT continues to count even while the device enters the debug mode.
                                                    Disabled:  SWT stops counting if the processor core when the device enters the debug mode.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:6c868a9e-19cd-46cb-b95c-518666f94df5">
                      <SHORT-NAME>WdgOperationMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Operation Mode
                                                    This is the Implementation Specific parameter.
                                                    
                                                    ResetOnTimeOut:   Generate a reset on a time-out.
                                                    Interrupt:    Generate an interrupt on an initial time-out, reset on a second consecutive time-out.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>ResetOnTimeOut</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ResetOnTimeOut</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>Interrupt</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:380c37c4-0885-4131-848a-435ed3c108a8">
                      <SHORT-NAME>WdgResetOnInvalidAccess</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Reset on Invalid Access
                                                    If window mode is enabled, the service sequence must be
                                                    performed in the last part of the window time out period. The window is open when
                                                    the down counter is less than the value in the SWT_WN register. Outside of this window,
                                                    service sequence writes are invalid access and generate:
                                                    
                                                    BusError:    Invalid access to the SWT generates a bus error.
                                                    SystemReset: Invalid access to the SWT causes a system reset if WEN=1.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>SystemReset</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>BusError</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SystemReset</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:2e702c03-9a3f-407f-9476-e14c2d713c75">
                      <SHORT-NAME>WdgClockSelection</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Clock Selection
                                                    The SWT counter clock is the FIRC - 48Mhz. 
                                                    The value of the clock need to
                                                    be set up in the Wdg/WdgGeneral/WdgClockValue. 
                                                    The value set up in the WdgClockValue will be used
                                                    by all the configurations and it is a precompile 
                                                    parameter.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>OscillatorClock</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>OscillatorClock</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SystemClock</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-FLOAT-PARAM-DEF UUID="ECUC:5eea5665-d07c-48e8-9a70-df01294b42dd">
                      <SHORT-NAME>WdgTimeoutPeriod</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Timeout Period
                                                    This is the Implementation Specific parameter.
                                                    Software Watchdog Time-Out Period in seconds. Selects the time-out period for the SWT.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0.002</DEFAULT-VALUE>
                      <MAX>65.536</MAX>
                      <MIN>0.002</MIN>
                    </ECUC-FLOAT-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:805f98b6-c65d-44ec-b470-02f172a3ef1f">
                      <SHORT-NAME>WdgWindowMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg WindowMode.
                                                    
                                                    Disabled:   Regular mode, service sequence can be done at any time.
                                                    Enabled :  Windowed mode, the service sequence is only valid when the down counter is less than value in the SWTWN register.
                                                    
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-FLOAT-PARAM-DEF UUID="ECUC:40d77dbd-b1d1-4a94-b243-3d3bbaeba91b">
                      <SHORT-NAME>WdgWindowPeriod</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                    
                                                    Vendor specific:
                                                    Wdg Window Period
                                                    This is the Implementation Specific parameter.
                                                    Window start value. When window mode is enabled, the service sequence can only be written when
                                                    the internal down counter is less than this value.
                                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0.0</DEFAULT-VALUE>
                      <MAX>89.4784853125</MAX>
                      <MIN>0.0</MIN>
                    </ECUC-FLOAT-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:f111edc2-382d-4d8e-9e96-7b23c31c31db">
                      <SHORT-NAME>WdgClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                
                                                Reference to the WdgClockReferencePoint from which the clock is derived.
                                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T2D41M10I0R0/Wdg/WdgClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:f95ef93f-f2e6-4fcd-a03a-506d16e374f0">
              <SHORT-NAME>WdgPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                        
                                        WdgPublishedInformation
                                        Container holding all Wdg specific published information parameters
                                        </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:193df69e-1eb1-437b-91ea-ebf29974bee4">
                  <SHORT-NAME>WdgTriggerMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                            Wdg Trigger Mode
                                            Watchdog trigger mode (toggle/window/both).
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>WDG_BOTH</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>WDG_BOTH</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>WDG_TOGGLE</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>WDG_WINDOW</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:c9239c3a-99db-4fb1-b1ff-1d7b4b0c9212">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                      Common container, aggregated by all modules. It contains published information about vendor and versions.
                                  </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:cae3aaaa-d6cb-4f1f-b11c-33643b9adedc">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  Vendor specific:
                                  Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:a3c9a9e0-abe2-459a-bd8d-cd421ef7364a">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  Vendor specific:
                                  Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:61769362-1fa4-4387-a81d-e42bc83570da">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  Vendor specific:
                                  Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:af950081-c65d-495b-91fc-94efceb5e8b0">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  Vendor specific:
                                  Module ID of this module from Module List.
                                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>102</DEFAULT-VALUE>
                  <MAX>102</MAX>
                  <MIN>102</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e469a6f5-5339-42a2-a4a8-998c183e67f0">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  Vendor specific:
                                  Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:0a8ff8b2-6c8e-4d95-93bd-9f36383bcee9">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                Vendor specific:
                                Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:4e0ef25d-a4fa-44f2-ab98-82734b0e8963">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                Vendor specific:
                                Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:5ece58a0-4462-4945-8c00-b2bf44c35ed9">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  In driver modules which can be instantiated several times on a single ECU, BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name. 
                                  This parameter is used to specify the vendor specific name. In total, the implementation specific name is generated as follows:
                                  
                                  &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt; 
                                  E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 
                                  This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:9e986773-96f5-45f6-8456-21cfffe2638d">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                      Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>