<?xml version='1.0'?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00046.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE>
      <SHORT-NAME>Spi</SHORT-NAME>
      <ELEMENTS>
        <ECUC-MODULE-CONFIGURATION-VALUES>
          <SHORT-NAME>Spi</SHORT-NAME>
          <DEFINITION-REF DEST="ECUC-MODULE-DEF">/TS_T40D11M40I0R0/Spi</DEFINITION-REF>
          <IMPLEMENTATION-CONFIG-VARIANT>VARIANT-PRE-COMPILE</IMPLEMENTATION-CONFIG-VARIANT>
          <POST-BUILD-VARIANT-USED>true</POST-BUILD-VARIANT-USED>
          <CONTAINERS>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/ArReleaseMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/ArReleaseMinorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/ArReleaseRevisionVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/ModuleId</DEFINITION-REF>
                  <VALUE>83</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/SwMajorVersion</DEFINITION-REF>
                  <VALUE>4</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/SwMinorVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/SwPatchVersion</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/CommonPublishedInformation/VendorId</DEFINITION-REF>
                  <VALUE>43</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>SpiAutosarExt</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiAllowBigSizeCollections</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiDisableDemReportErrorStatus</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiEnableDmaFastTransferSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiEnableHWUnitAsyncMode</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiEnableUserModeSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiJobStartNotificationEnable</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <REFERENCE-VALUES>
                <ECUC-REFERENCE-VALUE>
                  <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiAutosarExt/SpiAlternateClockRef</DEFINITION-REF>
                  <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_0</VALUE-REF>
                </ECUC-REFERENCE-VALUE>
              </REFERENCE-VALUES>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>EthSwt_SpiDriver</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver</DEFINITION-REF>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiChannel_SJA1105Q</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelType</DEFINITION-REF>
                      <VALUE>EB</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiDataWidth</DEFINITION-REF>
                      <VALUE>16</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiEbMaxLength</DEFINITION-REF>
                      <VALUE>1000</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiIbNBuffers</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiTransferStart</DEFINITION-REF>
                      <VALUE>MSB</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelEcucPartitionRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiChannel_SJA1110a</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelType</DEFINITION-REF>
                      <VALUE>EB</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiDataWidth</DEFINITION-REF>
                      <VALUE>16</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiEbMaxLength</DEFINITION-REF>
                      <VALUE>1000</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiIbNBuffers</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiTransferStart</DEFINITION-REF>
                      <VALUE>MSB</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelEcucPartitionRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiChannel_SJA1110b</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelId</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelType</DEFINITION-REF>
                      <VALUE>EB</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiDataWidth</DEFINITION-REF>
                      <VALUE>16</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiEbMaxLength</DEFINITION-REF>
                      <VALUE>1000</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiIbNBuffers</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiTransferStart</DEFINITION-REF>
                      <VALUE>MSB</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiChannel/SpiChannelEcucPartitionRef</DEFINITION-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiExternalDevice_SJA1105Q</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiBaudrate</DEFINITION-REF>
                      <VALUE>5000000.0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsContinous</DEFINITION-REF>
                      <VALUE>TRUE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsIdentifier</DEFINITION-REF>
                      <VALUE>PCS0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsPolarity</DEFINITION-REF>
                      <VALUE>LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsSelection</DEFINITION-REF>
                      <VALUE>CS_VIA_PERIPHERAL_ENGINE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiDataShiftEdge</DEFINITION-REF>
                      <VALUE>LEADING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiEnableCs</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiHwUnit</DEFINITION-REF>
                      <VALUE>CSIB0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiShiftClockIdleLevel</DEFINITION-REF>
                      <VALUE>LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeClk2Cs</DEFINITION-REF>
                      <VALUE>2.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeCs2Clk</DEFINITION-REF>
                      <VALUE>2.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeCs2Cs</DEFINITION-REF>
                      <VALUE>4.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiExternalDevice_SJA1110a</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiBaudrate</DEFINITION-REF>
                      <VALUE>5000000.0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsContinous</DEFINITION-REF>
                      <VALUE>TRUE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsIdentifier</DEFINITION-REF>
                      <VALUE>PCS0</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsPolarity</DEFINITION-REF>
                      <VALUE>LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsSelection</DEFINITION-REF>
                      <VALUE>CS_VIA_PERIPHERAL_ENGINE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiDataShiftEdge</DEFINITION-REF>
                      <VALUE>TRAILING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiEnableCs</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiHwUnit</DEFINITION-REF>
                      <VALUE>CSIB1</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiShiftClockIdleLevel</DEFINITION-REF>
                      <VALUE>LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeClk2Cs</DEFINITION-REF>
                      <VALUE>2.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeCs2Clk</DEFINITION-REF>
                      <VALUE>2.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeCs2Cs</DEFINITION-REF>
                      <VALUE>4.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiExternalDevice_SJA1110b</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiBaudrate</DEFINITION-REF>
                      <VALUE>5000000.0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsContinous</DEFINITION-REF>
                      <VALUE>TRUE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-STRING-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsIdentifier</DEFINITION-REF>
                      <VALUE>PCS1</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsPolarity</DEFINITION-REF>
                      <VALUE>LOW</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiCsSelection</DEFINITION-REF>
                      <VALUE>CS_VIA_PERIPHERAL_ENGINE</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiDataShiftEdge</DEFINITION-REF>
                      <VALUE>TRAILING</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiEnableCs</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiHwUnit</DEFINITION-REF>
                      <VALUE>CSIB1</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiShiftClockIdleLevel</DEFINITION-REF>
                      <VALUE>HIGH</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeClk2Cs</DEFINITION-REF>
                      <VALUE>2.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeCs2Clk</DEFINITION-REF>
                      <VALUE>2.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-FLOAT-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiExternalDevice/SpiTimeCs2Cs</DEFINITION-REF>
                      <VALUE>4.0E-7</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiJob_SJA1105Q</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiJobId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiJobPriority</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiDeviceAssignment</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiExternalDevice_SJA1105Q</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>SpiChannelList_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList/SpiChannelIndex</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList/SpiChannelAssignment</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiChannel_SJA1105Q</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiJob_SJA1110a</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiJobId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiJobPriority</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiDeviceAssignment</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiExternalDevice_SJA1110a</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>SpiChannelList_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList/SpiChannelIndex</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList/SpiChannelAssignment</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiChannel_SJA1110a</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiJob_SJA1110b</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiJobId</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiJobPriority</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiDeviceAssignment</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiExternalDevice_SJA1110b</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                  <SUB-CONTAINERS>
                    <ECUC-CONTAINER-VALUE>
                      <SHORT-NAME>SpiChannelList_0</SHORT-NAME>
                      <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList</DEFINITION-REF>
                      <PARAMETER-VALUES>
                        <ECUC-NUMERICAL-PARAM-VALUE>
                          <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList/SpiChannelIndex</DEFINITION-REF>
                          <VALUE>0</VALUE>
                        </ECUC-NUMERICAL-PARAM-VALUE>
                      </PARAMETER-VALUES>
                      <REFERENCE-VALUES>
                        <ECUC-REFERENCE-VALUE>
                          <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiJob/SpiChannelList/SpiChannelAssignment</DEFINITION-REF>
                          <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiChannel_SJA1110b</VALUE-REF>
                        </ECUC-REFERENCE-VALUE>
                      </REFERENCE-VALUES>
                    </ECUC-CONTAINER-VALUE>
                  </SUB-CONTAINERS>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiEthSwtSJA1105QSequence</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiEnableDmaFastTransfer</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiInterruptibleSequence</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiSequenceId</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiJobAssignment</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiJob_SJA1105Q</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiSequence_SJA1110a</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiEnableDmaFastTransfer</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiInterruptibleSequence</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiSequenceId</DEFINITION-REF>
                      <VALUE>1</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiJobAssignment</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiJob_SJA1110a</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiSequence_SJA1110b</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiEnableDmaFastTransfer</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiInterruptibleSequence</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiSequenceId</DEFINITION-REF>
                      <VALUE>2</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                  <REFERENCE-VALUES>
                    <ECUC-REFERENCE-VALUE>
                      <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiDriver/SpiSequence/SpiJobAssignment</DEFINITION-REF>
                      <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Spi/Spi/EthSwt_SpiDriver/SpiJob_SJA1110b</VALUE-REF>
                    </ECUC-REFERENCE-VALUE>
                  </REFERENCE-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>SpiGeneral</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiCancelApi</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiChannelBuffersAllowed</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiDevErrorDetect</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiGlobalDmaEnable</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiHwStatusApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiInterruptibleSeqAllowed</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiLevelDelivered</DEFINITION-REF>
                  <VALUE>2</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiMulticoreSupport</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiSupportConcurrentSyncTransmit</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-TEXTUAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiTimeoutMethod</DEFINITION-REF>
                  <VALUE>OSIF_COUNTER_DUMMY</VALUE>
                </ECUC-TEXTUAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiTransmitTimeout</DEFINITION-REF>
                  <VALUE>50000</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiVersionInfoApi</DEFINITION-REF>
                  <VALUE>1</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
              <REFERENCE-VALUES>
                <ECUC-REFERENCE-VALUE>
                  <DEFINITION-REF DEST="ECUC-REFERENCE-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiClockRef</DEFINITION-REF>
                  <VALUE-REF DEST="ECUC-CONTAINER-VALUE">/Mcu/Mcu/McuModuleConfiguration/McuClockSettingConfig_0/McuClockReferencePoint_1</VALUE-REF>
                </ECUC-REFERENCE-VALUE>
              </REFERENCE-VALUES>
              <SUB-CONTAINERS>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiPhyUnit_0</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiModifiedTransferFormatEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitAsyncUseDma</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitMapping</DEFINITION-REF>
                      <VALUE>SPI_5</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitMode</DEFINITION-REF>
                      <VALUE>SPI_MASTER</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitSync</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiSamplePoint</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
                <ECUC-CONTAINER-VALUE>
                  <SHORT-NAME>SpiPhyUnit_1</SHORT-NAME>
                  <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit</DEFINITION-REF>
                  <PARAMETER-VALUES>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiModifiedTransferFormatEnable</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitAsyncUseDma</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitMapping</DEFINITION-REF>
                      <VALUE>SPI_4</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-TEXTUAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-ENUMERATION-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitMode</DEFINITION-REF>
                      <VALUE>SPI_MASTER</VALUE>
                    </ECUC-TEXTUAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-BOOLEAN-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiPhyUnitSync</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                    <ECUC-NUMERICAL-PARAM-VALUE>
                      <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiGeneral/SpiPhyUnit/SpiSamplePoint</DEFINITION-REF>
                      <VALUE>0</VALUE>
                    </ECUC-NUMERICAL-PARAM-VALUE>
                  </PARAMETER-VALUES>
                </ECUC-CONTAINER-VALUE>
              </SUB-CONTAINERS>
            </ECUC-CONTAINER-VALUE>
            <ECUC-CONTAINER-VALUE>
              <SHORT-NAME>SpiPublishedInformation</SHORT-NAME>
              <DEFINITION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/TS_T40D11M40I0R0/Spi/SpiPublishedInformation</DEFINITION-REF>
              <PARAMETER-VALUES>
                <ECUC-NUMERICAL-PARAM-VALUE>
                  <DEFINITION-REF DEST="ECUC-INTEGER-PARAM-DEF">/TS_T40D11M40I0R0/Spi/SpiPublishedInformation/SpiMaxHwUnit</DEFINITION-REF>
                  <VALUE>0</VALUE>
                </ECUC-NUMERICAL-PARAM-VALUE>
              </PARAMETER-VALUES>
            </ECUC-CONTAINER-VALUE>
          </CONTAINERS>
        </ECUC-MODULE-CONFIGURATION-VALUES>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>
