# Introduction
The main function of temperature_dvfs example is to guide user to implement DVFS on i.MX RT1170 platform.
In the demo GPT and display are optional mudules. The key content is temperature sensor interrupt handler.
Because there are relatively few voltages and clocks that need to be adjusted, only the software configuration of clocks and voltages is currently enabled. We can consider applying setpoint configuration later.

# Hardware Illustration
No reworks to be done.

# How to setup the demo
The demo can run in IAR when flexspi_nor_debug is selected as configuration. 
It can also compiled by build_debug.sh or build_flexspi_nor_debug.sh in armgcc.
# Software Architecture

![software configuration](doc/tempsensor_dvfs.PNG)

