Callisto4Bootloader: arm_biquad_cascade_stereo_df2T_instance_f32 Struct Reference

Callisto4Bootloader

Data Fields
arm_biquad_cascade_stereo_df2T_instance_f32 Struct Reference

Instance structure for the floating-point transposed direct form II Biquad cascade filter. More...

`#include <arm_math.h>`

## Data Fields

uint8_t | numStages
float32_t * | pState
const float32_t * | pCoeffs

## Detailed Description

Instance structure for the floating-point transposed direct form II Biquad cascade filter.

Definition at line 3640 of file arm_math.h.

## Field Documentation

## ◆ numStages

uint8_t arm_biquad_cascade_stereo_df2T_instance_f32::numStages

number of 2nd order stages in the filter. Overall order is 2*numStages.

Definition at line 3642 of file arm_math.h.

## ◆ pCoeffs

const float32_t* arm_biquad_cascade_stereo_df2T_instance_f32::pCoeffs

points to the array of coefficients. The array is of length 5*numStages.

Definition at line 3644 of file arm_math.h.

## ◆ pState

float32_t* arm_biquad_cascade_stereo_df2T_instance_f32::pState

points to the array of state coefficients. The array is of length 4*numStages.

Definition at line 3643 of file arm_math.h.

The documentation for this struct was generated from the following file:

- CMSIS/arm_math.h