Callisto4Bootloader: ADC_ETC_Type Struct Reference

Callisto4Bootloader

Data Fields
ADC_ETC_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » ADC_ETC Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | CTRL
__IO uint32_t | DONE0_1_IRQ
__IO uint32_t | DONE2_ERR_IRQ
__IO uint32_t | DMA_CTRL
struct {
__IO uint32_t ADC_ETC_Type::TRIGn_CTRL
__IO uint32_t ADC_ETC_Type::TRIGn_COUNTER
__IO uint32_t ADC_ETC_Type::TRIGn_CHAIN_1_0
__IO uint32_t ADC_ETC_Type::TRIGn_CHAIN_3_2
__IO uint32_t ADC_ETC_Type::TRIGn_CHAIN_5_4
__IO uint32_t ADC_ETC_Type::TRIGn_CHAIN_7_6
__I uint32_t ADC_ETC_Type::TRIGn_RESULT_1_0
__I uint32_t ADC_ETC_Type::TRIGn_RESULT_3_2
__I uint32_t ADC_ETC_Type::TRIGn_RESULT_5_4
__I uint32_t ADC_ETC_Type::TRIGn_RESULT_7_6
} | TRIG [8]

## Detailed Description

ADC_ETC - Register Layout Typedef

Definition at line 1743 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h