Callisto4Bootloader: SRC Peripheral Access Layer

Callisto4Bootloader

Modules | Data Structures | Macros
SRC Peripheral Access Layer
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer

## Modules

| SRC Register Masks

## Data Structures

struct | SRC_Type

## Macros

#define | SRC_BASE (0x400F8000u)
#define | SRC ((SRC_Type *)SRC_BASE)
#define | SRC_BASE_ADDRS { SRC_BASE }
#define | SRC_BASE_PTRS { SRC }
#define | SRC_IRQS { SRC_IRQn }
#define | SRC_SCR_MWDR_MASK SRC_SCR_MASK_WDOG_RST_MASK
#define | SRC_SCR_MWDR_SHIFT SRC_SCR_MASK_WDOG_RST_SHIFT
#define | SRC_SCR_MWDR(x) SRC_SCR_MASK_WDOG_RST(x)
#define | SRC_SRSR_WDOG_MASK SRC_SRSR_WDOG_RST_B_MASK
#define | SRC_SRSR_WDOG_SHIFT SRC_SRSR_WDOG_RST_B_SHIFT
#define | SRC_SRSR_WDOG(x) SRC_SRSR_WDOG_RST_B(x)
#define | SRC_SRSR_JTAG_MASK SRC_SRSR_JTAG_RST_B_MASK
#define | SRC_SRSR_JTAG_SHIFT SRC_SRSR_JTAG_RST_B_SHIFT
#define | SRC_SRSR_JTAG(x) SRC_SRSR_JTAG_RST_B(x)
#define | SRC_SRSR_SJC_MASK SRC_SRSR_JTAG_SW_RST_MASK
#define | SRC_SRSR_SJC_SHIFT SRC_SRSR_JTAG_SW_RST_SHIFT
#define | SRC_SRSR_SJC(x) SRC_SRSR_JTAG_SW_RST(x)
#define | SRC_SRSR_TSR_MASK SRC_SRSR_TEMPSENSE_RST_B_MASK
#define | SRC_SRSR_TSR_SHIFT SRC_SRSR_TEMPSENSE_RST_B_SHIFT
#define | SRC_SRSR_TSR(x) SRC_SRSR_TEMPSENSE_RST_B(x)
#define | SRC_SRSR_W1C_BITS_MASK

## Detailed Description

## Macro Definition Documentation

## ◆ SRC

#define SRC ((SRC_Type *)SRC_BASE)

Peripheral SRC base pointer

Definition at line 39465 of file MIMXRT1062.h.

## ◆ SRC_BASE

#define SRC_BASE (0x400F8000u)

Peripheral SRC base address

Definition at line 39463 of file MIMXRT1062.h.

## ◆ SRC_BASE_ADDRS

#define SRC_BASE_ADDRS { SRC_BASE }

Array initializer of SRC peripheral base addresses

Definition at line 39467 of file MIMXRT1062.h.

## ◆ SRC_BASE_PTRS

#define SRC_BASE_PTRS { SRC }

Array initializer of SRC peripheral base pointers

Definition at line 39469 of file MIMXRT1062.h.

## ◆ SRC_IRQS

#define SRC_IRQS { SRC_IRQn }

Interrupt vectors for the SRC peripheral type

Definition at line 39471 of file MIMXRT1062.h.

## ◆ SRC_SCR_MWDR

#define SRC_SCR_MWDR | ( |  | x | ) | SRC_SCR_MASK_WDOG_RST(x)

Definition at line 39475 of file MIMXRT1062.h.

## ◆ SRC_SCR_MWDR_MASK

#define SRC_SCR_MWDR_MASK SRC_SCR_MASK_WDOG_RST_MASK

Definition at line 39473 of file MIMXRT1062.h.

## ◆ SRC_SCR_MWDR_SHIFT

#define SRC_SCR_MWDR_SHIFT SRC_SCR_MASK_WDOG_RST_SHIFT

Definition at line 39474 of file MIMXRT1062.h.

## ◆ SRC_SRSR_JTAG

#define SRC_SRSR_JTAG | ( |  | x | ) | SRC_SRSR_JTAG_RST_B(x)

Definition at line 39481 of file MIMXRT1062.h.

## ◆ SRC_SRSR_JTAG_MASK

#define SRC_SRSR_JTAG_MASK SRC_SRSR_JTAG_RST_B_MASK

Definition at line 39479 of file MIMXRT1062.h.

## ◆ SRC_SRSR_JTAG_SHIFT

#define SRC_SRSR_JTAG_SHIFT SRC_SRSR_JTAG_RST_B_SHIFT

Definition at line 39480 of file MIMXRT1062.h.

## ◆ SRC_SRSR_SJC

#define SRC_SRSR_SJC | ( |  | x | ) | SRC_SRSR_JTAG_SW_RST(x)

Definition at line 39484 of file MIMXRT1062.h.

## ◆ SRC_SRSR_SJC_MASK

#define SRC_SRSR_SJC_MASK SRC_SRSR_JTAG_SW_RST_MASK

Definition at line 39482 of file MIMXRT1062.h.

## ◆ SRC_SRSR_SJC_SHIFT

#define SRC_SRSR_SJC_SHIFT SRC_SRSR_JTAG_SW_RST_SHIFT

Definition at line 39483 of file MIMXRT1062.h.

## ◆ SRC_SRSR_TSR

#define SRC_SRSR_TSR | ( |  | x | ) | SRC_SRSR_TEMPSENSE_RST_B(x)

Definition at line 39487 of file MIMXRT1062.h.

## ◆ SRC_SRSR_TSR_MASK

#define SRC_SRSR_TSR_MASK SRC_SRSR_TEMPSENSE_RST_B_MASK

Definition at line 39485 of file MIMXRT1062.h.

## ◆ SRC_SRSR_TSR_SHIFT

#define SRC_SRSR_TSR_SHIFT SRC_SRSR_TEMPSENSE_RST_B_SHIFT

Definition at line 39486 of file MIMXRT1062.h.

## ◆ SRC_SRSR_W1C_BITS_MASK

#define SRC_SRSR_W1C_BITS_MASK

Value:
( SRC_SRSR_WDOG3_RST_B_MASK \
| SRC_SRSR_JTAG_SW_RST_MASK \
| SRC_SRSR_JTAG_RST_B_MASK \
| SRC_SRSR_WDOG_RST_B_MASK \
| SRC_SRSR_IPP_USER_RESET_B_MASK \
| SRC_SRSR_CSU_RESET_B_MASK \
| SRC_SRSR_LOCKUP_SYSRESETREQ_MASK \
| SRC_SRSR_IPP_RESET_B_MASK)

Definition at line 39489 of file MIMXRT1062.h.

## ◆ SRC_SRSR_WDOG

#define SRC_SRSR_WDOG | ( |  | x | ) | SRC_SRSR_WDOG_RST_B(x)

Definition at line 39478 of file MIMXRT1062.h.

## ◆ SRC_SRSR_WDOG_MASK

#define SRC_SRSR_WDOG_MASK SRC_SRSR_WDOG_RST_B_MASK

Definition at line 39476 of file MIMXRT1062.h.

## ◆ SRC_SRSR_WDOG_SHIFT

#define SRC_SRSR_WDOG_SHIFT SRC_SRSR_WDOG_RST_B_SHIFT

Definition at line 39477 of file MIMXRT1062.h.

SRC_SRSR_IPP_RESET_B_MASK
#define SRC_SRSR_IPP_RESET_B_MASK
Definition: MIMXRT1062.h:39361
SRC_SRSR_WDOG3_RST_B_MASK
#define SRC_SRSR_WDOG3_RST_B_MASK
Definition: MIMXRT1062.h:39410
SRC_SRSR_WDOG_RST_B_MASK
#define SRC_SRSR_WDOG_RST_B_MASK
Definition: MIMXRT1062.h:39389
SRC_SRSR_JTAG_RST_B_MASK
#define SRC_SRSR_JTAG_RST_B_MASK
Definition: MIMXRT1062.h:39396
SRC_SRSR_CSU_RESET_B_MASK
#define SRC_SRSR_CSU_RESET_B_MASK
Definition: MIMXRT1062.h:39375
SRC_SRSR_IPP_USER_RESET_B_MASK
#define SRC_SRSR_IPP_USER_RESET_B_MASK
Definition: MIMXRT1062.h:39382
SRC_SRSR_LOCKUP_SYSRESETREQ_MASK
#define SRC_SRSR_LOCKUP_SYSRESETREQ_MASK
Definition: MIMXRT1062.h:39368
SRC_SRSR_JTAG_SW_RST_MASK
#define SRC_SRSR_JTAG_SW_RST_MASK
Definition: MIMXRT1062.h:39403