Callisto4Bootloader: CONTROL_Type Union Reference

Callisto4Bootloader

Data Fields
CONTROL_Type Union Reference
Defines and Type Definitions » Status and Control Registers

Union type to access the Control Registers (CONTROL). More...

`#include <core_armv81mml.h>`

## Data Fields

struct {
uint32_t CONTROL_Type::nPRIV:1
uint32_t CONTROL_Type::SPSEL:1
uint32_t CONTROL_Type::FPCA:1
uint32_t CONTROL_Type::SFPA:1
uint32_t CONTROL_Type::_reserved1:28
} | b
uint32_t | w
struct {
uint32_t CONTROL_Type::nPRIV:1
uint32_t CONTROL_Type::SPSEL:1
uint32_t CONTROL_Type::_reserved1:30
} | b
struct {
uint32_t CONTROL_Type::nPRIV:1
uint32_t CONTROL_Type::SPSEL:1
uint32_t CONTROL_Type::FPCA:1
uint32_t CONTROL_Type::SFPA:1
uint32_t CONTROL_Type::_reserved1:28
} | b
struct {
uint32_t CONTROL_Type::nPRIV:1
uint32_t CONTROL_Type::SPSEL:1
uint32_t CONTROL_Type::FPCA:1
uint32_t CONTROL_Type::_reserved0:29
} | b

## Detailed Description

Union type to access the Control Registers (CONTROL).

Definition at line 422 of file core_armv81mml.h.

The documentation for this union was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h