Callisto4Bootloader: Data Structures

Callisto4Bootloader

Data Structures
Here are the data structures with brief descriptions:
[detail level 12]

C__iar_u32 |
C_flexspi_nor_config |
C_FlexSPIConfig | FlexSPI Memory Configuration Block
C_FlexSpiXfer | FlexSPI Transfer Context
C_lut_sequence | FlexSPI LUT Sequence structure
C_rtwdog_config | Describes RTWDOG configuration structure
C_rtwdog_work_mode | Defines RTWDOG work mode
C_serial_nor_config_option |
C_wdog_config | Describes WDOG configuration structure
C_wdog_work_mode | Defines WDOG work mode
C ADC_ETC_Type |
C ADC_Type |
C AIPSTZ_Type |
C AOI_Type |
C APSR_Type | Union type to access the Application Program Status Register (APSR)
C arm_bilinear_interp_instance_f32 | Instance structure for the floating-point bilinear interpolation function
C arm_bilinear_interp_instance_q15 | Instance structure for the Q15 bilinear interpolation function
C arm_bilinear_interp_instance_q31 | Instance structure for the Q31 bilinear interpolation function
C arm_bilinear_interp_instance_q7 | Instance structure for the Q15 bilinear interpolation function
C arm_biquad_cas_df1_32x64_ins_q31 | Instance structure for the high precision Q31 Biquad cascade filter
C arm_biquad_cascade_df2T_instance_f32 | Instance structure for the floating-point transposed direct form II Biquad cascade filter
C arm_biquad_cascade_df2T_instance_f64 | Instance structure for the floating-point transposed direct form II Biquad cascade filter
C arm_biquad_cascade_stereo_df2T_instance_f32 | Instance structure for the floating-point transposed direct form II Biquad cascade filter
C arm_biquad_casd_df1_inst_f32 | Instance structure for the floating-point Biquad cascade filter
C arm_biquad_casd_df1_inst_q15 | Instance structure for the Q15 Biquad cascade filter
C arm_biquad_casd_df1_inst_q31 | Instance structure for the Q31 Biquad cascade filter
C arm_cfft_instance_f32 | Instance structure for the floating-point CFFT/CIFFT function
C arm_cfft_instance_q15 | Instance structure for the fixed-point CFFT/CIFFT function
C arm_cfft_instance_q31 | Instance structure for the fixed-point CFFT/CIFFT function
C arm_cfft_radix2_instance_f32 | Instance structure for the floating-point CFFT/CIFFT function
C arm_cfft_radix2_instance_q15 | Instance structure for the Q15 CFFT/CIFFT function
C arm_cfft_radix2_instance_q31 | Instance structure for the Radix-2 Q31 CFFT/CIFFT function
C arm_cfft_radix4_instance_f32 | Instance structure for the floating-point CFFT/CIFFT function
C arm_cfft_radix4_instance_q15 | Instance structure for the Q15 CFFT/CIFFT function
C arm_cfft_radix4_instance_q31 | Instance structure for the Q31 CFFT/CIFFT function
C arm_dct4_instance_f32 | Instance structure for the floating-point DCT4/IDCT4 function
C arm_dct4_instance_q15 | Instance structure for the Q15 DCT4/IDCT4 function
C arm_dct4_instance_q31 | Instance structure for the Q31 DCT4/IDCT4 function
C arm_fir_decimate_instance_f32 | Instance structure for floating-point FIR decimator
C arm_fir_decimate_instance_q15 | Instance structure for the Q15 FIR decimator
C arm_fir_decimate_instance_q31 | Instance structure for the Q31 FIR decimator
C arm_fir_instance_f32 | Instance structure for the floating-point FIR filter
C arm_fir_instance_q15 | Instance structure for the Q15 FIR filter
C arm_fir_instance_q31 | Instance structure for the Q31 FIR filter
C arm_fir_instance_q7 | Instance structure for the Q7 FIR filter
C arm_fir_interpolate_instance_f32 | Instance structure for the floating-point FIR interpolator
C arm_fir_interpolate_instance_q15 | Instance structure for the Q15 FIR interpolator
C arm_fir_interpolate_instance_q31 | Instance structure for the Q31 FIR interpolator
C arm_fir_lattice_instance_f32 | Instance structure for the floating-point FIR lattice filter
C arm_fir_lattice_instance_q15 | Instance structure for the Q15 FIR lattice filter
C arm_fir_lattice_instance_q31 | Instance structure for the Q31 FIR lattice filter
C arm_fir_sparse_instance_f32 | Instance structure for the floating-point sparse FIR filter
C arm_fir_sparse_instance_q15 | Instance structure for the Q15 sparse FIR filter
C arm_fir_sparse_instance_q31 | Instance structure for the Q31 sparse FIR filter
C arm_fir_sparse_instance_q7 | Instance structure for the Q7 sparse FIR filter
C arm_iir_lattice_instance_f32 | Instance structure for the floating-point IIR lattice filter
C arm_iir_lattice_instance_q15 | Instance structure for the Q15 IIR lattice filter
C arm_iir_lattice_instance_q31 | Instance structure for the Q31 IIR lattice filter
C arm_linear_interp_instance_f32 | Instance structure for the floating-point Linear Interpolate function
C arm_lms_instance_f32 | Instance structure for the floating-point LMS filter
C arm_lms_instance_q15 | Instance structure for the Q15 LMS filter
C arm_lms_instance_q31 | Instance structure for the Q31 LMS filter
C arm_lms_norm_instance_f32 | Instance structure for the floating-point normalized LMS filter
C arm_lms_norm_instance_q15 | Instance structure for the Q15 normalized LMS filter
C arm_lms_norm_instance_q31 | Instance structure for the Q31 normalized LMS filter
C arm_matrix_instance_f32 | Instance structure for the floating-point matrix structure
C arm_matrix_instance_f64 | Instance structure for the floating-point matrix structure
C arm_matrix_instance_q15 | Instance structure for the Q15 matrix structure
C arm_matrix_instance_q31 | Instance structure for the Q31 matrix structure
C ARM_MPU_Region_t |
C arm_pid_instance_f32 | Instance structure for the floating-point PID Control
C arm_pid_instance_q15 | Instance structure for the Q15 PID Control
C arm_pid_instance_q31 | Instance structure for the Q31 PID Control
C arm_rfft_fast_instance_f32 | Instance structure for the floating-point RFFT/RIFFT function
C arm_rfft_instance_f32 | Instance structure for the floating-point RFFT/RIFFT function
C arm_rfft_instance_q15 | Instance structure for the Q15 RFFT/RIFFT function
C arm_rfft_instance_q31 | Instance structure for the Q31 RFFT/RIFFT function
C BEE_Type |
C bootloader_api_entry_t |
C BPT_t |
C c4_SRC_reg_t | System Reset Controller (SRC)
►C c4_WDOG_reg_t | Structure to overlay on the watchdog registers
C c4_WDOG_wicr | Watchdog Interrupt Control
C CAN_Type |
C CCM_ANALOG_Type |
C CCM_Type |
C clock_driver_interface_t |
C CMP_Type |
C CONTROL_Type | Union type to access the Control Registers (CONTROL)
C CoreDebug_Type | Structure type to access the Core Debug Register (CoreDebug)
C CPUID_t | Structure for CPU ID base register in System Control Block (SCB)
C CSI_Type |
C CSU_Type |
C DCD_t | Device Configuration Data (DCD)
C DCDC_Type |
C DCP_Type |
C DMA_Type |
C DMAMUX_Type |
C DWT_Type | Structure type to access the Data Watchpoint and Trace Register (DWT)
C ENC_Type |
C ENET_Type |
C EWM_Type |
C flash_run_context_t |
C FLEXIO_Type |
C FLEXRAM_Type |
C flexspi_dll_time_t |
C FlexSPI_Header_t | FlexSPI Configuration Block
C flexspi_nor_driver_interface_t |
C FLEXSPI_Type |
C FPU_Type | Structure type to access the Floating Point Unit (FPU)
C GPC_Type |
C GPIO_Type |
C GPT_Type |
C I2S_Type |
C IOMUXC_GPR_Type |
C IOMUXC_SNVS_GPR_Type |
C IOMUXC_SNVS_Type |
C IOMUXC_Type |
C IPSR_Type | Union type to access the Interrupt Program Status Register (IPSR)
C ITM_Type | Structure type to access the Instrumentation Trace Macrocell Register (ITM)
C IVT_t | Structure to overlay on Image Vector Table
C KPP_Type |
C LCDIF_Type |
C LPI2C_Type |
C LPSPI_Type |
C LPUART_Type |
C NVIC_Type | Structure type to access the Nested Vectored Interrupt Controller (NVIC)
C OCOTP_Type |
C PGC_Type |
C PIT_Type |
C PMU_Type |
C PWM_Type |
C PXP_Type |
C ROMC_Type |
C rtwdog_driver_interface_t |
C RTWDOG_Type |
C run_bootloader_ctx_t |
C SCB_Type | Structure type to access the System Control Block (SCB)
C SCnSCB_Type | Structure type to access the System Control and ID Register not in the SCB
C SEMC_Type |
C serialNOR_t | Serial NOR configuration block Contains FlexSPIheader common block and NOR specific configuration
C SNVS_Type |
C SPDIF_Type |
C SRC_Type |
C StandardVersion | Structure of version property
C SysTick_Type | Structure type to access the System Timer (SysTick)
C TEMPMON_Type |
C TMR_Type |
C TPI_Type | Structure type to access the Trace Port Interface Register (TPI)
C TRNG_Type |
C TSC_Type |
C USB_ANALOG_Type |
C USB_Type |
C USBNC_Type |
C USBPHY_Type |
C USDHC_Type |
C wdog_driver_interface_t |
C WDOG_Type |
C XBARA_Type |
C XBARB_Type |
C xPSR_Type | Union type to access the Special-Purpose Program Status Registers (xPSR)
C XTALOSC24M_Type |