Callisto4Bootloader: IPSR_Type Union Reference

Callisto4Bootloader

Data Fields
IPSR_Type Union Reference
Defines and Type Definitions » Status and Control Registers

Union type to access the Interrupt Program Status Register (IPSR). More...

`#include <core_armv81mml.h>`

## Data Fields

struct {
uint32_t IPSR_Type::ISR:9
uint32_t IPSR_Type::_reserved0:23
} | b
uint32_t | w
struct {
uint32_t IPSR_Type::ISR:9
uint32_t IPSR_Type::_reserved0:23
} | b
struct {
uint32_t IPSR_Type::ISR:9
uint32_t IPSR_Type::_reserved0:23
} | b
struct {
uint32_t IPSR_Type::ISR:9
uint32_t IPSR_Type::_reserved0:23
} | b

## Detailed Description

Union type to access the Interrupt Program Status Register (IPSR).

Definition at line 353 of file core_armv81mml.h.

The documentation for this union was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h