Callisto4Bootloader: board/clock_config.h Source File

Callisto4Bootloader

clock_config.h
Go to the documentation of this file.
1 #ifndef _CLOCK_CONFIG_H_
2 #define _CLOCK_CONFIG_H_
3
4 #include "fsl_common.h"
5
6 /*******************************************************************************
7 * Definitions
8 ******************************************************************************/
9 #define BOARD_XTAL0_CLK_HZ 24000000U
11 #define BOARD_XTAL32K_CLK_HZ 32768U
12 /*******************************************************************************
13 ************************ BOARD_InitBootClocks function ************************
14 ******************************************************************************/
15
16 #if defined(__cplusplus)
17 extern "C" {
18 #endif /* __cplusplus*/
19
24 void BOARD_InitBootClocks(void);
25
26 #if defined(__cplusplus)
27 }
28 #endif /* __cplusplus*/
29
30 /*******************************************************************************
31 ********************** Configuration BOARD_BootClockRUN ***********************
32 ******************************************************************************/
33 /*******************************************************************************
34 * Definitions for BOARD_BootClockRUN configuration
35 ******************************************************************************/
36 #define BOARD_BOOTCLOCKRUN_CORE_CLOCK 600000000U
38 /* Clock outputs (values are in Hz): */
39 #define BOARD_BOOTCLOCKRUN_AHB_CLK_ROOT 600000000UL
40 #define BOARD_BOOTCLOCKRUN_CAN_CLK_ROOT 40000000UL
41 #define BOARD_BOOTCLOCKRUN_CKIL_SYNC_CLK_ROOT 32768UL
42 #define BOARD_BOOTCLOCKRUN_CLKO1_CLK 0UL
43 #define BOARD_BOOTCLOCKRUN_CLKO2_CLK 0UL
44 #define BOARD_BOOTCLOCKRUN_CLK_1M 1000000UL
45 #define BOARD_BOOTCLOCKRUN_CLK_24M 24000000UL
46 #define BOARD_BOOTCLOCKRUN_CSI_CLK_ROOT 12000000UL
47 #define BOARD_BOOTCLOCKRUN_ENET1_TX_CLK 2400000UL
48 #define BOARD_BOOTCLOCKRUN_ENET2_125M_CLK 1200000UL
49 #define BOARD_BOOTCLOCKRUN_ENET2_TX_CLK 1200000UL
50 #define BOARD_BOOTCLOCKRUN_ENET_125M_CLK 2400000UL
51 #define BOARD_BOOTCLOCKRUN_ENET_25M_REF_CLK 1200000UL
52 #define BOARD_BOOTCLOCKRUN_FLEXIO1_CLK_ROOT 30000000UL
53 #define BOARD_BOOTCLOCKRUN_FLEXIO2_CLK_ROOT 30000000UL
54 #define BOARD_BOOTCLOCKRUN_FLEXSPI2_CLK_ROOT 130909090UL
55 #define BOARD_BOOTCLOCKRUN_FLEXSPI_CLK_ROOT 130909090UL
56 #define BOARD_BOOTCLOCKRUN_GPT1_IPG_CLK_HIGHFREQ 75000000UL
57 #define BOARD_BOOTCLOCKRUN_GPT2_IPG_CLK_HIGHFREQ 75000000UL
58 #define BOARD_BOOTCLOCKRUN_IPG_CLK_ROOT 150000000UL
59 #define BOARD_BOOTCLOCKRUN_LCDIF_CLK_ROOT 67500000UL
60 #define BOARD_BOOTCLOCKRUN_LPI2C_CLK_ROOT 60000000UL
61 #define BOARD_BOOTCLOCKRUN_LPSPI_CLK_ROOT 105600000UL
62 #define BOARD_BOOTCLOCKRUN_LVDS1_CLK 1200000000UL
63 #define BOARD_BOOTCLOCKRUN_MQS_MCLK 63529411UL
64 #define BOARD_BOOTCLOCKRUN_PERCLK_CLK_ROOT 75000000UL
65 #define BOARD_BOOTCLOCKRUN_PLL7_MAIN_CLK 24000000UL
66 #define BOARD_BOOTCLOCKRUN_SAI1_CLK_ROOT 63529411UL
67 #define BOARD_BOOTCLOCKRUN_SAI1_MCLK1 63529411UL
68 #define BOARD_BOOTCLOCKRUN_SAI1_MCLK2 63529411UL
69 #define BOARD_BOOTCLOCKRUN_SAI1_MCLK3 30000000UL
70 #define BOARD_BOOTCLOCKRUN_SAI2_CLK_ROOT 63529411UL
71 #define BOARD_BOOTCLOCKRUN_SAI2_MCLK1 63529411UL
72 #define BOARD_BOOTCLOCKRUN_SAI2_MCLK2 0UL
73 #define BOARD_BOOTCLOCKRUN_SAI2_MCLK3 30000000UL
74 #define BOARD_BOOTCLOCKRUN_SAI3_CLK_ROOT 63529411UL
75 #define BOARD_BOOTCLOCKRUN_SAI3_MCLK1 63529411UL
76 #define BOARD_BOOTCLOCKRUN_SAI3_MCLK2 0UL
77 #define BOARD_BOOTCLOCKRUN_SAI3_MCLK3 30000000UL
78 #define BOARD_BOOTCLOCKRUN_SEMC_CLK_ROOT 75000000UL
79 #define BOARD_BOOTCLOCKRUN_SPDIF0_CLK_ROOT 30000000UL
80 #define BOARD_BOOTCLOCKRUN_SPDIF0_EXTCLK_OUT 0UL
81 #define BOARD_BOOTCLOCKRUN_TRACE_CLK_ROOT 117333333UL
82 #define BOARD_BOOTCLOCKRUN_UART_CLK_ROOT 80000000UL
83 #define BOARD_BOOTCLOCKRUN_USBPHY1_CLK 0UL
84 #define BOARD_BOOTCLOCKRUN_USBPHY2_CLK 0UL
85 #define BOARD_BOOTCLOCKRUN_USDHC1_CLK_ROOT 198000000UL
86 #define BOARD_BOOTCLOCKRUN_USDHC2_CLK_ROOT 198000000UL
87
90 extern const clock_arm_pll_config_t armPllConfig_BOARD_BootClockRUN;
93 extern const clock_usb_pll_config_t usb1PllConfig_BOARD_BootClockRUN;
96 extern const clock_sys_pll_config_t sysPllConfig_BOARD_BootClockRUN;
99 extern const clock_video_pll_config_t videoPllConfig_BOARD_BootClockRUN;
100
101 /*******************************************************************************
102 * API for BOARD_BootClockRUN configuration
103 ******************************************************************************/
104 #if defined(__cplusplus)
105 extern "C" {
106 #endif /* __cplusplus*/
107
112 void BOARD_BootClockRUN(void);
113
114 #if defined(__cplusplus)
115 }
116 #endif /* __cplusplus*/
117
118 #endif /* _CLOCK_CONFIG_H_ */
119
sysPllConfig_BOARD_BootClockRUN
const clock_sys_pll_config_t sysPllConfig_BOARD_BootClockRUN
Sys PLL for BOARD_BootClockRUN configuration.
Definition: clock_config.c:142
BOARD_InitBootClocks
void BOARD_InitBootClocks(void)
This function executes default configuration of clocks.
Definition: clock_config.c:39
videoPllConfig_BOARD_BootClockRUN
const clock_video_pll_config_t videoPllConfig_BOARD_BootClockRUN
Video PLL set for BOARD_BootClockRUN configuration.
Definition: clock_config.c:154
usb1PllConfig_BOARD_BootClockRUN
const clock_usb_pll_config_t usb1PllConfig_BOARD_BootClockRUN
Usb1 PLL set for BOARD_BootClockRUN configuration.
Definition: clock_config.c:149
armPllConfig_BOARD_BootClockRUN
const clock_arm_pll_config_t armPllConfig_BOARD_BootClockRUN
Arm PLL set for BOARD_BootClockRUN configuration.
Definition: clock_config.c:137
BOARD_BootClockRUN
void BOARD_BootClockRUN(void)
This function executes configuration of clocks.
Definition: clock_config.c:164