Callisto4Bootloader: NVIC_Type Struct Reference

Callisto4Bootloader

Data Fields
NVIC_Type Struct Reference
Defines and Type Definitions » Status and Control Registers » Nested Vectored Interrupt Controller (NVIC)

Structure type to access the Nested Vectored Interrupt Controller (NVIC). More...

`#include <core_armv81mml.h>`

## Data Fields

__IOM uint32_t | ISER [16U]
uint32_t | RESERVED0 [16U]
__IOM uint32_t | ICER [16U]
uint32_t | RSERVED1 [16U]
__IOM uint32_t | ISPR [16U]
uint32_t | RESERVED2 [16U]
__IOM uint32_t | ICPR [16U]
uint32_t | RESERVED3 [16U]
__IOM uint32_t | IABR [16U]
uint32_t | RESERVED4 [16U]
__IOM uint32_t | ITNS [16U]
uint32_t | RESERVED5 [16U]
__IOM uint8_t | IPR [496U]
uint32_t | RESERVED6 [580U]
__OM uint32_t | STIR
__IOM uint32_t | IPR [124U]
uint32_t | RESERVED1 [24U]
__IOM uint8_t | IP [240U]

## Detailed Description

Structure type to access the Nested Vectored Interrupt Controller (NVIC).

Definition at line 461 of file core_armv81mml.h.

The documentation for this struct was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h