Callisto4Bootloader: SCB_Type Struct Reference

Callisto4Bootloader

Data Fields
SCB_Type Struct Reference
Defines and Type Definitions » Status and Control Registers » Nested Vectored Interrupt Controller (NVIC) » System Control Block (SCB)

Structure type to access the System Control Block (SCB). More...

`#include <core_armv81mml.h>`

## Data Fields

__IM uint32_t | CPUID
__IOM uint32_t | ICSR
__IOM uint32_t | VTOR
__IOM uint32_t | AIRCR
__IOM uint32_t | SCR
__IOM uint32_t | CCR
__IOM uint8_t | SHPR [12U]
__IOM uint32_t | SHCSR
__IOM uint32_t | CFSR
__IOM uint32_t | HFSR
__IOM uint32_t | DFSR
__IOM uint32_t | MMFAR
__IOM uint32_t | BFAR
__IOM uint32_t | AFSR
__IM uint32_t | ID_PFR [2U]
__IM uint32_t | ID_DFR
__IM uint32_t | ID_ADR
__IM uint32_t | ID_MMFR [4U]
__IM uint32_t | ID_ISAR [6U]
__IM uint32_t | CLIDR
__IM uint32_t | CTR
__IM uint32_t | CCSIDR
__IOM uint32_t | CSSELR
__IOM uint32_t | CPACR
__IOM uint32_t | NSACR
uint32_t | RESERVED3 [92U]
__OM uint32_t | STIR
uint32_t | RESERVED4 [15U]
__IM uint32_t | MVFR0
__IM uint32_t | MVFR1
__IM uint32_t | MVFR2
uint32_t | RESERVED5 [1U]
__OM uint32_t | ICIALLU
uint32_t | RESERVED6 [1U]
__OM uint32_t | ICIMVAU
__OM uint32_t | DCIMVAC
__OM uint32_t | DCISW
__OM uint32_t | DCCMVAU
__OM uint32_t | DCCMVAC
__OM uint32_t | DCCSW
__OM uint32_t | DCCIMVAC
__OM uint32_t | DCCISW
uint32_t | RESERVED7 [6U]
__IOM uint32_t | ITCMCR
__IOM uint32_t | DTCMCR
__IOM uint32_t | AHBPCR
__IOM uint32_t | CACR
__IOM uint32_t | AHBSCR
uint32_t | RESERVED8 [1U]
__IOM uint32_t | ABFSR
uint32_t | RESERVED0
uint32_t | RESERVED1
__IOM uint32_t | SHPR [2U]
__IM uint32_t | ID_AFR
__IM uint32_t | ID_MFR [4U]

## Detailed Description

Structure type to access the System Control Block (SCB).

Definition at line 497 of file core_armv81mml.h.

The documentation for this struct was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h