Callisto4Bootloader: File List

Callisto4Bootloader

File List
Here is a list of all files with brief descriptions:
[detail level 12]

▼ board |
board.c |
board.h |
clock_config.c |
clock_config.h |
dcd.c |
dcd.h |
peripherals.c |
peripherals.h |
pin_mux.c |
pin_mux.h |
▼ CMSIS |
arm_common_tables.h |
arm_const_structs.h |
arm_math.h |
cmsis_armcc.h | CMSIS compiler ARMCC (Arm Compiler 5) header file
cmsis_armclang.h | CMSIS compiler armclang (Arm Compiler 6) header file
cmsis_armclang_ltm.h | CMSIS compiler armclang (Arm Compiler 6) header file
cmsis_compiler.h | CMSIS compiler generic header file
cmsis_gcc.h | CMSIS compiler GCC header file
cmsis_iccarm.h | CMSIS compiler ICCARM (IAR Compiler for Arm) header file
cmsis_version.h | CMSIS Core(M) Version definitions
core_armv81mml.h | CMSIS Armv8.1-M Mainline Core Peripheral Access Layer Header File
core_armv8mbl.h | CMSIS Armv8-M Baseline Core Peripheral Access Layer Header File
core_armv8mml.h | CMSIS Armv8-M Mainline Core Peripheral Access Layer Header File
core_cm7.h | CMSIS Cortex-M7 Core Peripheral Access Layer Header File
mpu_armv7.h |
mpu_armv8.h |
▼ device |
fsl_device_registers.h |
MIMXRT1062.h | CMSIS Peripheral Access Layer for MIMXRT1062
MIMXRT1062_features.h |
system_MIMXRT1062.c |
system_MIMXRT1062.h |
▼ drivers |
bootloader_common.h |
bootloader_config.h |
flexspi_nor_flash.h |
fsl_flexspi.c |
fsl_flexspi.h |
fsl_rtwdog.h |
fsl_wdog.c |
fsl_wdog.h |
target_config.h |
▼ include |
c4_colours.h | Enumeration of LED colour combinations
c4_error_codes.h | Enumeration of Error Codes
c4_parser.h | Interface to simple parser
c4_privilege_modes.h | Provide mechanisms to specify which stack to use and for the processor to operate in Unprivileged mode and access Privileged mode
c4_qspi.h | Interface to QSPI Flash
c4_tftp.h | Functions to connect to an TFTP server and download application files and configurations
c4_watchdog.h | Interface to enable watchdog functions
▼ lib |
bl_api.c |
bl_api.h |
c4_colours.c | File to implement the coloured LED on the iMIMXRT1062 based board
c4_error_codes.c | Implementation of error code display via UART and LED
c4_parser.c | Parse ASCII config file
c4_privilege_modes.c | Implementation of privilege modes
c4_qspi.c | Implements read, write and erase functionality of QSPI
c4_qspi_types.h | Private header file for QSPI interface to allow definitions to be shared with test
c4_tftp.c | Implementation of TFTP protocol to send and receive application binary, application configuration, operation logs, and error logs
c4_watchdog.c | Implements watchdog functionality
c4_watchdog_types.h | Definition of types to aid manipulation of watchdog registers
▼ PfmLib |
platform_eeprom.c |
▼ src |
bootloader.c |
bootloader_types.h | Type defintions used by the bootloader
▼ startup |
startup_mimxrt1062.c |
▼ test |
c4_privilege_modes_test.c | Test operation in privileged and unprivileged modes
c4_privilege_modes_test.h | Interface to test privilege modes
c4_qspi_test.c | Test QSPI interface
c4_qspi_test.h |
c4_svc_test.c |
c4_svc_test.h |
excep_test.c |
excep_test.h |
excep_test_configuration.h |
watchdog_test.c |
watchdog_test.h |