Callisto4Bootloader: CoreDebug_Type Struct Reference

Callisto4Bootloader

Data Fields
CoreDebug_Type Struct Reference
Defines and Type Definitions » Status and Control Registers » Nested Vectored Interrupt Controller (NVIC) » System Control Block (SCB) » System Controls not in SCB (SCnSCB) » System Tick Timer (SysTick) » Instrumentation Trace Macrocell (ITM) » Data Watchpoint and Trace (DWT) » Trace Port Interface (TPI) » Floating Point Unit (FPU) » Core Debug Registers (CoreDebug)

Structure type to access the Core Debug Register (CoreDebug). More...

`#include <core_armv81mml.h>`

## Data Fields

__IOM uint32_t | DHCSR
__OM uint32_t | DCRSR
__IOM uint32_t | DCRDR
__IOM uint32_t | DEMCR
uint32_t | RESERVED4 [1U]
__IOM uint32_t | DAUTHCTRL
__IOM uint32_t | DSCSR

## Detailed Description

Structure type to access the Core Debug Register (CoreDebug).

Definition at line 1875 of file core_armv81mml.h.

The documentation for this struct was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h