Callisto4Bootloader: TSC_Type Struct Reference

Callisto4Bootloader

Data Fields
TSC_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » TSC Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | BASIC_SETTING
uint8_t | RESERVED_0 [12]
__IO uint32_t | PRE_CHARGE_TIME
uint8_t | RESERVED_1 [12]
__IO uint32_t | FLOW_CONTROL
uint8_t | RESERVED_2 [12]
__I uint32_t | MEASEURE_VALUE
uint8_t | RESERVED_3 [12]
__IO uint32_t | INT_EN
uint8_t | RESERVED_4 [12]
__IO uint32_t | INT_SIG_EN
uint8_t | RESERVED_5 [12]
__IO uint32_t | INT_STATUS
uint8_t | RESERVED_6 [12]
__IO uint32_t | DEBUG_MODE
uint8_t | RESERVED_7 [12]
__IO uint32_t | DEBUG_MODE2

## Detailed Description

TSC - Register Layout Typedef

Definition at line 40931 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h