Callisto4Bootloader: SEMC_Type Struct Reference

Callisto4Bootloader

Data Fields
SEMC_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » SEMC Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | MCR
__IO uint32_t | IOCR
__IO uint32_t | BMCR0
__IO uint32_t | BMCR1
__IO uint32_t | BR [9]
__IO uint32_t | DLLCR
__IO uint32_t | INTEN
__IO uint32_t | INTR
__IO uint32_t | SDRAMCR0
__IO uint32_t | SDRAMCR1
__IO uint32_t | SDRAMCR2
__IO uint32_t | SDRAMCR3
__IO uint32_t | NANDCR0
__IO uint32_t | NANDCR1
__IO uint32_t | NANDCR2
__IO uint32_t | NANDCR3
__IO uint32_t | NORCR0
__IO uint32_t | NORCR1
__IO uint32_t | NORCR2
__IO uint32_t | NORCR3
__IO uint32_t | SRAMCR0
__IO uint32_t | SRAMCR1
__IO uint32_t | SRAMCR2
uint32_t | SRAMCR3
__IO uint32_t | DBICR0
__IO uint32_t | DBICR1
uint8_t | RESERVED_0 [8]
__IO uint32_t | IPCR0
__IO uint32_t | IPCR1
__IO uint32_t | IPCR2
__IO uint32_t | IPCMD
__IO uint32_t | IPTXDAT
uint8_t | RESERVED_1 [12]
__I uint32_t | IPRXDAT
uint8_t | RESERVED_2 [12]
__I uint32_t | STS0
uint32_t | STS1
__I uint32_t | STS2
uint32_t | STS3
uint32_t | STS4
uint32_t | STS5
uint32_t | STS6
uint32_t | STS7
uint32_t | STS8
uint32_t | STS9
uint32_t | STS10
uint32_t | STS11
__I uint32_t | STS12
__I uint32_t | STS13
uint32_t | STS14
uint32_t | STS15

## Detailed Description

SEMC - Register Layout Typedef

Definition at line 36346 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h