Callisto4Bootloader: PIT_Type Struct Reference

Callisto4Bootloader

Data Fields
PIT_Type Struct Reference
Mapping Information » Edma_request » Iomuxc_pads » Device Peripheral Access Layer » PIT Peripheral Access Layer

`#include <MIMXRT1062.h>`

## Data Fields

__IO uint32_t | MCR
uint8_t | RESERVED_0 [220]
__I uint32_t | LTMR64H
__I uint32_t | LTMR64L
uint8_t | RESERVED_1 [24]
struct {
__IO uint32_t PIT_Type::LDVAL
__I uint32_t PIT_Type::CVAL
__IO uint32_t PIT_Type::TCTRL
__IO uint32_t PIT_Type::TFLG
} | CHANNEL [4]

## Detailed Description

PIT - Register Layout Typedef

Definition at line 30726 of file MIMXRT1062.h.

The documentation for this struct was generated from the following file:

- device/MIMXRT1062.h