Callisto4Bootloader: APSR_Type Union Reference

Callisto4Bootloader

Data Fields
APSR_Type Union Reference
Defines and Type Definitions » Status and Control Registers

Union type to access the Application Program Status Register (APSR). More...

`#include <core_armv81mml.h>`

## Data Fields

struct {
uint32_t APSR_Type::_reserved0:16
uint32_t APSR_Type::GE:4
uint32_t APSR_Type::_reserved1:7
uint32_t APSR_Type::Q:1
uint32_t APSR_Type::V:1
uint32_t APSR_Type::C:1
uint32_t APSR_Type::Z:1
uint32_t APSR_Type::N:1
} | b
uint32_t | w
struct {
uint32_t APSR_Type::_reserved0:28
uint32_t APSR_Type::V:1
uint32_t APSR_Type::C:1
uint32_t APSR_Type::Z:1
uint32_t APSR_Type::N:1
} | b
struct {
uint32_t APSR_Type::_reserved0:16
uint32_t APSR_Type::GE:4
uint32_t APSR_Type::_reserved1:7
uint32_t APSR_Type::Q:1
uint32_t APSR_Type::V:1
uint32_t APSR_Type::C:1
uint32_t APSR_Type::Z:1
uint32_t APSR_Type::N:1
} | b
struct {
uint32_t APSR_Type::_reserved0:16
uint32_t APSR_Type::GE:4
uint32_t APSR_Type::_reserved1:7
uint32_t APSR_Type::Q:1
uint32_t APSR_Type::V:1
uint32_t APSR_Type::C:1
uint32_t APSR_Type::Z:1
uint32_t APSR_Type::N:1
} | b

## Detailed Description

Union type to access the Application Program Status Register (APSR).

Definition at line 314 of file core_armv81mml.h.

The documentation for this union was generated from the following files:

- CMSIS/core_armv81mml.h
- CMSIS/core_armv8mbl.h
- CMSIS/core_armv8mml.h
- CMSIS/core_cm7.h