<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:93e6601e-da37-4f47-8685-8d3f54ae5df6">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:bde61c8d-7fb8-490e-a49c-762d3bd1cae0">
          <SHORT-NAME>Lin_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Lin</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:754b773c-6809-46a7-be78-94f24abb9262">
          <SHORT-NAME>Lin</SHORT-NAME>
          <DESC>
            <L-2 L="EN">
                           Configuration of the Lin (Local Interconnect Network) module. </L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>1.0.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2010-12-03</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <REFINED-MODULE-DEF-REF DEST="ECUC-MODULE-DEF">/AUTOSAR/EcucDefs/Lin</REFINED-MODULE-DEF-REF>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:f9793957-805b-400b-921f-acc6d3289e14">
              <SHORT-NAME>AutosarExt</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                            
                                AutosarExt
                                Autosar Requirements: 
                                This container contains the global configuration parameters of the Non-Autosar Lin driver. 
                                   This container is a MultipleConfigurationContainer, i.e. this container and 
                                   its sub-containers exist once per configuration set.
                            </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72a8a638-4009-4639-124a-bb4daf863a7b">
                  <SHORT-NAME>LinDisableDemReportErrorStatus</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                              
                                  LinDisableDemReportErrorStatus
                                  Switches the Diagnostic Error Reporting and Notification OFF.
                              </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72a8a638-4009-4639-124a-bb4daf863a7c">
                  <SHORT-NAME>LinDisableFrameTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                LinDisableFrameTimeout
                                                The master will accept the frame that is longer than TFrame_Maximum.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:72a8a638-4009-4639-124a-bb4daf863a77">
                  <SHORT-NAME>LinEnableUserModeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                LinEnableUserModeSupport
                                                When this parameter is enabled, the LIN module will adapt to run from User Mode
                                                Note:
                                                Lin module does not include registers protection. So, It is accessible to all registered in any public mode. Lin module is not affected by this field
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:386c52b6-2650-435a-a896-b6f81bccf83a">
              <SHORT-NAME>LinGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                              
                                  LinGeneral
                                  Autosar Requirements: LIN183_Conf
                                  This container contains the parameters related to each LIN Driver Unit. 
                                     This container is a MultipleConfigurationContainer, i.e. this container and 
                                     its sub-containers exit once per configuration set.
                              </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7228a638-4009-4639-8e1a-bb3d9f762a7b">
                  <SHORT-NAME>LinDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                              
                                  LinDevErrorDetect
                                  Autosar Requirements: LIN066_Conf
                                                Switches the Default Error Detection and Notification ON or OFF.
                              </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:8a1935ff-76b3-4a7e-aa67-e516f2704cfa">
                  <SHORT-NAME>LinIndex</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                              
                                  Specifies the InstanceId of this module instance. If only one instance is present it shall have the Id 0.
                                  Note, this parameter is not used in the current implementation.
                              </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:ea0e01de-6a8a-4565-840a-76cb28e5c197">
                  <SHORT-NAME>LinTimeoutDuration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">                
                                              
                              Specifies the maximum number of loops for blocking function until a timeout is raised in short term wait loops
                              </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1000</DEFAULT-VALUE>
                  <MAX>65535</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:be230747-6176-4c0b-90e2-290362e2d3ef">
                  <SHORT-NAME>LinVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                  
                  LinVersionInfoApi
                  Autosar Requirements: LIN067_Conf
                  Switches the Lin_GetVersionInfo function ON or OFF.
                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:4c0d3fc1-6d2c-4614-8f58-fa7632263cbb">
              <SHORT-NAME>LinDemEventParameterRefs</SHORT-NAME>
              <DESC>
                <L-2 L="EN">Container for the references to DemEventParameter elements which shall be invoked using the API Dem_SetEventStatus API in case the corresponding error occurs. The EventId is taken from the referenced DemEventParameter's DemEventId value. The standardized errors are provided in the container and can be extended by vendor specific error references.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <REFERENCES>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:111e0a82-ab9f-4c95-879f-b686bbba6c65">
                  <SHORT-NAME>LIN_E_TIMEOUT</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Timeout caused by hardware error&quot; has occured.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:ea2b8cf8-0ae8-4a24-bd07-1759472cf680">
              <SHORT-NAME>LinGlobalConfig</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                              
                              This container contains the global configuration parameter of the Lin driver. This container is a MultipleConfigurationContainer, i.e. this container and its sub-containers exit once per configuration set.                                        
                              </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:fdac1ad9-1217-44a8-bc3f-341635a20162">
                  <SHORT-NAME>LinChannel</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                  
                                  This container contains the configuration (parameters) of the LIN Controller(s).
                                  Note:&quot;User should use unique names for naming the LIN channels across different LinGlobalConfig Sets.&quot;
                                  </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:aac952ef-7cb7-4b94-acc5-b6c4ca835e7a">
                      <SHORT-NAME>LinChannelId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    
                                    Identifies the LIN channel. Replaces LIN_CHANNEL_INDEX_NAME from the LIN SWS.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>5</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:087f3523-f919-4b2d-841a-d18846908390">
                      <SHORT-NAME>LinChannelBaudRate</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                 
                                   LinChannelBaudRate
                                   Autosar Requirements: LIN180_Conf
                                   Specifies the baud rate of the LIN channel in 'bps'. Valid range: 1000..20000.
                                 </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>9600</DEFAULT-VALUE>
                      <MAX>20000</MAX>
                      <MIN>1000</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:2121e93b-3d41-4334-bcb4-6b273af183ec">
                      <SHORT-NAME>LinHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                       
                                    Selects the physical LIN Channel.
                                    Note: 
                                    This Parameter is an Implementation Specific Parameter.                       
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>eSCI_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eSCI_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eSCI_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eSCI_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eSCI_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eSCI_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>eSCI_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:572061dc-2b5c-4638-839d-2f4cd6fed1de">
                      <SHORT-NAME>LinChannelWakeupSupport</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                                       
                                    LinChannelWakeupSupport
                                    Autosar Requirements: LIN182_Conf
                                     Specifies if the LIN hardware channel supports wake up functionality.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:5419eaab-b72b-4ee1-9e89-22e203491b61">
                      <SHORT-NAME>LinClockRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    Reference to the LIN clock source configuration, which is set in the MCU driver configuration.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-REFERENCE-DEF UUID="ECUC:f5db6990-abc4-4480-bf42-27253f38f1e4">
                      <SHORT-NAME>LinClockRef_Alternate</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
								  Alternate reference to the LIN clock source configuration, which is set in the MCU driver configuration, used in Low Power Mode.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                    <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:59f8b925-adff-4508-8c3e-219d335e9f24">
                      <SHORT-NAME>LinChannelEcuMWakeupSource</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">This parameter contains a reference to the Wakeup Source for this controller as defined in the ECU State Manager.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource</DESTINATION-REF>
                    </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:5375a2dc-49f5-478c-8683-2aa697669008">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                                         
                                             Common container, aggregated by all modules. It contains published information about vendor and versions.
                                         </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:935af21d-a6f3-49c0-87e8-d2d3496a369c">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d80476cd-88a3-4bbd-b2bc-ddfd34e8647c">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:fc62a62f-5cb5-4c64-97d2-af849706fced">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:cc1aa557-fbff-4180-967b-ce245123bdee">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Module ID of this module from Module List.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>82</DEFAULT-VALUE>
                  <MAX>82</MAX>
                  <MIN>82</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:aed451e3-079d-48ea-a1f8-4e867daa4cf1">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b253ab94-d3c5-451f-8583-de105a2e7c5c">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:ec50d75b-5108-417f-a312-33c3438e7386">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:e9531a20-2560-4772-ba2a-c3a7610f5208">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                
                                                    In driver modules which can be instantiated several times on a single ECU, BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name. 
                                                    This parameter is used to specify the vendor specific name. In total, the implementation specific name is generated as follows:
                                                    &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt;. 
                                                    E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 
                                                    This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.
                                                
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:dbc03ef9-e4e5-415a-94d4-d41afce3c311">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                            
                                                Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                                            </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>