<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:4c5e3679-f5c4-49bf-9cea-d9be54e6eec7">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:c85149b7-c7bb-43ff-a18f-89f69b316fa0">
          <SHORT-NAME>Eth_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Eth</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:ebb8fd61-9918-4168-968c-3d703f5338dd">
          <SHORT-NAME>Eth</SHORT-NAME>
          <DESC>
            <L-2 L="EN">Configuration of the Eth (Ethernet Driver) module.</L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.6.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2014-10-31</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <REFINED-MODULE-DEF-REF DEST="ECUC-MODULE-DEF">/AUTOSAR/EcucDefs/Eth</REFINED-MODULE-DEF-REF>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-LINK-TIME</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:7e85fcfb-efe1-44d1-8afb-11b8ee9a0cf8">
              <SHORT-NAME>EthConfigSet</SHORT-NAME>
              <DESC>
                <L-2 L="EN">This container contains the configuration parameters and sub containers of the AUTOSAR Eth module.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:61af2394-882b-4c8b-81b3-667fdcc2c875">
                  <SHORT-NAME>EthCtrlConfig</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Configuration of the individual controller</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7d39dfd4-3492-400f-994c-1122305ad1924">
                      <SHORT-NAME>EthCtrlEnableMii</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables / Disables Media Independent Interface (MII) for transceiver access</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:26d9064e-2dc0-4722-b0b6-47c8e70f50cf">
                      <SHORT-NAME>EthCtrlEnableRxInterrupt</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables / Disables receive interrupt</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:165643c3-0de1-4d10-82bd-1234f2e5c486">
                      <SHORT-NAME>EthCtrlEnableTxInterrupt</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables / Disables transmit interrupt</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:86858da1-891d-4da7-952b-1af645591a7c">
                      <SHORT-NAME>EthCtrlIdx</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    Specifies the instance ID of the configured controller.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>ECU</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>255</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:86858da1-891d-4da7-952b-1af646591b7c">
                      <SHORT-NAME>EthCtrlMacLayerType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    Defines the MAC layer type of the ethernet controller.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>ECU</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>ETH_MAC_LAYER_TYPE_XMII</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_TYPE_XMII</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_TYPE_XGMII</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_TYPE_XXGMII</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:86858da1-891d-4da7-952b-1af645592b7c">
                      <SHORT-NAME>EthCtrlMacLayerSubType</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    Defines the MAC layer subtype of a switch port.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>ECU</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>STANDARD</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>REDUCED</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>SERIAL</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STANDARD</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:86858da1-891d-4da7-952b-1af111222a7c">
                      <SHORT-NAME>EthCtrlMacLayerSpeed</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    This bit = 0 &amp; Port Select(Eth line speed) = 1 =&gt; Speed = 10Mbps.
                                    This bit = 0 &amp; Port Select = 0 =&gt; Speed = 1Gbps.
                                    This bit = 1 &amp; Port Select = 1 =&gt; Speed = 100Mbps.
                                    This bit = 1 &amp; Port Select = 0 =&gt; Speed = 2.5Gbps.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>ECU</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DEFAULT-VALUE>ETH_MAC_LAYER_SPEED_10M</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_SPEED_10M</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_SPEED_100M</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_SPEED_1G</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>ETH_MAC_LAYER_SPEED_10G</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-STRING-PARAM-DEF UUID="ECUC:af1b57ea-5e70-4a83-a3db-3b9d604db304">
                      <SHORT-NAME>EthCtrlPhyAddress</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Specifies the unique 48-bit physical address (MAC address) of the controller in network byte order.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <ECUC-STRING-PARAM-DEF-VARIANTS>
                        <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                          <DEFAULT-VALUE>66:55:44:33:22:11</DEFAULT-VALUE>
                        </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      </ECUC-STRING-PARAM-DEF-VARIANTS>
                    </ECUC-STRING-PARAM-DEF>
                  </PARAMETERS>
                  <SUB-CONTAINERS>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:64e78874-950e-43c2-87fb-deff0f9d1217">
                      <SHORT-NAME>EthDemEventParameterRefs</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Container for the references to DemEventParameter elements which shall be invoked using the API Dem_ReportErrorStatus in case the corresponding error occurs. The EventId is taken from the referenced DemEventParameter's DemEventId value. The standardized errors are provided in the container and can be extended by vendor specific error references.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>LINK</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <REFERENCES>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:9686c2ed-dff4-4311-9568-bdcd583b4efe">
                          <SHORT-NAME>ETH_E_ACCESS</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Controller access failed&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:66a6db40-a8e0-43bf-a6f3-9def2e1866a0">
                          <SHORT-NAME>ETH_E_ALIGNMENT</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Alignment Error&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:7096a2ed-4004-4e82-bd36-f4df1522377d">
                          <SHORT-NAME>ETH_E_CRC</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;CRC Failure&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:67f01d1a-3a72-458e-a4ab-056d12c90b7d">
                          <SHORT-NAME>ETH_E_LATECOLLISION</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Late Collisions&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:33fd9cf3-513d-4b2e-8b31-3d07342c6612">
                          <SHORT-NAME>ETH_E_MULTIPLECOLLISION</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Multiple Collisions&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:0d8c1897-e226-4438-8e91-f58e7b74a9c7">
                          <SHORT-NAME>ETH_E_OVERSIZEFRAME</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Oversized Frame&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:7c3c19f2-72c3-4b60-bd4c-033e0c6fc41a">
                          <SHORT-NAME>ETH_E_RX_FRAMES_LOST</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;receive frames lost&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:7bbd76b3-0215-4b02-8c5a-2163e44555a5">
                          <SHORT-NAME>ETH_E_SINGLECOLLISION</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Single Collisions&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:8f4b3f61-6fa7-468b-9955-8dabed4ac40f">
                          <SHORT-NAME>ETH_E_UNDERSIZEFRAME</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Undersized Frame&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                      </REFERENCES>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:59f1ae22-2f03-4273-ac9e-ab7f0f3aa316">
                      <SHORT-NAME>EthVendorSpecific</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    Vendor specific: Vendor specific configuration of the individual controller
                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <PARAMETERS>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:839f673c-9f8a-4de8-a812-e8559ad990d6">
                          <SHORT-NAME>EthInternalLoopbackMode</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                        Vendor specific: Enables internal loopback mode - Receiver is internally connected with the transceiver. No external signals are used.
                                    </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:165643c3-0de1-4d10-82bd-5e5cf367c486">
                          <SHORT-NAME>EthPromiscousEn</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Enables /Disable filter addr of the incoming packet is SA.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:165643c3-0de1-4d10-82bd-5e5cf3457c486">
                          <SHORT-NAME>EthDisBroadcast</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Enables /Disable Broadcast Packets.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>false</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:c0a50b61-24f4-45c0-bc45-d5d912abc4c7c49">
                          <SHORT-NAME>EthMiiSpeed</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                        Vendor specific: Controls the frequency of the MII management interface clock relative to the internal bus clock.
                                        Any non-zero value results in the FEC_MDC frequency of 1/(MII_SPEED x 2) of the internal bus frequency.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>5</DEFAULT-VALUE>
                          <MAX>63</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:c8c32912-bc2d-4bc9-a3f5-24b39aa9a07a">
                          <SHORT-NAME>EthFullDuplexEnable</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                        Vendor specific: Enables / disables full duplex mode.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                          <DEFAULT-VALUE>true</DEFAULT-VALUE>
                        </ECUC-BOOLEAN-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:86858da1-891d-4da7-952b-1af645591b7e">
                          <SHORT-NAME>EthTxQueueNum</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                        Select number of queue to transmit.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DEFAULT-VALUE>1</DEFAULT-VALUE>
                          <MAX>255</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                        <ECUC-INTEGER-PARAM-DEF UUID="ECUC:86858de1-891d-4da7-952b-1af645591b7c">
                          <SHORT-NAME>EthRxQueueNum</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                        Select number of queue to Receive.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>NXP</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DEFAULT-VALUE>1</DEFAULT-VALUE>
                          <MAX>255</MAX>
                          <MIN>0</MIN>
                        </ECUC-INTEGER-PARAM-DEF>
                      </PARAMETERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:7bbd76b3-0215-4b02-8c5a-21345678555a5">
                      <SHORT-NAME>EthCtrlConfigEgress</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                    Controller Configuration Egress : Egress Controller configuration of the individual controller
                                </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <REFERENCES>
                        <ECUC-REFERENCE-DEF UUID="ECUC:7bbd76b3-0215-4b02-8c5a-2164e44555a5">
                          <SHORT-NAME>EthCtrlConfigEgressLastSchedulerRef</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">Reference to the DemEventParameter which shall be issued when the error &quot;Single Collisions&quot; has occured.</L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <SCOPE>LOCAL</SCOPE>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Eth/EthConfigSet/EthCtrlConfig/EthCtrlConfigEgress/EthCtrlConfigScheduler</DESTINATION-REF>
                        </ECUC-REFERENCE-DEF>
                      </REFERENCES>
                      <SUB-CONTAINERS>
                        <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:76704b6a-fa43-4bd4-bf87-3e27b65gf4ac9d">
                          <SHORT-NAME>EthCtrlConfigEgressFifo</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                            Controller Configuration Egress : Egress Controller configuration of the individual controller
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <PARAMETERS>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:76704b6a-fa43-4bd4-bf87-3e27b5efac9d">
                              <SHORT-NAME>EthCtrlConfigEgressFifoBufLenByte</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Limits the maximum transmit buffer length (frame length) in bytes. Maximal frame payload is equal to the configured value decreased by 14 bytes that are used for the frame header.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>128</DEFAULT-VALUE>
                              <MAX>2047</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1118-4b32-9424-8d5fdcaf9e1e">
                              <SHORT-NAME>EthCtrlConfigEgressFifoBufTotal</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Fifo buffer count.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>16</DEFAULT-VALUE>
                              <MAX>255</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1228-4b32-9424-8d5fdcaf9e2a">
                              <SHORT-NAME>EthCtrlConfigEgressFifoIdx</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Configures the number of transmit buffers.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>0</DEFAULT-VALUE>
                              <MAX>255</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1118-5a32-9424-8d5fdcaf9e2a">
                              <SHORT-NAME>EthCtrlConfigEgressFifoPriorityAssignment</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Configures the number of transmit buffers.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                              <SCOPE>LOCAL</SCOPE>
                              <MULTIPLICITY-CONFIG-CLASSES>
                                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              </MULTIPLICITY-CONFIG-CLASSES>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>0</DEFAULT-VALUE>
                              <MAX>7</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                          </PARAMETERS>
                        </ECUC-PARAM-CONF-CONTAINER-DEF>
                        <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:10dc5fce-1118-4b32-3245-8d5f68764544666a">
                          <SHORT-NAME>EthCtrlConfigScheduler</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                            Controller Configuration Scheduler : Represents a Scheduler on the egress side.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <SUB-CONTAINERS>
                            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:10dc5fce-1118-4b32-3245-8d5f66666666a">
                              <SHORT-NAME>EthCtrlConfigSchedulerPredecessor</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">
                                                    Controller Configuration Scheduler Predecessors: Defines an ordered list of predecessors for this scheduler.
                                                </L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <PARAMETERS>
                                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1118-4b32-3245-8d5fdcaf9e2a">
                                  <SHORT-NAME>EthCtrlConfigSchedulerPredecessorOrder</SHORT-NAME>
                                  <DESC>
                                    <L-2 L="EN">Defines the order of the scheduler predecessors.</L-2>
                                  </DESC>
                                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                                  <SCOPE>LOCAL</SCOPE>
                                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                                  <VALUE-CONFIG-CLASSES>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                  </VALUE-CONFIG-CLASSES>
                                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                                  <MAX>255</MAX>
                                  <MIN>0</MIN>
                                </ECUC-INTEGER-PARAM-DEF>
                              </PARAMETERS>
                              <REFERENCES>
                                <ECUC-CHOICE-REFERENCE-DEF UUID="ECUC:10dc5fce-11245-4b32-9424-8d5fdcaf9e2a">
                                  <SHORT-NAME>EthCtrlConfigSchedulerPredecessorRef</SHORT-NAME>
                                  <DESC>
                                    <L-2 L="EN">Choice reference to the scheduler predecessor.</L-2>
                                  </DESC>
                                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                                  <SCOPE>LOCAL</SCOPE>
                                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                                  <VALUE-CONFIG-CLASSES>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                  </VALUE-CONFIG-CLASSES>
                                  <DESTINATION-REFS>
                                    <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Eth/EthConfigSet/EthCtrlConfig/EthCtrlConfigEgress/EthCtrlConfigEgressFifo</DESTINATION-REF>
                                    <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Eth/EthConfigSet/EthCtrlConfig/EthCtrlConfigEgress/EthCtrlConfigScheduler</DESTINATION-REF>
                                    <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Eth/EthConfigSet/EthCtrlConfig/EthCtrlConfigEgress/EthCtrlConfigShaper</DESTINATION-REF>
                                  </DESTINATION-REFS>
                                </ECUC-CHOICE-REFERENCE-DEF>
                              </REFERENCES>
                            </ECUC-PARAM-CONF-CONTAINER-DEF>
                          </SUB-CONTAINERS>
                        </ECUC-PARAM-CONF-CONTAINER-DEF>
                        <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:10dc5fce-1118-4b32-9424-8d5123f9e2a">
                          <SHORT-NAME>EthCtrlConfigShaper</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                            Controller Configuration Shaper : Represents a Shaper an the egress side.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <PARAMETERS>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1118-4b32-9424-8d5eadaf9e2a">
                              <SHORT-NAME>EthCtrlConfigShaperIdleSlope</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Defines the increase of credit in bits per second for the AVB shaper.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>0</DEFAULT-VALUE>
                              <MAX>1000000000</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                          </PARAMETERS>
                          <REFERENCES>
                            <ECUC-REFERENCE-DEF UUID="ECUC:10dc5fce-4448-4b32-9424-8d5fdcaf9e2a">
                              <SHORT-NAME>EthCtrlConfigShaperPredecessorFifoRef</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Reference to the fifo which is the predecessor for this shaper.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Eth/EthConfigSet/EthCtrlConfig/EthCtrlConfigEgress/EthCtrlConfigEgressFifo</DESTINATION-REF>
                            </ECUC-REFERENCE-DEF>
                          </REFERENCES>
                          <SUB-CONTAINERS>
                            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:a240e482-f8b4-4ccb-b0d1-8537012345f6d">
                              <SHORT-NAME>EthVendorSpecific</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">
                                               Vendor specific: General vendor specific configuration of Ethernet Driver module
                                                </L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <PARAMETERS>
                                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10ef456f-1118-4b32-9424-8d5eadaf9e2a">
                                  <SHORT-NAME>EthCtrlConfigShaperSendSlope</SHORT-NAME>
                                  <DESC>
                                    <L-2 L="EN">Defines the decrease of credit in bits per second for the AVB shaper.</L-2>
                                  </DESC>
                                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                                  <SCOPE>LOCAL</SCOPE>
                                  <ORIGIN>NXP</ORIGIN>
                                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                                  <VALUE-CONFIG-CLASSES>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                  </VALUE-CONFIG-CLASSES>
                                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                                  <MAX>1000000000</MAX>
                                  <MIN>0</MIN>
                                </ECUC-INTEGER-PARAM-DEF>
                                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10ef456f-1118-4b32-9424-8d5564327f">
                                  <SHORT-NAME>EthCtrlConfigHiCredit</SHORT-NAME>
                                  <DESC>
                                    <L-2 L="EN">Define the maximum value that can be accumulated in the credit parameter.</L-2>
                                  </DESC>
                                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                                  <SCOPE>LOCAL</SCOPE>
                                  <ORIGIN>NXP</ORIGIN>
                                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                                  <VALUE-CONFIG-CLASSES>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                  </VALUE-CONFIG-CLASSES>
                                  <DEFAULT-VALUE>134217728</DEFAULT-VALUE>
                                  <MAX>536870911</MAX>
                                  <MIN>0</MIN>
                                </ECUC-INTEGER-PARAM-DEF>
                                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10ef456f-1118-4b32-9424-8d77665444d">
                                  <SHORT-NAME>EthCtrlConfigLoCredit</SHORT-NAME>
                                  <DESC>
                                    <L-2 L="EN">Define the minimum value that can be accumulated in the credit parameter.</L-2>
                                  </DESC>
                                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                                  <SCOPE>LOCAL</SCOPE>
                                  <ORIGIN>NXP</ORIGIN>
                                  <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                                  <VALUE-CONFIG-CLASSES>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                    <ECUC-VALUE-CONFIGURATION-CLASS>
                                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                    </ECUC-VALUE-CONFIGURATION-CLASS>
                                  </VALUE-CONFIG-CLASSES>
                                  <DEFAULT-VALUE>402653184</DEFAULT-VALUE>
                                  <MAX>536870911</MAX>
                                  <MIN>0</MIN>
                                </ECUC-INTEGER-PARAM-DEF>
                              </PARAMETERS>
                            </ECUC-PARAM-CONF-CONTAINER-DEF>
                          </SUB-CONTAINERS>
                        </ECUC-PARAM-CONF-CONTAINER-DEF>
                      </SUB-CONTAINERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:d2f023de-e145-12345-b152-23f611c4e584">
                      <SHORT-NAME>EthCtrlConfigIngress</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                                        Controller Configuration Ingress : Configuration of one Ethernet controler ingress behavior.
                                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SUB-CONTAINERS>
                        <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:d2f023de-e145-46eb-b152-123456c4e584">
                          <SHORT-NAME>EthCtrlConfigIngressFifo</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                                            Controller Configuration Ingress : Represents a Fifo at the ingress side.
                                        </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                          <MULTIPLICITY-CONFIG-CLASSES>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>LINK</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                            <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          </MULTIPLICITY-CONFIG-CLASSES>
                          <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                          <PARAMETERS>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d2f023de-e145-46eb-b152-23f611c4e584">
                              <SHORT-NAME>EthCtrlConfigIngressFifoBufLenByte</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Limits the maximum receive buffer length (frame length) in bytes.                                                 To compute the value: the frame payload length shall be extended                                                 by 14 bytes for frame header and 4 bytes for the frame CRC,                                                 then it shall be increased to a multiple of 16 bytes. </L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                              <DEFAULT-VALUE>64</DEFAULT-VALUE>
                              <MAX>2032</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:03a45d10-c0aa-44c0-9ff7-7eebdbf94c7c">
                              <SHORT-NAME>EthCtrlConfigIngressFifoBufTotal</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Fifo buffer count.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>16</DEFAULT-VALUE>
                              <MAX>255</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1118-4b32-9424-8d5fdcaf9e3f">
                              <SHORT-NAME>EthCtrlConfigIngressFifoIdx</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Ingress Fifo index.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                              <SCOPE>LOCAL</SCOPE>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                              <DEFAULT-VALUE>0</DEFAULT-VALUE>
                              <MAX>255</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                            <ECUC-INTEGER-PARAM-DEF UUID="ECUC:10dc5fce-1118-4b32-9424-8d78dcaf9e2a">
                              <SHORT-NAME>EthCtrlConfigIngressFifoPriorityAssignment</SHORT-NAME>
                              <DESC>
                                <L-2 L="EN">Message ingress prority assignment.</L-2>
                              </DESC>
                              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                              <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                              <SCOPE>LOCAL</SCOPE>
                              <MULTIPLICITY-CONFIG-CLASSES>
                                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                              </MULTIPLICITY-CONFIG-CLASSES>
                              <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                              <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                              <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                              <VALUE-CONFIG-CLASSES>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>LINK</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                                <ECUC-VALUE-CONFIGURATION-CLASS>
                                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                                </ECUC-VALUE-CONFIGURATION-CLASS>
                              </VALUE-CONFIG-CLASSES>
                              <DEFAULT-VALUE>0</DEFAULT-VALUE>
                              <MAX>7</MAX>
                              <MIN>0</MIN>
                            </ECUC-INTEGER-PARAM-DEF>
                          </PARAMETERS>
                        </ECUC-PARAM-CONF-CONTAINER-DEF>
                      </SUB-CONTAINERS>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                  </SUB-CONTAINERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:601d84ff-38c7-4c13-9f7d-cb74dafebae4">
              <SHORT-NAME>EthGeneral</SHORT-NAME>
              <DESC>
                <L-2 L="EN">General configuration of Ethernet Driver module</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ba826417-4631-45aa-a826-c2197826cce2">
                  <SHORT-NAME>EthDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables development error detection.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6e96cafd-be35-4b19-9af2-b094f3384801">
                  <SHORT-NAME>EthGetCounterValuesApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables Eth_GetDropCount API.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:962ec9c9-decd-48f5-8869-28ec5cd1f187">
                  <SHORT-NAME>EthGetRxStatsApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables EthGetRxStatsApi API.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:962ec9c9-decd-48f5-8869-28ec5cd1f188">
                  <SHORT-NAME>EthGetTxStatsApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables EthGetTxStatsApi API.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:962ec9c9-decd-48f5-8869-111122d1f188">
                  <SHORT-NAME>EthGetDropCountApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables EthGetDropCountApi API.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:962ec9c9-decd-48f5-8869-28ec5cd1ff22">
                  <SHORT-NAME>EthGetEtherStatsApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables EthGetEtherStatsApi API.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:962ec9c9-decd-48f5-8869-28ec5cd1f189">
                  <SHORT-NAME>EthGetTxErrorCounterValuesApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables EthGetTxErrorCounterValuesApi API.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:788e1613-b8ee-4dff-b458-c914b9783b2e">
                  <SHORT-NAME>EthGlobalTimeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables/Disables the GlobalTime APIs used amongst others by Global Time Synchronization over Ethernet.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:6aaf0d93-a6cb-481a-902c-c65865abde8a">
                  <SHORT-NAME>EthIndex</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Specifies the InstanceId of this module instance. If only one instance is present it shall have the Id 0.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-FLOAT-PARAM-DEF UUID="ECUC:4e68cddf-2c20-4ecb-97a7-a8ddcb95d16a">
                  <SHORT-NAME>EthMainFunctionPeriod</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Specifies the period of main function Eth_MainFunction in seconds.                                          Ethernet driver does not require this information but the BSW scheduler.                                          ASR define Infinity as limitation, but it is abnormal if the period is longer than 65.535 second</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0.0</DEFAULT-VALUE>
                  <MAX>65.535</MAX>
                  <MIN>0.0</MIN>
                </ECUC-FLOAT-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:7e6614fd-901b-46f1-ab12-b80a10d8e2e7">
                  <SHORT-NAME>EthMaxCtrlsSupported</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Limits the total number of supported controllers.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>255</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:1b42b17c-01dc-4617-abf9-48d5deddc074">
                  <SHORT-NAME>EthUpdatePhysAddrFilter</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables/Disables optional API Eth_UpdatePhysAddrFilter.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:4548795d-6059-49cc-89df-5f6c20e0a0ae">
                  <SHORT-NAME>EthVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enables / Disables version info API</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:a6bc8ec0-2e28-4b30-83d1-7ed6b2a1eb1e">
                  <SHORT-NAME>EthCtrlOffloading</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Configuration of hardware offloading features.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9e4e8407-a9c7-42f3-808f-68e241b683fb">
                      <SHORT-NAME>EthCtrlEnableOffloadChecksumICMP</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables  /  Disables  hardware offloading for ICMP checksums.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ee78a930-e716-445e-aabd-9aed81f5f8d6">
                      <SHORT-NAME>EthCtrlEnableOffloadChecksumIPv4</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables  /  Disables  hardware offloading for IPv4 checksums.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:b6e30534-9d47-4854-b983-4f37d0ac0da7">
                      <SHORT-NAME>EthCtrlEnableOffloadChecksumTCP</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables  /  Disables  hardware offloading for TCP checksums.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:8bbe5cf9-08cb-4842-826c-6fe0eca28407">
                      <SHORT-NAME>EthCtrlEnableOffloadChecksumUDP</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">Enables  /  Disables  hardware offloading for UDP checksums.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:a240e482-f8b4-4ccb-b0d1-85370539f54c">
                  <SHORT-NAME>EthVendorSpecific</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                       Vendor specific: General vendor specific configuration of Ethernet Driver module
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:a40daac0-f25e-44a6-bbd0-3794527ab038">
                      <SHORT-NAME>EthBridgeSupport</SHORT-NAME>
                      <DESC>
                        <L-2 L="FOR-ALL"> 
                                Vendor specific: When this option is ON, the Ethernet Bridge feature allows difference source address. 
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:a40daac0-f25e-44a6-bbd0-3794527ab858">
                      <SHORT-NAME>EthDisableDemEventDetect</SHORT-NAME>
                      <DESC>
                        <L-2 L="FOR-ALL"> 
                                Vendor specific: When this option is ON the Diagnostic Event Manager is disabled, no diagnostic error events are reported. 
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:7e02e722-7a66-4519-a197-59763332a28f">
                      <SHORT-NAME>EthMulticastPoolSize</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                            Vendor specific: Defines maximal count of addresses in multicast pool.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>15</DEFAULT-VALUE>
                      <MAX>512</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:fbb4800a-1114-4ef4-9a8b-396befc038de">
                      <SHORT-NAME>EthEnableUserModeSupport</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                            
                                When this parameter is enabled, the Eth module will adapt to run from User Mode, with the following measures:
                                (if applicable) a) configuring REG_PROT for the Eth Controllers so that the registers under protection eth be accessed from user mode by setting UAA bit in REG_PROT_GCR to 1
                                (if applicable) b) using 'call trusted function' stubs for all internal function calls that access registers requiring supervisor mode.
                                (if applicable) c) other module specific measures for more information, please see chapter 5.7 User Mode Support in IM
                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:fb6193b0-f869-4932-b893-5260a87654765d">
                      <SHORT-NAME>EthSwtManagementSupportApi</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        Vendor specific: Enables / disables the Switch management APIs to support a Switch port specific
                        communication attribute access.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:fb6193b0-f869-4932-b893-5260af111a3e">
                      <SHORT-NAME>EthUseMultiBufferRxFrames</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        Vendor specific: Enables / disables support of spreading Eth frames over
                        multiple RX buffers.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>Freescale</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6a14477a-1ba5-4864-a922-4651a6e935b1">
                      <SHORT-NAME>EthEnableRxFrameWrap</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        Vendor specific: Enables / disables support of multi-buffers frames
                        wrapped over the receive buffer ring. Parameter is only accessible
                        and considered during generation when value of EthUseMultiBufferRxFrames
                        is set to 'true'.
                      </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>Freescale</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:d36750fb-5e75-4e34-8a48-33921f04741a">
                      <SHORT-NAME>EthUseMultiBufferTxFrames</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        Vendor specific: Enables / disables support of spreading Eth frames over
                        multiple TX buffers.
                      </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d36750fb-5e75-4e34-8a48-3391122334455ff">
                      <SHORT-NAME>EthMaxFrameLength</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        Vendor specific: Maximum frame lengt.
                      </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <SCOPE>LOCAL</SCOPE>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>2047</DEFAULT-VALUE>
                      <MAX>2047</MAX>
                      <MIN>64</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                  </PARAMETERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:4a4455b9-6a43-4f86-bf73-dad9bd3d9316">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                    Common container, aggregated by all modules. It contains published information about vendor and versions.
                  </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:1cf13a57-ad8e-444b-8610-c5c52f086a60">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:75722624-3bae-4af9-bebf-ebb98c908f30">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:987054f3-afce-4681-b8d1-d8f3ff66df92">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:100545fd-f592-4d92-9d32-934beabc095b">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Module ID of this module from Module List.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>88</DEFAULT-VALUE>
                  <MAX>88</MAX>
                  <MIN>88</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d1b8ea5e-0174-4f67-9c67-0575509bfc8e">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:9c1aba23-4ff6-485b-89a7-7a45bd19b97f">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:702850db-94e5-4e3e-bc4e-9239784c4e75">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:6a2eb605-a654-427b-93c0-c9d5cb92c356">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      In driver modules which can be instantiated several times on a single ECU,
                      BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name. 
                      This parameter is used to specify the vendor specific name.
                      In total, the implementation specific name is generated as follows:
                      [ModuleName]_[VendorId]_[VendorApiInfix][Api name from SWS].
                      E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a
                      VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write. 
                      This parameter is mandatory for all modules with upper multiplicity &gt; 1.
                      It shall not be used for modules with upper multiplicity =1.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:a4c6d14e-0812-4a52-8455-3b3e6070dcca">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                        Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-LINK-TIME</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>