<?xml version="1.0"?>
<AUTOSAR xmlns="http://autosar.org/schema/r4.0" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://autosar.org/schema/r4.0 AUTOSAR_00044.xsd">
  <AR-PACKAGES>
    <AR-PACKAGE UUID="ECUC:b736806f-0bbf-44c8-bb9b-8a69a74a0def">
      <SHORT-NAME>TS_T2D41M10I0R0</SHORT-NAME>
      <ELEMENTS>
        <ECUC-DEFINITION-COLLECTION UUID="ECUC:5e2ab28a-52bc-4820-8f3d-23cf92d2e993">
          <SHORT-NAME>Gpt_EcuParameterDefinition</SHORT-NAME>
          <MODULE-REFS>
            <MODULE-REF DEST="ECUC-MODULE-DEF">/TS_T2D41M10I0R0/Gpt</MODULE-REF>
          </MODULE-REFS>
        </ECUC-DEFINITION-COLLECTION>
        <ECUC-MODULE-DEF UUID="ECUC:d70ceb7b-c498-4d61-aa01-fa7c04d2806c">
          <SHORT-NAME>Gpt</SHORT-NAME>
          <DESC>
            <L-2 L="EN">
                  
                  Configuration of the Gpt (General Purpose Timer) module.
                  </L-2>
          </DESC>
          <ADMIN-DATA>
            <DOC-REVISIONS>
              <DOC-REVISION>
                <REVISION-LABEL>4.1.0</REVISION-LABEL>
                <ISSUED-BY>AUTOSAR</ISSUED-BY>
                <DATE>2010-12-03</DATE>
              </DOC-REVISION>
            </DOC-REVISIONS>
          </ADMIN-DATA>
          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
          <POST-BUILD-VARIANT-SUPPORT>true</POST-BUILD-VARIANT-SUPPORT>
          <REFINED-MODULE-DEF-REF DEST="ECUC-MODULE-DEF">/AUTOSAR/EcucDefs/Gpt</REFINED-MODULE-DEF-REF>
          <SUPPORTED-CONFIG-VARIANTS>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-POST-BUILD</SUPPORTED-CONFIG-VARIANT>
            <SUPPORTED-CONFIG-VARIANT>VARIANT-PRE-COMPILE</SUPPORTED-CONFIG-VARIANT>
          </SUPPORTED-CONFIG-VARIANTS>
          <CONTAINERS>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:7d918cce-a524-4501-ad5f-9ce8c67fc9c3">
              <SHORT-NAME>GptDemEventParameterRefs</SHORT-NAME>
              <DESC>
                <L-2 L="EN">Container for the references to DemEventParameter elements which shall be invoked using the API Dem_SetEventStatus in case the corresponding error occurs.                          The EventId is taken from the referenced DemEventParameter's DemEventId value.</L-2>
              </DESC>
              <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <MULTIPLICITY-CONFIG-CLASSES>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                  <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
              </MULTIPLICITY-CONFIG-CLASSES>
              <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
              <REFERENCES>
                <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:6055f74a-670e-4f85-9621-982c8bab0939">
                  <SHORT-NAME>GPT_E_TIMEOUT</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                                Reference to configured DEM event to report &quot;Timeout failure&quot;.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Dem/DemConfigSet/DemEventParameter</DESTINATION-REF>
                </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
              </REFERENCES>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:cd0335d7-f7fd-41f0-98d7-208937c37066">
              <SHORT-NAME>GptChannelConfigSet</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                  
                    This container is the base of an Configuration Set which contains the configured GPT channels. 
                    This way, different configuration sets can be defined for post-build process.
                  </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:07c7e4eb-893e-41ff-8495-dbddbfdaed20">
                  <SHORT-NAME>GptChannelConfiguration</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                      
                        This container contains the channel-wide configuration (parameters) of the GPT Driver
                      </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:06a53468-cc91-4fcf-8e5d-59602a241338">
                      <SHORT-NAME>GptChannelId</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        
                        Channel Id of the GPT channel. This value will be assigned to the symbolic name derived of the GptChannelConfiguration container short name.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>0</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:909509cc-4634-4c39-8e48-9babfb67da30">
                      <SHORT-NAME>GptHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                      
                      Vendor specific: Selects the physical GPT Channel.
                      </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>EMIOS_0_CH_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>PIT_0_CH_RTI</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>PIT_0_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>PIT_0_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>PIT_0_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>PIT_0_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:2b6019f0-4c30-408f-ab54-45eee4ac63c2">
                      <SHORT-NAME>GptChannelMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        
                        Specifies the behaviour of the timerchannel after the timeout has expired
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>GPT_CH_MODE_ONESHOT</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>GPT_CH_MODE_CONTINUOUS</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>GPT_CH_MODE_ONESHOT</SHORT-NAME>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-FLOAT-PARAM-DEF UUID="ECUC:f94d0799-902c-4d55-8dc3-719d65676bab">
                      <SHORT-NAME>GptChannelTickFrequency</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        
                        EN: Specifies the tick frequency of the timer channel in Hz.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>0.0</DEFAULT-VALUE>
                      <MAX>1.6E8</MAX>
                      <MIN>0.0</MIN>
                    </ECUC-FLOAT-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:98970b00-6a8c-4d69-bb54-0138d07d1e83">
                      <SHORT-NAME>GptChannelPrescaler</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         Vendor specific: The GPT module specific clock prescaler value. 
                                Note with STM: 
                                - STM prescaler should be between 1-256. 
                                Note with EMIOS: 
                                - EMIOS prescaler should be between 1-4. 
                                Note with PIT: 
                                - PIT prescaler should be 1. 
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>256</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:2fe548f7-27e7-4395-9c6a-e40e5ad701bb">
                      <SHORT-NAME>GptChannelPrescalerAlternate</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         Vendor specific: The GPT module specific clock prescaler value. 
                                Note with STM: 
                                - STM prescaler should be between 1-256. 
                                Note with EMIOS: 
                                - EMIOS prescaler should be between 1-4. 
                                Note with PIT: 
                                - PIT prescaler should be 1.                                 
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>256</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b4052610-87a4-41ee-ae69-e60eca5e9959">
                      <SHORT-NAME>GptChannelTickValueMax</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         Maximum value in ticks, the timer channel is able to count. 
                               With the next tick, the timer rolls over to zero.
                               It is mandatory to set 4294967295 for the PITRTI, PIT and STM channels
                               (coresponding to the 32 bits counter resolution) and 16777215 for
                               the EMIOS channels (corresponding to the 24 bits counter resolution)!
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>16777215</DEFAULT-VALUE>
                      <MAX>4294967295</MAX>
                      <MIN>16777215</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:04ebe0e7-6f02-474f-abf5-ef1f0243d2e5">
                      <SHORT-NAME>GptFreezeEnable</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        
                          Vendor specific: Select to set Freeze enable for the hw resources.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:5b45dd65-a5c8-4d8b-b821-305056680189">
                      <SHORT-NAME>GptEnableWakeup</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        
                          Enables wakeup capability of CPU for a channel.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:2fe548f7-27e7-4395-9c55-e40e5ad701bb">
                      <SHORT-NAME>GptChainMode</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         Vendor specific: Enable/disable Chain Mode for PIT.                            
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>false</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                    <ECUC-FUNCTION-NAME-DEF UUID="ECUC:d7132119-f0cc-4907-8022-6eaceb7fe604">
                      <SHORT-NAME>GptNotification</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                        
                        Function pointer to callback function(for non-wakeup notification).
                        The field is editable only if the switch GptEnableDisableNotificationApi is true.
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-MULTIPLICITY>true</POST-BUILD-VARIANT-MULTIPLICITY>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <ECUC-FUNCTION-NAME-DEF-VARIANTS>
                        <ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                          <DEFAULT-VALUE>NULL_PTR</DEFAULT-VALUE>
                        </ECUC-FUNCTION-NAME-DEF-CONDITIONAL>
                      </ECUC-FUNCTION-NAME-DEF-VARIANTS>
                    </ECUC-FUNCTION-NAME-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:5332d705-fc82-4376-a2b5-0dd21da3fb8e">
                      <SHORT-NAME>GptChannelClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                            
                                Reference to the GptClockReferencePoint from which the channel clock is derived.
                           </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Gpt/GptDriverConfiguration/GptClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                  <SUB-CONTAINERS>
                    <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:e30a5e2f-800e-4bd9-ab90-348eb3840014">
                      <SHORT-NAME>GptWakeupConfiguration</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                            
                              This container defines the wakeup source codes reported to Ecu State Manager.
                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <MULTIPLICITY-CONFIG-CLASSES>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                        <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      </MULTIPLICITY-CONFIG-CLASSES>
                      <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                      <REFERENCES>
                        <ECUC-SYMBOLIC-NAME-REFERENCE-DEF UUID="ECUC:a0417082-d81a-4d14-b58c-6e533fb218d2">
                          <SHORT-NAME>GptWakeupSourceRef</SHORT-NAME>
                          <DESC>
                            <L-2 L="EN">
                            
                              In case the wakeup-capability is true this value is transmitted to the Ecu State Manager. Implementation Type: reference to EcuM_WakeupSourceType
                            </L-2>
                          </DESC>
                          <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                          <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                          <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                          <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                          <VALUE-CONFIG-CLASSES>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                            <ECUC-VALUE-CONFIGURATION-CLASS>
                              <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                              <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                            </ECUC-VALUE-CONFIGURATION-CLASS>
                          </VALUE-CONFIG-CLASSES>
                          <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/EcuM/EcuMConfiguration/EcuMCommonConfiguration/EcuMWakeupSource</DESTINATION-REF>
                        </ECUC-SYMBOLIC-NAME-REFERENCE-DEF>
                      </REFERENCES>
                    </ECUC-PARAM-CONF-CONTAINER-DEF>
                  </SUB-CONTAINERS>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de2adbaf-35ef-fd23-89de-65665795e1bh">
              <SHORT-NAME>GptHwConfiguration</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                            List of all HW channel resources for GPT module.
                            </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>42</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>42</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:42bdb265-2e2e-9d91-abcd-977c9fc0cb5g">
                  <SHORT-NAME>GptIsrHwId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    ID of HW interrupt resources.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>true</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>EMIOS_0_CH_1</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_0</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_1</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_2</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_3</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_4</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_5</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_6</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_7</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_16</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_17</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_18</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_19</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_20</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_21</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_22</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_0_CH_23</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_0</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_1</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_2</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_3</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_4</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_5</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_6</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_7</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_16</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_17</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_18</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_19</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_20</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_21</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_22</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>EMIOS_1_CH_23</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>PIT_0_CH_RTI</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>PIT_0_CH_0</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>PIT_0_CH_1</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>PIT_0_CH_2</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>PIT_0_CH_3</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>STM_0_CH_0</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>STM_0_CH_1</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>STM_0_CH_2</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>STM_0_CH_3</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>STM_0_PREDEF</SHORT-NAME>
                      <ORIGIN>NXP</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:04fbe442-ffd3-56fd-8e68-9f7c9fc0cb2a">
                  <SHORT-NAME>GptIsrEnable</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Enable/Disable HW channels' Interrupt Sources.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:04ebf442-ffd3-fd56-8e68-7c9f9fc023c1">
                  <SHORT-NAME>GptChannelIsUsed</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    This column configures HW channels which are going to be used.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>LOCAL</SCOPE>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:4a7cfc3b-225f-491f-a419-3c42feaa78e0">
              <SHORT-NAME>GptConfigurationOfOptApiServices</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                    
                    This container contains all configuration switches for configuring optional API services of the GPT driver.
                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7043a635-908e-4097-b992-49e237f5f38c">
                  <SHORT-NAME>GptDeinitApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the service Gpt_DeInit() from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:08b40b71-4849-411b-abd0-84973f8fd4b8">
                  <SHORT-NAME>GptEnableDisableNotificationApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the services Gpt_EnableNotification() and Gpt_DisableNotification from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:a8c9dd24-0e73-41d5-ad00-db9690b32938">
                  <SHORT-NAME>GptTimeElapsedApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the service Gpt_GetTimeElapsed() from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:41867b3c-4324-4f47-a119-e8b1a0c094f2">
                  <SHORT-NAME>GptTimeRemainingApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the service Gpt_GetTimeRemaining() from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:e3717f6d-21ff-46f5-9858-f76c3f8aceeb">
                  <SHORT-NAME>GptVersionInfoApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the service Gpt_GetVersionInfo() from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:9b0cd624-ab46-40d1-9b1e-b2628fec48de">
                  <SHORT-NAME>GptWakeupFunctionalityApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the services Gpt_SetMode(), Gpt_EnableWakeup() Gpt_DisableWakeup() and Gpt_Cbk_CheckWakeup() from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:d510961f-5031-4b4e-88a6-967e476fa789">
                  <SHORT-NAME>GptPredefTimerFunctionalityApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Adds / removes the services Gpt_SetMode(), Gpt_EnableWakeup() Gpt_DisableWakeup() and Gpt_Cbk_CheckWakeup() from the code.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:add160d6-c3d6-4fe9-9d18-eaec5511cbae">
              <SHORT-NAME>GptAutosarExt</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                    
                    Enabling the settings of this section will configure the driver in a mode not compliant with AUTOSAR requirements.
                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:6adf1308-a3e5-4fbc-be65-0db07f521fca">
                  <SHORT-NAME>GptEnableDualClockMode</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Enables prescaler settings at mode transition.true: Enabled.false: Disabled.
                    Note This feature is not required by Autosar.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ad9a2e36-01ea-40bb-b809-87de828c9bf7">
                  <SHORT-NAME>GptChangeNextTimeoutValueApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Vendor specific: Enables settings for changing the channel counter compare value of a running counter.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:f466e20d-5bba-65fa-be74-2bd1bb0f0b88">
                  <SHORT-NAME>GptEnableUserModeSupport</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    When this parameter is enabled, the GPT module will adapt to run from User Mode. There is no difference between User mode and Privileged mode in GPT module.
                    Note: Implementation Specific Parameter.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:f466e20d-5eba-65fa-be7d-2bd1bb0f0b88">
                  <SHORT-NAME>ChainModeApi</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Vendor specific: Enable/disable API for Chain Mode support.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:465add12-24b7-47c2-861c-fd363f561967">
              <SHORT-NAME>GptDriverConfiguration</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                    
                    This container contains the module-wide configuration (parameters) of the GPT Driver.
                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:dde63254-fdc0-4af6-a0ae-3963c88e9c99">
                  <SHORT-NAME>GptDevErrorDetect</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Enables/Disables development error detection.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:769c2cd9-7582-4935-9012-f5ead6167283">
                  <SHORT-NAME>GptPredefTimer100us32bitEnable</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Enables/Disables the feature 100us/ tick
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>ECU</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:bb0d4be5-b45b-4d8a-a7da-6780e46e0c8c">
                  <SHORT-NAME>GptPredefTimer1usEnablingGrade</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Specifies the grade of enabling the GPT Predef Timers with 1us tick duration.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <SCOPE>ECU</SCOPE>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>GPT_PREDEF_TIMER_1US_16BIT_ENABLED</DEFAULT-VALUE>
                  <LITERALS>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>GPT_PREDEF_TIMER_1US_16BIT_ENABLED</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>GPT_PREDEF_TIMER_1US_16_24BIT_ENABLED</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>GPT_PREDEF_TIMER_1US_16_24_32BIT_ENABLED</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                    <ECUC-ENUMERATION-LITERAL-DEF>
                      <SHORT-NAME>GPT_PREDEF_TIMER_1US_DISABLED</SHORT-NAME>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                    </ECUC-ENUMERATION-LITERAL-DEF>
                  </LITERALS>
                </ECUC-ENUMERATION-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:9396fef6-fec8-4120-a0cd-3833f32b0ee7">
                  <SHORT-NAME>GptTimeout</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">This is a timeout value which is used to wait till
                    - PIT_RTI_LDVAL is synchronized into the RTI clock domain
                    If the Status is not updated then after this timeout the GPT_E_TIMEOUT
                    production error will be reported and the rest of the functionality will be skipped.
                    This parameter is used for PitRti only
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>65535</DEFAULT-VALUE>
                  <MAX>4294967295</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:8436de9b-c7e1-4720-08e9-145e3870a2cb">
                  <SHORT-NAME>GptDisableDemReportErrorStatus</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">Enable/Disable Dem error reporting.</L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>false</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
                <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:08a65f92-5ac0-4d8b-8cc9-9263e702a1db">
                  <SHORT-NAME>GptReportWakeupSource</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Enables/Disables wakeup source reporting.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <DEFAULT-VALUE>true</DEFAULT-VALUE>
                </ECUC-BOOLEAN-PARAM-DEF>
              </PARAMETERS>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:2b10b724-7d04-4254-85fc-71e78b377def">
                  <SHORT-NAME>GptClockReferencePoint</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                     This container contains a parameter, which represents a reference to a container of the type McuClockReferencePoint (defined in module MCU).
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY-INFINITE>1</UPPER-MULTIPLICITY-INFINITE>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:af46503c-4886-4887-abe7-32f96bb97515">
                      <SHORT-NAME>GptClockReference</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                    
                      Reference to a container of the type McuClockReferencePoint, to select an input clock.
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>AUTOSAR_ECUC</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Mcu/McuModuleConfiguration/McuClockSettingConfig/McuClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:de21gbaf-35ef-fp13-89de-65665795e1b9">
              <SHORT-NAME>GptPredefTimerConfiguration</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                    
                    Container for configuring the Predefined Timer functionality.
                    </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <SUB-CONTAINERS>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:3215fa18-6acc-4b74-9b26-cf7ac8ef3aad">
                  <SHORT-NAME>GptPredefTimer_1us_16Bit</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    This container contains the 1U_16BIT predef timer configuration (parameters) of the GPT Driver
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:f6c4bc62-1cb7-47a5-969c-3592bfaf73b7">
                      <SHORT-NAME>GptHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                     
                    Vendor specific: Selects the physical GPT Channel. PIT not use for this feature  
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>EMIOS_0_CH_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_PREDEF</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b79d1912-8f35-466c-a55d-a19c6dbb8527">
                      <SHORT-NAME>GptChannelPrescaler</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         
                        Vendor specific: The GPT module specific clock prescaler value. 
                        Note with STM: 
                        - STM prescaler should be between 1-256. 
                        Note with EMIOS: 
                        - EMIOS prescaler should be between 1-4. 
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>256</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:30afbbf6-2c2a-4ae2-b8f1-658c55b422da">
                      <SHORT-NAME>GptFreezeEnable</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> 
                     
                    Vendor specific: Select to set Freeze enable for the hw resources. 
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:835f71df-3c76-4bc6-a0ba-822fff255b9f">
                      <SHORT-NAME>GptChannelClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                     
                    Reference to the GptClockReferencePoint from which the channel clock is derived.
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Gpt/GptDriverConfiguration/GptClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:2003cbc8-e4ae-4e5d-96ae-ca32210801eb">
                  <SHORT-NAME>GptPredefTimer_1us_24Bit</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    This container contains the 1U_24BIT predef timer configuration (parameters) of the GPT Driver
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:0d417622-d56b-4486-bbde-433e761024cc">
                      <SHORT-NAME>GptHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific: Selects the physical GPT Channel. </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>EMIOS_0_CH_0</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_0_CH_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_0</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_1</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_2</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_3</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_4</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_5</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_6</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_7</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_16</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_17</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_18</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_19</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_20</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_21</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_22</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>EMIOS_1_CH_23</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_PREDEF</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:d8765e1d-4beb-46d1-a490-f32f0acef30d">
                      <SHORT-NAME>GptChannelPrescaler</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                             Vendor specific: The GPT module specific clock prescaler value. 
                                Note with STM: 
                                - STM prescaler should be between 1-256. 
                                Note with EMIOS: 
                                - EMIOS prescaler should be between 1-4. 
                            </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>256</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:7a1b3fc8-23b5-4d19-9748-b2df413e1fbf">
                      <SHORT-NAME>GptFreezeEnable</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                    
                    Vendor specific: Select to set Freeze enable for the hw resources.
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:39c5d524-627b-43c7-bc17-9ab961ed1c96">
                      <SHORT-NAME>GptChannelClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Reference to the GptClockReferencePoint from which the channel clock is derived.   </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Gpt/GptDriverConfiguration/GptClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:44099f60-650a-4d06-8558-8ab6cda0837c">
                  <SHORT-NAME>GptPredefTimer_1us_32Bit</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    This container contains the predef timer configuration (parameters) of the GPT Driver
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:45dd89b6-23c8-46f0-bf6d-d3327a580792">
                      <SHORT-NAME>GptHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Vendor specific: Selects the physical GPT Channel.</L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>STM_0_PREDEF</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_PREDEF</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:a65dbd38-66d1-464a-b7eb-843446b56c4f">
                      <SHORT-NAME>GptChannelPrescaler</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         Vendor specific: The GPT module specific clock prescaler value. 
                            Note with STM: 
                            - STM prescaler should be between 1-256. 
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>256</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:cd9ffabf-8ea6-473f-9537-c0e7218c30d0">
                      <SHORT-NAME>GptFreezeEnable</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                     
                    Vendor specific: Select to set Freeze enable for the hw resources.
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:d86e6636-a8b8-4b72-bd03-d5c16f7054ad">
                      <SHORT-NAME>GptChannelClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN"> Reference to the GptClockReferencePoint from which the channel clock is derived.   </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Gpt/GptDriverConfiguration/GptClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
                <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:ea27cdd7-9b60-4497-ad50-9e703cde9949">
                  <SHORT-NAME>GptPredefTimer_100us_32Bit</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                        
                        This container contains the channel-wide configuration (parameters) of the GPT Driver
                        </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <PARAMETERS>
                    <ECUC-ENUMERATION-PARAM-DEF UUID="ECUC:e2585adb-1fb4-425a-9cbc-17601243136a">
                      <SHORT-NAME>GptHwChannel</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                         
                        Vendor specific: Selects the physical GPT Channel. PIT not use for this feature
                        </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>STM_0_PREDEF</DEFAULT-VALUE>
                      <LITERALS>
                        <ECUC-ENUMERATION-LITERAL-DEF>
                          <SHORT-NAME>STM_0_PREDEF</SHORT-NAME>
                          <ORIGIN>NXP</ORIGIN>
                        </ECUC-ENUMERATION-LITERAL-DEF>
                      </LITERALS>
                    </ECUC-ENUMERATION-PARAM-DEF>
                    <ECUC-INTEGER-PARAM-DEF UUID="ECUC:e8a8f704-7527-46ac-9dad-ab1e5e4ea7ef">
                      <SHORT-NAME>GptChannelPrescaler</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                     Vendor specific: The GPT module specific clock prescaler value. 
                        Note with STM: 
                        - STM prescaler should be between 1-256. 
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>1</DEFAULT-VALUE>
                      <MAX>256</MAX>
                      <MIN>1</MIN>
                    </ECUC-INTEGER-PARAM-DEF>
                    <ECUC-BOOLEAN-PARAM-DEF UUID="ECUC:ed0bc8c8-9f2e-4d9b-b5c3-da1eddc9ce99">
                      <SHORT-NAME>GptFreezeEnable</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                     Vendor specific: Select to set Freeze enable for the hw resources.
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                      <DEFAULT-VALUE>true</DEFAULT-VALUE>
                    </ECUC-BOOLEAN-PARAM-DEF>
                  </PARAMETERS>
                  <REFERENCES>
                    <ECUC-REFERENCE-DEF UUID="ECUC:f776f5b0-74e5-407a-991a-448a2c04d691">
                      <SHORT-NAME>GptChannelClkSrcRef</SHORT-NAME>
                      <DESC>
                        <L-2 L="EN">
                     
                    Reference to the GptClockReferencePoint from which the channel clock is derived.
                    </L-2>
                      </DESC>
                      <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                      <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                      <ORIGIN>NXP</ORIGIN>
                      <POST-BUILD-VARIANT-VALUE>true</POST-BUILD-VARIANT-VALUE>
                      <VALUE-CONFIG-CLASSES>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>PRE-COMPILE</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                        <ECUC-VALUE-CONFIGURATION-CLASS>
                          <CONFIG-CLASS>POST-BUILD</CONFIG-CLASS>
                          <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                        </ECUC-VALUE-CONFIGURATION-CLASS>
                      </VALUE-CONFIG-CLASSES>
                      <DESTINATION-REF DEST="ECUC-PARAM-CONF-CONTAINER-DEF">/AUTOSAR/EcucDefs/Gpt/GptDriverConfiguration/GptClockReferencePoint</DESTINATION-REF>
                    </ECUC-REFERENCE-DEF>
                  </REFERENCES>
                </ECUC-PARAM-CONF-CONTAINER-DEF>
              </SUB-CONTAINERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
            <ECUC-PARAM-CONF-CONTAINER-DEF UUID="ECUC:e3b5bfba-c75a-41e7-ae8d-054a5936bf60">
              <SHORT-NAME>CommonPublishedInformation</SHORT-NAME>
              <DESC>
                <L-2 L="EN">
                          
                           Common container, aggregated by all modules. It contains published information about vendor and versions.
                          </L-2>
              </DESC>
              <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
              <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
              <PARAMETERS>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:5d1dbd9a-a034-44fb-b538-8df4626443f8">
                  <SHORT-NAME>ArReleaseMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Major version number of AUTOSAR specification on which the appropriate implementation is based on.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>4</DEFAULT-VALUE>
                  <MAX>4</MAX>
                  <MIN>4</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:cc14e1e3-6b42-4faa-b2dd-2cb8012d70ef">
                  <SHORT-NAME>ArReleaseMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Minor version number of AUTOSAR specification on which the appropriate implementation is based on.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>3</DEFAULT-VALUE>
                  <MAX>3</MAX>
                  <MIN>3</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:b1f51ed9-15d6-4645-9c0d-ecea80d0c2cd">
                  <SHORT-NAME>ArReleaseRevisionVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Revision version number of AUTOSAR specification on which the appropriate implementation is based on.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:414b6ad6-8f74-49b2-a741-0e10a36d75d5">
                  <SHORT-NAME>ModuleId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Module ID of this module from Module List.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>100</DEFAULT-VALUE>
                  <MAX>100</MAX>
                  <MIN>100</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:bcb51c98-142e-4b25-b4a0-29cd3d458b9b">
                  <SHORT-NAME>SwMajorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Major version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>1</DEFAULT-VALUE>
                  <MAX>1</MAX>
                  <MIN>1</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:76f70dac-e672-4723-ba2c-8dd310c02d4e">
                  <SHORT-NAME>SwMinorVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Minor version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:51150d97-ef68-458c-a6d6-d18a1d0db9ee">
                  <SHORT-NAME>SwPatchVersion</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Patch level version number of the vendor specific implementation of the module. The numbering is vendor specific.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>0</DEFAULT-VALUE>
                  <MAX>0</MAX>
                  <MIN>0</MIN>
                </ECUC-INTEGER-PARAM-DEF>
                <ECUC-STRING-PARAM-DEF UUID="ECUC:13cf3ced-3268-4526-86ad-4fa0ff66624e">
                  <SHORT-NAME>VendorApiInfix</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    In driver modules which can be instantiated several times on a single ECU, BSW00347 requires that the name of APIs is extended by the VendorId and a vendor specific name.
                    This parameter is used to specify the vendor specific name. In total, the implementation specific name is generated as follows:
                    &lt;ModuleName&gt;_&gt;VendorId&gt;_&lt;VendorApiInfix&gt;.
                    E.g.  assuming that the VendorId of the implementor is 123 and the implementer chose a VendorApiInfix of &quot;v11r456&quot; a api name Can_Write defined in the SWS will translate to Can_123_v11r456Write.
                    This parameter is mandatory for all modules with upper multiplicity &gt; 1. It shall not be used for modules with upper multiplicity =1.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>0</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <MULTIPLICITY-CONFIG-CLASSES>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                    <ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-MULTIPLICITY-CONFIGURATION-CLASS>
                  </MULTIPLICITY-CONFIG-CLASSES>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-MULTIPLICITY>false</POST-BUILD-VARIANT-MULTIPLICITY>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <ECUC-STRING-PARAM-DEF-VARIANTS>
                    <ECUC-STRING-PARAM-DEF-CONDITIONAL>
                      <DEFAULT-VALUE>
                      </DEFAULT-VALUE>
                    </ECUC-STRING-PARAM-DEF-CONDITIONAL>
                  </ECUC-STRING-PARAM-DEF-VARIANTS>
                </ECUC-STRING-PARAM-DEF>
                <ECUC-INTEGER-PARAM-DEF UUID="ECUC:21b7fca6-5a29-4938-989e-433371b2f963">
                  <SHORT-NAME>VendorId</SHORT-NAME>
                  <DESC>
                    <L-2 L="EN">
                    
                    Vendor ID of the dedicated implementation of this module according to the AUTOSAR vendor list.
                    </L-2>
                  </DESC>
                  <LOWER-MULTIPLICITY>1</LOWER-MULTIPLICITY>
                  <UPPER-MULTIPLICITY>1</UPPER-MULTIPLICITY>
                  <ORIGIN>NXP</ORIGIN>
                  <POST-BUILD-VARIANT-VALUE>false</POST-BUILD-VARIANT-VALUE>
                  <VALUE-CONFIG-CLASSES>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-POST-BUILD</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                    <ECUC-VALUE-CONFIGURATION-CLASS>
                      <CONFIG-CLASS>PUBLISHED-INFORMATION</CONFIG-CLASS>
                      <CONFIG-VARIANT>VARIANT-PRE-COMPILE</CONFIG-VARIANT>
                    </ECUC-VALUE-CONFIGURATION-CLASS>
                  </VALUE-CONFIG-CLASSES>
                  <SYMBOLIC-NAME-VALUE>false</SYMBOLIC-NAME-VALUE>
                  <DEFAULT-VALUE>43</DEFAULT-VALUE>
                  <MAX>43</MAX>
                  <MIN>43</MIN>
                </ECUC-INTEGER-PARAM-DEF>
              </PARAMETERS>
            </ECUC-PARAM-CONF-CONTAINER-DEF>
          </CONTAINERS>
        </ECUC-MODULE-DEF>
      </ELEMENTS>
    </AR-PACKAGE>
  </AR-PACKAGES>
</AUTOSAR>