
Marking local functions:


Marking externally visible functions: SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01 SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00 SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00 Uart_schm_read_msr


Marking externally visible variables:

Clearing variable flags:

Reclaiming functions:
Reclaiming variables:
Clearing address taken flags:
Symbol table:

Sys_GetCoreID/37 (Sys_GetCoreID) @06c30380
  Type: function
  Visibility: external public
  References: 
  Referring: 
  Availability: not_available
  Function flags: optimize_size
  Called by: SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08/36 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08/35 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07/34 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07/33 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06/32 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06/31 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05/30 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05/29 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04/28 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04/27 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03/26 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03/25 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02/24 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02/23 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01/22 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01/21 (1073741824 (estimated locally),1.00 per call) SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00/20 (1073741824 (estimated locally),1.00 per call) SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00/19 (1073741824 (estimated locally),1.00 per call) 
  Calls: 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08/36 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08) @06c30b60
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_08/17 (read)reentry_guard_UART_EXCLUSIVE_AREA_08/17 (write)msr_UART_EXCLUSIVE_AREA_08/16 (read)reentry_guard_UART_EXCLUSIVE_AREA_08/17 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08/35 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08) @06c308c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_08/17 (read)msr_UART_EXCLUSIVE_AREA_08/16 (write)reentry_guard_UART_EXCLUSIVE_AREA_08/17 (read)reentry_guard_UART_EXCLUSIVE_AREA_08/17 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07/34 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07) @06c30540
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_07/15 (read)reentry_guard_UART_EXCLUSIVE_AREA_07/15 (write)msr_UART_EXCLUSIVE_AREA_07/14 (read)reentry_guard_UART_EXCLUSIVE_AREA_07/15 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07/33 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07) @06c302a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_07/15 (read)msr_UART_EXCLUSIVE_AREA_07/14 (write)reentry_guard_UART_EXCLUSIVE_AREA_07/15 (read)reentry_guard_UART_EXCLUSIVE_AREA_07/15 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06/32 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06) @06d3ed20
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_06/13 (read)reentry_guard_UART_EXCLUSIVE_AREA_06/13 (write)msr_UART_EXCLUSIVE_AREA_06/12 (read)reentry_guard_UART_EXCLUSIVE_AREA_06/13 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06/31 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06) @06d3e700
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_06/13 (read)msr_UART_EXCLUSIVE_AREA_06/12 (write)reentry_guard_UART_EXCLUSIVE_AREA_06/13 (read)reentry_guard_UART_EXCLUSIVE_AREA_06/13 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05/30 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05) @06d3eee0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_05/11 (read)reentry_guard_UART_EXCLUSIVE_AREA_05/11 (write)msr_UART_EXCLUSIVE_AREA_05/10 (read)reentry_guard_UART_EXCLUSIVE_AREA_05/11 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05/29 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05) @06d3ec40
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_05/11 (read)msr_UART_EXCLUSIVE_AREA_05/10 (write)reentry_guard_UART_EXCLUSIVE_AREA_05/11 (read)reentry_guard_UART_EXCLUSIVE_AREA_05/11 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04/28 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04) @06d3e8c0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_04/9 (read)reentry_guard_UART_EXCLUSIVE_AREA_04/9 (write)msr_UART_EXCLUSIVE_AREA_04/8 (read)reentry_guard_UART_EXCLUSIVE_AREA_04/9 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04/27 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04) @06d3e620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_04/9 (read)msr_UART_EXCLUSIVE_AREA_04/8 (write)reentry_guard_UART_EXCLUSIVE_AREA_04/9 (read)reentry_guard_UART_EXCLUSIVE_AREA_04/9 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03/26 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03) @06d3e2a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_03/7 (read)reentry_guard_UART_EXCLUSIVE_AREA_03/7 (write)msr_UART_EXCLUSIVE_AREA_03/6 (read)reentry_guard_UART_EXCLUSIVE_AREA_03/7 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03/25 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03) @06d3e000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_03/7 (read)msr_UART_EXCLUSIVE_AREA_03/6 (write)reentry_guard_UART_EXCLUSIVE_AREA_03/7 (read)reentry_guard_UART_EXCLUSIVE_AREA_03/7 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02/24 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02) @06d37700
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_02/5 (read)reentry_guard_UART_EXCLUSIVE_AREA_02/5 (write)msr_UART_EXCLUSIVE_AREA_02/4 (read)reentry_guard_UART_EXCLUSIVE_AREA_02/5 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02/23 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02) @06d370e0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_02/5 (read)msr_UART_EXCLUSIVE_AREA_02/4 (write)reentry_guard_UART_EXCLUSIVE_AREA_02/5 (read)reentry_guard_UART_EXCLUSIVE_AREA_02/5 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01/22 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01) @06d37c40
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_01/3 (read)reentry_guard_UART_EXCLUSIVE_AREA_01/3 (write)msr_UART_EXCLUSIVE_AREA_01/2 (read)reentry_guard_UART_EXCLUSIVE_AREA_01/3 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01/21 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01) @06d379a0
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_01/3 (read)msr_UART_EXCLUSIVE_AREA_01/2 (write)reentry_guard_UART_EXCLUSIVE_AREA_01/3 (read)reentry_guard_UART_EXCLUSIVE_AREA_01/3 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00/20 (SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00) @06d37620
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_00/1 (read)reentry_guard_UART_EXCLUSIVE_AREA_00/1 (write)msr_UART_EXCLUSIVE_AREA_00/0 (read)reentry_guard_UART_EXCLUSIVE_AREA_00/1 (read)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00/19 (SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00) @06d37380
  Type: function definition analyzed
  Visibility: externally_visible public
  References: reentry_guard_UART_EXCLUSIVE_AREA_00/1 (read)msr_UART_EXCLUSIVE_AREA_00/0 (write)reentry_guard_UART_EXCLUSIVE_AREA_00/1 (read)reentry_guard_UART_EXCLUSIVE_AREA_00/1 (write)
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: Sys_GetCoreID/37 (1073741824 (estimated locally),1.00 per call) 
Uart_schm_read_msr/18 (Uart_schm_read_msr) @06d37000
  Type: function definition analyzed
  Visibility: externally_visible public
  References: 
  Referring: 
  Availability: available
  Function flags: count:1073741824 (estimated locally) body optimize_size
  Called by: 
  Calls: 
reentry_guard_UART_EXCLUSIVE_AREA_08/17 (reentry_guard_UART_EXCLUSIVE_AREA_08) @06d36288
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08/35 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08/35 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08/35 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08/36 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08/36 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08/36 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_08/16 (msr_UART_EXCLUSIVE_AREA_08) @06d361f8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08/35 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08/36 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_07/15 (reentry_guard_UART_EXCLUSIVE_AREA_07) @06d36168
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07/33 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07/33 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07/33 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07/34 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07/34 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07/34 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_07/14 (msr_UART_EXCLUSIVE_AREA_07) @06d360d8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07/33 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07/34 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_06/13 (reentry_guard_UART_EXCLUSIVE_AREA_06) @06d36048
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06/31 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06/31 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06/31 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06/32 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06/32 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06/32 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_06/12 (msr_UART_EXCLUSIVE_AREA_06) @06c19f78
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06/31 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06/32 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_05/11 (reentry_guard_UART_EXCLUSIVE_AREA_05) @06c19ee8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05/29 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05/29 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05/29 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05/30 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05/30 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05/30 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_05/10 (msr_UART_EXCLUSIVE_AREA_05) @06c19e58
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05/29 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05/30 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_04/9 (reentry_guard_UART_EXCLUSIVE_AREA_04) @06c19dc8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04/27 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04/27 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04/27 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04/28 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04/28 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04/28 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_04/8 (msr_UART_EXCLUSIVE_AREA_04) @06c19d38
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04/27 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04/28 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_03/7 (reentry_guard_UART_EXCLUSIVE_AREA_03) @06c19ca8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03/25 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03/25 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03/25 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03/26 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03/26 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03/26 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_03/6 (msr_UART_EXCLUSIVE_AREA_03) @06c19c18
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03/25 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03/26 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_02/5 (reentry_guard_UART_EXCLUSIVE_AREA_02) @06c19b88
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02/23 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02/23 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02/23 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02/24 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02/24 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02/24 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_02/4 (msr_UART_EXCLUSIVE_AREA_02) @06c19af8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02/23 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02/24 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_01/3 (reentry_guard_UART_EXCLUSIVE_AREA_01) @06c19a68
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01/21 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01/21 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01/21 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01/22 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01/22 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01/22 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_01/2 (msr_UART_EXCLUSIVE_AREA_01) @06c199d8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01/21 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01/22 (read)
  Availability: available
  Varpool flags:
reentry_guard_UART_EXCLUSIVE_AREA_00/1 (reentry_guard_UART_EXCLUSIVE_AREA_00) @06c19948
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00/19 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00/19 (read)SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00/19 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00/20 (read)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00/20 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00/20 (read)
  Availability: available
  Varpool flags:
msr_UART_EXCLUSIVE_AREA_00/0 (msr_UART_EXCLUSIVE_AREA_00) @06c198b8
  Type: variable definition analyzed
  Visibility: force_output prevailing_def_ironly
  References: 
  Referring: SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00/19 (write)SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00/20 (read)
  Availability: available
  Varpool flags:
SchM_Exit_Uart_UART_EXCLUSIVE_AREA_08 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_08 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_08[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_08[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_07 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_07 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_07[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_07[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_06 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_06 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_06[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_06[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_05 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_05 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_05[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_05[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_04 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_04 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_04[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_04[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_03 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_03 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_03[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_03[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_02 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_02 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_02[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_01 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_01 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_01[u32CoreId_10] ={v} _5;
  return;

}


SchM_Exit_Uart_UART_EXCLUSIVE_AREA_00 ()
{
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;
  long unsigned int _6;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  _3 = _2 + 4294967295;
  reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} _3;
  # DEBUG BEGIN_STMT
  _4 ={v} msr_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  _5 = _4 & 1;
  if (_5 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 3> [local count: 536870913]:
  _6 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  if (_6 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsie i");

  <bb 5> [local count: 1073741824]:
  return;

}


SchM_Enter_Uart_UART_EXCLUSIVE_AREA_00 ()
{
  register uint32 reg_tmp;
  uint32 u32CoreId;
  unsigned char _1;
  long unsigned int _2;
  long unsigned int _3;
  long unsigned int _4;
  long unsigned int _5;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  _1 = Sys_GetCoreID ();
  u32CoreId_10 = (uint32) _1;
  # DEBUG u32CoreId => u32CoreId_10
  # DEBUG BEGIN_STMT
  _2 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  if (_2 == 0)
    goto <bb 3>; [50.00%]
  else
    goto <bb 6>; [50.00%]

  <bb 3> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  # DEBUG INLINE_ENTRY Uart_schm_read_msr
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_14);
  # DEBUG reg_tmp => reg_tmp_14
  # DEBUG BEGIN_STMT
  # DEBUG reg_tmp => NULL
  # DEBUG msr => reg_tmp_14
  # DEBUG BEGIN_STMT
  _3 = reg_tmp_14 & 1;
  if (_3 == 0)
    goto <bb 4>; [50.00%]
  else
    goto <bb 5>; [50.00%]

  <bb 4> [local count: 268435456]:
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" cpsid i");

  <bb 5> [local count: 536870913]:
  # DEBUG BEGIN_STMT
  msr_UART_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} reg_tmp_14;

  <bb 6> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  _4 ={v} reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10];
  _5 = _4 + 1;
  reentry_guard_UART_EXCLUSIVE_AREA_00[u32CoreId_10] ={v} _5;
  return;

}


Uart_schm_read_msr ()
{
  register uint32 reg_tmp;

  <bb 2> [local count: 1073741824]:
  # DEBUG BEGIN_STMT
  # DEBUG BEGIN_STMT
  __asm__ __volatile__(" mrs %0, primask " : "=r" reg_tmp_1);
  # DEBUG reg_tmp => reg_tmp_1
  # DEBUG BEGIN_STMT
  return reg_tmp_1;

}


